TurboJPEG 3.1

Loading...
Searching...
No Matches
Data Structures | Macros | Typedefs | Enumerations | Functions | Variables
TurboJPEG

TurboJPEG API. More...

## Data Structures
struct | tjscalingfactor
| Scaling factor. More...
struct | tjregion
| Cropping region. More...
struct | tjtransform
| Lossless transform. More...

## Macros
#define | TJ_NUMINIT
| The number of initialization options.
#define | TJ_NUMSAMP
| The number of chrominance subsampling options.
#define | TJ_NUMPF
| The number of pixel formats.
#define | TJ_NUMCS
| The number of JPEG colorspaces.
#define | TJ_NUMERR
| The number of error codes.
#define | TJ_NUMXOP
| The number of transform operations.
#define | TJXOPT_PERFECT
| This option causes tj3Transform() to return an error if the transform is not perfect.
#define | TJXOPT_TRIM
| Discard any partial iMCUs that cannot be transformed.
#define | TJXOPT_CROP
| Enable lossless cropping.
#define | TJXOPT_GRAY
| Discard the color data in the source image, and generate a grayscale destination image.
#define | TJXOPT_NOOUTPUT
| Do not generate a destination image.
#define | TJXOPT_PROGRESSIVE
| Generate a progressive destination image instead of a single-scan destination image.
#define | TJXOPT_COPYNONE
| Do not copy any extra markers (including Exif and ICC profile data) from the source image to the destination image.
#define | TJXOPT_ARITHMETIC
| Enable arithmetic entropy coding in the destination image.
#define | TJXOPT_OPTIMIZE
| Enable Huffman table optimization for the destination image.
#define | TJSCALED(dimension, scalingFactor)
| Compute the scaled value of `dimension` using the given scaling factor.

## Typedefs
typedef struct tjtransform | tjtransform
| Lossless transform.
typedef void * | tjhandle
| TurboJPEG instance handle.

## Enumerations
enum | TJINIT { TJINIT_COMPRESS , TJINIT_DECOMPRESS , TJINIT_TRANSFORM }
| Initialization options. More...
enum | TJSAMP { TJSAMP_444 , TJSAMP_422 , TJSAMP_420 , TJSAMP_GRAY , TJSAMP_440 , TJSAMP_411 , TJSAMP_441 , TJSAMP_UNKNOWN }
| Chrominance subsampling options. More...
enum | TJPF { TJPF_RGB , TJPF_BGR , TJPF_RGBX , TJPF_BGRX , TJPF_XBGR , TJPF_XRGB , TJPF_GRAY , TJPF_RGBA , TJPF_BGRA , TJPF_ABGR , TJPF_ARGB , TJPF_CMYK , TJPF_UNKNOWN }
| Pixel formats. More...
enum | TJCS { TJCS_RGB , TJCS_YCbCr , TJCS_GRAY , TJCS_CMYK , TJCS_YCCK }
| JPEG colorspaces. More...
enum | TJPARAM { TJPARAM_STOPONWARNING , TJPARAM_BOTTOMUP , TJPARAM_NOREALLOC , TJPARAM_QUALITY , TJPARAM_SUBSAMP , TJPARAM_JPEGWIDTH , TJPARAM_JPEGHEIGHT , TJPARAM_PRECISION , TJPARAM_COLORSPACE , TJPARAM_FASTUPSAMPLE , TJPARAM_FASTDCT , TJPARAM_OPTIMIZE , TJPARAM_PROGRESSIVE , TJPARAM_SCANLIMIT , TJPARAM_ARITHMETIC , TJPARAM_LOSSLESS , TJPARAM_LOSSLESSPSV , TJPARAM_LOSSLESSPT , TJPARAM_RESTARTBLOCKS , TJPARAM_RESTARTROWS , TJPARAM_XDENSITY , TJPARAM_YDENSITY , TJPARAM_DENSITYUNITS , TJPARAM_MAXMEMORY , TJPARAM_MAXPIXELS , TJPARAM_SAVEMARKERS }
| Parameters. More...
enum | TJERR { TJERR_WARNING , TJERR_FATAL }
| Error codes. More...
enum | TJXOP { TJXOP_NONE , TJXOP_HFLIP , TJXOP_VFLIP , TJXOP_TRANSPOSE , TJXOP_TRANSVERSE , TJXOP_ROT90 , TJXOP_ROT180 , TJXOP_ROT270 }
| Transform operations for tj3Transform() More...

## Functions
DLLEXPORT tjhandle | tj3Init (int initType)
| Create a new TurboJPEG instance.
DLLEXPORT void | tj3Destroy (tjhandle handle)
| Destroy a TurboJPEG instance.
DLLEXPORT char * | tj3GetErrorStr (tjhandle handle)
| Returns a descriptive error message explaining why the last command failed.
DLLEXPORT int | tj3GetErrorCode (tjhandle handle)
| Returns a code indicating the severity of the last error.
DLLEXPORT int | tj3Set (tjhandle handle, int param, int value)
| Set the value of a parameter.
DLLEXPORT int | tj3Get (tjhandle handle, int param)
| Get the value of a parameter.
DLLEXPORT void * | tj3Alloc (size_t bytes)
| Allocate a byte buffer for use with TurboJPEG.
DLLEXPORT void | tj3Free (void *buffer)
| Free a byte buffer previously allocated by TurboJPEG.
DLLEXPORT size_t | tj3JPEGBufSize (int width, int height, int jpegSubsamp)
| The maximum size of the buffer (in bytes) required to hold a JPEG image with the given parameters.
DLLEXPORT size_t | tj3YUVBufSize (int width, int align, int height, int subsamp)
| The size of the buffer (in bytes) required to hold a unified planar YUV image with the given parameters.
DLLEXPORT size_t | tj3YUVPlaneSize (int componentID, int width, int stride, int height, int subsamp)
| The size of the buffer (in bytes) required to hold a YUV image plane with the given parameters.
DLLEXPORT int | tj3YUVPlaneWidth (int componentID, int width, int subsamp)
| The plane width of a YUV image plane with the given parameters.
DLLEXPORT int | tj3YUVPlaneHeight (int componentID, int height, int subsamp)
| The plane height of a YUV image plane with the given parameters.
DLLEXPORT int | tj3SetICCProfile (tjhandle handle, unsigned char *iccBuf, size_t iccSize)
| Embed an ICC (International Color Consortium) color management profile in JPEG images generated by subsequent compression and lossless transformation operations.
DLLEXPORT int | tj3Compress8 (tjhandle handle, const unsigned char *srcBuf, int width, int pitch, int height, int pixelFormat, unsigned char **jpegBuf, size_t *jpegSize)
| Compress a packed-pixel RGB, grayscale, or CMYK image with 2 to 8 bits of data precision per sample into a JPEG image with the same data precision.
DLLEXPORT int | tj3Compress12 (tjhandle handle, const short *srcBuf, int width, int pitch, int height, int pixelFormat, unsigned char **jpegBuf, size_t *jpegSize)
| Compress a packed-pixel RGB, grayscale, or CMYK image with 9 to 12 bits of data precision per sample into a JPEG image with the same data precision.
DLLEXPORT int | tj3Compress16 (tjhandle handle, const unsigned short *srcBuf, int width, int pitch, int height, int pixelFormat, unsigned char **jpegBuf, size_t *jpegSize)
| Compress a packed-pixel RGB, grayscale, or CMYK image with 13 to 16 bits of data precision per sample into a lossless JPEG image with the same data precision.
DLLEXPORT int | tj3CompressFromYUVPlanes8 (tjhandle handle, const unsigned char *const *srcPlanes, int width, const int *strides, int height, unsigned char **jpegBuf, size_t *jpegSize)
| Compress a set of 8-bit-per-sample Y, U (Cb), and V (Cr) image planes into an 8-bit-per-sample JPEG image.
DLLEXPORT int | tj3CompressFromYUV8 (tjhandle handle, const unsigned char *srcBuf, int width, int align, int height, unsigned char **jpegBuf, size_t *jpegSize)
| Compress an 8-bit-per-sample unified planar YUV image into an 8-bit-per-sample JPEG image.
DLLEXPORT int | tj3EncodeYUVPlanes8 (tjhandle handle, const unsigned char *srcBuf, int width, int pitch, int height, int pixelFormat, unsigned char **dstPlanes, int *strides)
| Encode an 8-bit-per-sample packed-pixel RGB or grayscale image into separate 8-bit-per-sample Y, U (Cb), and V (Cr) image planes.
DLLEXPORT int | tj3EncodeYUV8 (tjhandle handle, const unsigned char *srcBuf, int width, int pitch, int height, int pixelFormat, unsigned char *dstBuf, int align)
| Encode an 8-bit-per-sample packed-pixel RGB or grayscale image into an 8-bit-per-sample unified planar YUV image.
DLLEXPORT int | tj3DecompressHeader (tjhandle handle, const unsigned char *jpegBuf, size_t jpegSize)
| Retrieve information about a JPEG image without decompressing it, or prime the decompressor with quantization and Huffman tables.
DLLEXPORT int | tj3GetICCProfile (tjhandle handle, unsigned char **iccBuf, size_t *iccSize)
| Retrieve the ICC (International Color Consortium) color management profile (if any) that was previously extracted from a JPEG image.
DLLEXPORT tjscalingfactor * | tj3GetScalingFactors (int *numScalingFactors)
| Returns a list of fractional scaling factors that the JPEG decompressor supports.
DLLEXPORT int | tj3SetScalingFactor (tjhandle handle, tjscalingfactor scalingFactor)
| Set the scaling factor for subsequent lossy decompression operations.
DLLEXPORT int | tj3SetCroppingRegion (tjhandle handle, tjregion croppingRegion)
| Set the cropping region for partially decompressing a lossy JPEG image into a packed-pixel image.
DLLEXPORT int | tj3Decompress8 (tjhandle handle, const unsigned char *jpegBuf, size_t jpegSize, unsigned char *dstBuf, int pitch, int pixelFormat)
| Decompress a JPEG image with 2 to 8 bits of data precision per sample into a packed-pixel RGB, grayscale, or CMYK image with the same data precision.
DLLEXPORT int | tj3Decompress12 (tjhandle handle, const unsigned char *jpegBuf, size_t jpegSize, short *dstBuf, int pitch, int pixelFormat)
| Decompress a JPEG image with 9 to 12 bits of data precision per sample into a packed-pixel RGB, grayscale, or CMYK image with the same data precision.
DLLEXPORT int | tj3Decompress16 (tjhandle handle, const unsigned char *jpegBuf, size_t jpegSize, unsigned short *dstBuf, int pitch, int pixelFormat)
| Decompress a lossless JPEG image with 13 to 16 bits of data precision per sample into a packed-pixel RGB, grayscale, or CMYK image with the same data precision.
DLLEXPORT int | tj3DecompressToYUVPlanes8 (tjhandle handle, const unsigned char *jpegBuf, size_t jpegSize, unsigned char **dstPlanes, int *strides)
| Decompress an 8-bit-per-sample JPEG image into separate 8-bit-per-sample Y, U (Cb), and V (Cr) image planes.
DLLEXPORT int | tj3DecompressToYUV8 (tjhandle handle, const unsigned char *jpegBuf, size_t jpegSize, unsigned char *dstBuf, int align)
| Decompress an 8-bit-per-sample JPEG image into an 8-bit-per-sample unified planar YUV image.
DLLEXPORT int | tj3DecodeYUVPlanes8 (tjhandle handle, const unsigned char *const *srcPlanes, const int *strides, unsigned char *dstBuf, int width, int pitch, int height, int pixelFormat)
| Decode a set of 8-bit-per-sample Y, U (Cb), and V (Cr) image planes into an 8-bit-per-sample packed-pixel RGB or grayscale image.
DLLEXPORT int | tj3DecodeYUV8 (tjhandle handle, const unsigned char *srcBuf, int align, unsigned char *dstBuf, int width, int pitch, int height, int pixelFormat)
| Decode an 8-bit-per-sample unified planar YUV image into an 8-bit-per-sample packed-pixel RGB or grayscale image.
DLLEXPORT size_t | tj3TransformBufSize (tjhandle handle, const tjtransform *transform)
| The maximum size of the buffer (in bytes) required to hold a JPEG image transformed with the given transform parameters and/or cropping region.
DLLEXPORT int | tj3Transform (tjhandle handle, const unsigned char *jpegBuf, size_t jpegSize, int n, unsigned char **dstBufs, size_t *dstSizes, const tjtransform *transforms)
| Losslessly transform a JPEG image into another JPEG image.
DLLEXPORT unsigned char * | tj3LoadImage8 (tjhandle handle, const char *filename, int *width, int align, int *height, int *pixelFormat)
| Load a packed-pixel image with 2 to 8 bits of data precision per sample from disk into memory.
DLLEXPORT short * | tj3LoadImage12 (tjhandle handle, const char *filename, int *width, int align, int *height, int *pixelFormat)
| Load a packed-pixel image with 9 to 12 bits of data precision per sample from disk into memory.
DLLEXPORT unsigned short * | tj3LoadImage16 (tjhandle handle, const char *filename, int *width, int align, int *height, int *pixelFormat)
| Load a packed-pixel image with 13 to 16 bits of data precision per sample from disk into memory.
DLLEXPORT int | tj3SaveImage8 (tjhandle handle, const char *filename, const unsigned char *buffer, int width, int pitch, int height, int pixelFormat)
| Save a packed-pixel image with 2 to 8 bits of data precision per sample from memory to disk.
DLLEXPORT int | tj3SaveImage12 (tjhandle handle, const char *filename, const short *buffer, int width, int pitch, int height, int pixelFormat)
| Save a packed-pixel image with 9 to 12 bits of data precision per sample from memory to disk.
DLLEXPORT int | tj3SaveImage16 (tjhandle handle, const char *filename, const unsigned short *buffer, int width, int pitch, int height, int pixelFormat)
| Save a packed-pixel image with 13 to 16 bits of data precision per sample from memory to disk.

## Variables
static const int | tjMCUWidth [TJ_NUMSAMP]
| iMCU width (in pixels) for a given level of chrominance subsampling
static const int | tjMCUHeight [TJ_NUMSAMP]
| iMCU height (in pixels) for a given level of chrominance subsampling
static const int | tjRedOffset [TJ_NUMPF]
| Red offset (in samples) for a given pixel format.
static const int | tjGreenOffset [TJ_NUMPF]
| Green offset (in samples) for a given pixel format.
static const int | tjBlueOffset [TJ_NUMPF]
| Blue offset (in samples) for a given pixel format.
static const int | tjAlphaOffset [TJ_NUMPF]
| Alpha offset (in samples) for a given pixel format.
static const int | tjPixelSize [TJ_NUMPF]
| Pixel size (in samples) for a given pixel format.
static const tjregion | TJUNCROPPED
| A tjregion structure that specifies no cropping.
static const tjscalingfactor | TJUNSCALED
| A tjscalingfactor structure that specifies a scaling factor of 1/1 (no scaling)

## Detailed Description

TurboJPEG API.

This API provides an interface for generating, decoding, and transforming planar YUV and JPEG images in memory.

## YUV Image Format Notes

Technically, the JPEG format uses the YCbCr colorspace (which is technically not a colorspace but a color transform), but per the convention of the digital video community, the TurboJPEG API uses "YUV" to refer to an image format consisting of Y, Cb, and Cr image planes.

Each plane is simply a 2D array of bytes, each byte representing the value of one of the components (Y, Cb, or Cr) at a particular location in the image. The width and height of each plane are determined by the image width, height, and level of chrominance subsampling. The luminance plane width is the image width padded to the nearest multiple of the horizontal subsampling factor (1 in the case of 4:4:4, grayscale, 4:4:0, or 4:4:1; 2 in the case of 4:2:2 or 4:2:0; 4 in the case of 4:1:1.) Similarly, the luminance plane height is the image height padded to the nearest multiple of the vertical subsampling factor (1 in the case of 4:4:4, 4:2:2, grayscale, or 4:1:1; 2 in the case of 4:2:0 or 4:4:0; 4 in the case of 4:4:1.) This is irrespective of any additional padding that may be specified as an argument to the various YUV functions. The chrominance plane width is equal to the luminance plane width divided by the horizontal subsampling factor, and the chrominance plane height is equal to the luminance plane height divided by the vertical subsampling factor.

For example, if the source image is 35 x 35 pixels and 4:2:2 subsampling is used, then the luminance plane would be 36 x 35 bytes, and each of the chrominance planes would be 18 x 35 bytes. If you specify a row alignment of 4 bytes on top of this, then the luminance plane would be 36 x 35 bytes, and each of the chrominance planes would be 20 x 35 bytes.

## Macro Definition Documentation

## ◆ TJ_NUMCS

#define TJ_NUMCS

The number of JPEG colorspaces.

## ◆ TJ_NUMERR

#define TJ_NUMERR

The number of error codes.

## ◆ TJ_NUMINIT

#define TJ_NUMINIT

The number of initialization options.

## ◆ TJ_NUMPF

#define TJ_NUMPF

The number of pixel formats.

## ◆ TJ_NUMSAMP

#define TJ_NUMSAMP

The number of chrominance subsampling options.

## ◆ TJ_NUMXOP

#define TJ_NUMXOP

The number of transform operations.

## ◆ TJSCALED

#define TJSCALED | ( |  | dimension,
|  |  | scalingFactor
| ) |  |

Compute the scaled value of `dimension` using the given scaling factor.

This macro performs the integer equivalent of `ceil(dimension * scalingFactor)`.

## ◆ TJXOPT_ARITHMETIC

#define TJXOPT_ARITHMETIC

Enable arithmetic entropy coding in the destination image.

Arithmetic entropy coding generally improves compression relative to Huffman entropy coding (the default), but it reduces decompression performance considerably. Can be combined with TJXOPT_PROGRESSIVE.

## ◆ TJXOPT_COPYNONE

#define TJXOPT_COPYNONE

Do not copy any extra markers (including Exif and ICC profile data) from the source image to the destination image.

## ◆ TJXOPT_CROP

#define TJXOPT_CROP

Enable lossless cropping.

See tj3Transform() for more information.

## ◆ TJXOPT_GRAY

#define TJXOPT_GRAY

Discard the color data in the source image, and generate a grayscale destination image.

## ◆ TJXOPT_NOOUTPUT

#define TJXOPT_NOOUTPUT

Do not generate a destination image.

(This can be used in conjunction with a custom filter to capture the transformed DCT coefficients without transcoding them.)

## ◆ TJXOPT_OPTIMIZE

#define TJXOPT_OPTIMIZE

Enable Huffman table optimization for the destination image.

Huffman table optimization improves compression slightly (generally 5% or less.)

## ◆ TJXOPT_PERFECT

#define TJXOPT_PERFECT

This option causes tj3Transform() to return an error if the transform is not perfect.

Lossless transforms operate on iMCUs, the size of which depends on the level of chrominance subsampling used (see tjMCUWidth and tjMCUHeight.) If the image's width or height is not evenly divisible by the iMCU size, then there will be partial iMCUs on the right and/or bottom edges. It is not possible to move these partial iMCUs to the top or left of the image, so any transform that would require that is "imperfect." If this option is not specified, then any partial iMCUs that cannot be transformed will be left in place, which will create odd-looking strips on the right or bottom edge of the image.

## ◆ TJXOPT_PROGRESSIVE

#define TJXOPT_PROGRESSIVE

Generate a progressive destination image instead of a single-scan destination image.

Progressive JPEG images generally have better compression ratios than single-scan JPEG images (much better if the image has large areas of solid color), but progressive JPEG decompression is considerably slower than single-scan JPEG decompression. Can be combined with TJXOPT_ARITHMETIC. Implies TJXOPT_OPTIMIZE unless TJXOPT_ARITHMETIC is also specified.

## ◆ TJXOPT_TRIM

#define TJXOPT_TRIM

Discard any partial iMCUs that cannot be transformed.

## Typedef Documentation

## ◆ tjhandle

typedef void* tjhandle

TurboJPEG instance handle.

## ◆ tjtransform

typedef struct tjtransform tjtransform

Lossless transform.

## Enumeration Type Documentation

## ◆ TJCS

enum TJCS

JPEG colorspaces.

Enumerator
TJCS_RGB | RGB colorspace. When generating the JPEG image, the R, G, and B components in the source image are reordered into image planes, but no colorspace conversion or subsampling is performed. RGB JPEG images can be generated from and decompressed to packed-pixel images with any of the extended RGB or grayscale pixel formats, but they cannot be generated from or decompressed to planar YUV images.
TJCS_YCbCr | YCbCr colorspace. YCbCr is not an absolute colorspace but rather a mathematical transformation of RGB designed solely for storage and transmission. YCbCr images must be converted to RGB before they can be displayed. In the YCbCr colorspace, the Y (luminance) component represents the black & white portion of the original image, and the Cb and Cr (chrominance) components represent the color portion of the original image. Historically, the analog equivalent of this transformation allowed the same signal to be displayed to both black & white and color televisions, but JPEG images use YCbCr primarily because it allows the color data to be optionally subsampled in order to reduce network and disk usage. YCbCr is the most common JPEG colorspace, and YCbCr JPEG images can be generated from and decompressed to packed-pixel images with any of the extended RGB or grayscale pixel formats. YCbCr JPEG images can also be generated from and decompressed to planar YUV images.
TJCS_GRAY | Grayscale colorspace. The JPEG image retains only the luminance data (Y component), and any color data from the source image is discarded. Grayscale JPEG images can be generated from and decompressed to packed-pixel images with any of the extended RGB or grayscale pixel formats, or they can be generated from and decompressed to planar YUV images.
TJCS_CMYK | CMYK colorspace. When generating the JPEG image, the C, M, Y, and K components in the source image are reordered into image planes, but no colorspace conversion or subsampling is performed. CMYK JPEG images can only be generated from and decompressed to packed-pixel images with the CMYK pixel format.
TJCS_YCCK | YCCK colorspace. YCCK (AKA "YCbCrK") is not an absolute colorspace but rather a mathematical transformation of CMYK designed solely for storage and transmission. It is to CMYK as YCbCr is to RGB. CMYK pixels can be reversibly transformed into YCCK, and as with YCbCr, the chrominance components in the YCCK pixels can be subsampled without incurring major perceptual loss. YCCK JPEG images can only be generated from and decompressed to packed-pixel images with the CMYK pixel format.

## ◆ TJERR

enum TJERR

Error codes.

Enumerator
TJERR_WARNING | The error was non-fatal and recoverable, but the destination image may still be corrupt.
TJERR_FATAL | The error was fatal and non-recoverable.

## ◆ TJINIT

enum TJINIT

Initialization options.

Enumerator
TJINIT_COMPRESS | Initialize the TurboJPEG instance for compression.
TJINIT_DECOMPRESS | Initialize the TurboJPEG instance for decompression.
TJINIT_TRANSFORM | Initialize the TurboJPEG instance for lossless transformation (both compression and decompression.)

## ◆ TJPARAM

enum TJPARAM

Parameters.

Enumerator
TJPARAM_STOPONWARNING | Error handling behavior. Value `0` [default] Allow the current compression/decompression/transform operation to complete unless a fatal error is encountered. `1` Immediately discontinue the current compression/decompression/transform operation if a warning (non-fatal error) occurs.
TJPARAM_BOTTOMUP | Row order in packed-pixel source/destination images. Value `0` [default] top-down (X11) order `1` bottom-up (Windows, OpenGL) order
TJPARAM_NOREALLOC | JPEG destination buffer (re)allocation [compression, lossless transformation]. Value `0` [default] Attempt to allocate or reallocate the JPEG destination buffer as needed. `1` Generate an error if the JPEG destination buffer is invalid or too small.
TJPARAM_QUALITY | Perceptual quality of lossy JPEG images [compression only]. Value `1`-`100` (`1` = worst quality but best compression, `100` = best quality but worst compression) [no default; must be explicitly specified]
TJPARAM_SUBSAMP | Chrominance subsampling level. The JPEG or YUV image uses (decompression, decoding) or will use (lossy compression, encoding) the specified level of chrominance subsampling. Value One of the chrominance subsampling options [no default; must be explicitly specified for lossy compression, encoding, and decoding]
TJPARAM_JPEGWIDTH | JPEG width (in pixels) [decompression only, read-only].
TJPARAM_JPEGHEIGHT | JPEG height (in pixels) [decompression only, read-only].
TJPARAM_PRECISION | Data precision (bits per sample) The JPEG image uses (decompression) or will use (lossless compression) the specified number of bits per sample. This parameter also specifies the target data precision when loading a PBMPLUS file with tj3LoadImage8(), tj3LoadImage12(), or tj3LoadImage16() and the source data precision when saving a PBMPLUS file with tj3SaveImage8(), tj3SaveImage12(), or tj3SaveImage16(). The data precision is the number of bits in the maximum sample value, which may not be the same as the width of the data type used to store the sample. Value `8` or `12` for lossy JPEG images; `2` to `16` for lossless JPEG and PBMPLUS images 12-bit JPEG data precision implies TJPARAM_OPTIMIZE unless TJPARAM_ARITHMETIC is set.
TJPARAM_COLORSPACE | JPEG colorspace. The JPEG image uses (decompression) or will use (lossy compression) the specified colorspace. Value One of the JPEG colorspaces [default for lossy compression: automatically selected based on the subsampling level and pixel format]
TJPARAM_FASTUPSAMPLE | Chrominance upsampling algorithm [lossy decompression only]. Value `0` [default] Use smooth upsampling when decompressing a JPEG image that was generated using chrominance subsampling. This creates a smooth transition between neighboring chrominance components in order to reduce upsampling artifacts in the decompressed image. `1` Use the fastest chrominance upsampling algorithm available, which may combine upsampling with color conversion.
TJPARAM_FASTDCT | DCT/IDCT algorithm [lossy compression and decompression]. Value `0` [default] Use the most accurate DCT/IDCT algorithm available. `1` Use the fastest DCT/IDCT algorithm available. This parameter is provided mainly for backward compatibility with libjpeg, which historically implemented several different DCT/IDCT algorithms because of performance limitations with 1990s CPUs. In the libjpeg-turbo implementation of the TurboJPEG API: The "fast" and "accurate" DCT/IDCT algorithms perform similarly on modern x86/x86-64 CPUs that support AVX2 instructions. The "fast" algorithm is generally only about 5-15% faster than the "accurate" algorithm on other types of CPUs. The difference in accuracy between the "fast" and "accurate" algorithms is the most pronounced at JPEG quality levels above 90 and tends to be more pronounced with decompression than with compression. For JPEG quality levels above 97, the "fast" algorithm degrades and is not fully accelerated, so it is slower than the "accurate" algorithm.
TJPARAM_OPTIMIZE | Huffman table optimization [lossy compression, lossless transformation]. Value `0` [default] The JPEG image will use the default Huffman tables. `1` Optimal Huffman tables will be computed for the JPEG image. For lossless transformation, this can also be specified using TJXOPT_OPTIMIZE. Huffman table optimization improves compression slightly (generally 5% or less), but it reduces compression performance considerably.
TJPARAM_PROGRESSIVE | Progressive JPEG. In a progressive JPEG image, the DCT coefficients are split across multiple "scans" of increasing quality. Thus, a low-quality scan containing the lowest-frequency DCT coefficients can be transmitted first and refined with subsequent higher-quality scans containing higher-frequency DCT coefficients. When using Huffman entropy coding, the progressive JPEG format also provides an "end-of-bands (EOB) run" feature that allows large groups of zeroes, potentially spanning multiple MCUs, to be represented using only a few bytes. Value `0` [default for compression, lossless transformation] The lossy JPEG image is (decompression) or will be (compression, lossless transformation) single-scan. `1` The lossy JPEG image is (decompression) or will be (compression, lossless transformation) progressive. For lossless transformation, this can also be specified using TJXOPT_PROGRESSIVE. Progressive JPEG images generally have better compression ratios than single-scan JPEG images (much better if the image has large areas of solid color), but progressive JPEG compression and decompression is considerably slower than single-scan JPEG compression and decompression. Can be combined with TJPARAM_ARITHMETIC. Implies TJPARAM_OPTIMIZE unless TJPARAM_ARITHMETIC is also set.
TJPARAM_SCANLIMIT | Progressive JPEG scan limit for lossy JPEG images [decompression, lossless transformation]. Setting this parameter causes the decompression and transform functions to return an error if the number of scans in a progressive JPEG image exceeds the specified limit. The primary purpose of this is to allow security-critical applications to guard against an exploit of the progressive JPEG format described in this report. Value maximum number of progressive JPEG scans that the decompression and transform functions will process [default: `0` (no limit)] See also TJPARAM_PROGRESSIVE
TJPARAM_ARITHMETIC | Arithmetic entropy coding. Value `0` [default for compression, lossless transformation] The lossy JPEG image uses (decompression) or will use (compression, lossless transformation) Huffman entropy coding. `1` The lossy JPEG image uses (decompression) or will use (compression, lossless transformation) arithmetic entropy coding. For lossless transformation, this can also be specified using TJXOPT_ARITHMETIC. Arithmetic entropy coding generally improves compression relative to Huffman entropy coding, but it reduces compression and decompression performance considerably. Can be combined with TJPARAM_PROGRESSIVE.
TJPARAM_LOSSLESS | Lossless JPEG. Value `0` [default for compression] The JPEG image is (decompression) or will be (compression) lossy/DCT-based. `1` The JPEG image is (decompression) or will be (compression) lossless/predictive. In most cases, lossless JPEG compression and decompression is considerably slower than lossy JPEG compression and decompression, and lossless JPEG images are much larger than lossy JPEG images. Thus, lossless JPEG images are typically used only for applications that require mathematically lossless compression. Also note that the following features are not available with lossless JPEG images: Colorspace conversion (lossless JPEG images always use TJCS_RGB, TJCS_GRAY, or TJCS_CMYK, depending on the pixel format of the source image) Chrominance subsampling (lossless JPEG images always use TJSAMP_444) JPEG quality selection DCT/IDCT algorithm selection Progressive JPEG Arithmetic entropy coding Compression from/decompression to planar YUV images Decompression scaling Lossless transformation See also TJPARAM_LOSSLESSPSV, TJPARAM_LOSSLESSPT
TJPARAM_LOSSLESSPSV | Lossless JPEG predictor selection value (PSV) Value `1`-`7` [default for compression: `1`] Lossless JPEG compression shares no algorithms with lossy JPEG compression. Instead, it uses differential pulse-code modulation (DPCM), an algorithm whereby each sample is encoded as the difference between the sample's value and a "predictor", which is based on the values of neighboring samples. If Ra is the sample immediately to the left of the current sample, Rb is the sample immediately above the current sample, and Rc is the sample diagonally to the left and above the current sample, then the relationship between the predictor selection value and the predictor is as follows:
PSV | Predictor
--- | ---
1 | Ra
2 | Rb
3 | Rc
4 | Ra + Rb – Rc
5 | Ra + (Rb – Rc) / 2
6 | Rb + (Ra – Rc) / 2
7 | (Ra + Rb) / 2
Predictors 1-3 are 1-dimensional predictors, whereas Predictors 4-7 are 2-dimensional predictors. The best predictor for a particular image depends on the image. See also TJPARAM_LOSSLESS
TJPARAM_LOSSLESSPT | Lossless JPEG point transform (Pt) Value `0` through precision - 1, where precision is the JPEG data precision in bits [default for compression: `0`] A point transform value of `0` is necessary in order to generate a fully lossless JPEG image. (A non-zero point transform value right-shifts the input samples by the specified number of bits, which is effectively a form of lossy color quantization.) See also TJPARAM_LOSSLESS, TJPARAM_PRECISION
TJPARAM_RESTARTBLOCKS | JPEG restart marker interval in MCUs [lossy compression, lossless transformation]. The nature of entropy coding is such that a corrupt JPEG image cannot be decompressed beyond the point of corruption unless it contains restart markers. A restart marker stops and restarts the entropy coding algorithm so that, if a JPEG image is corrupted, decompression can resume at the next marker. Thus, adding more restart markers improves the fault tolerance of the JPEG image, but adding too many restart markers can adversely affect the compression ratio and performance. In typical JPEG images, an MCU (Minimum Coded Unit) is the minimum set of interleaved "data units" (8x8 DCT blocks if the image is lossy or samples if the image is lossless) necessary to represent at least one data unit per component. (For example, an MCU in an interleaved lossy JPEG image that uses 4:2:2 subsampling consists of two luminance blocks followed by one block for each chrominance component.) In single-component or non-interleaved JPEG images, an MCU is the same as a data unit. Value the number of MCUs between each restart marker [default: `0` (no restart markers)] Setting this parameter to a non-zero value sets TJPARAM_RESTARTROWS to 0.
TJPARAM_RESTARTROWS | JPEG restart marker interval in MCU rows [compression, lossless transformation]. See TJPARAM_RESTARTBLOCKS for a description of restart markers and MCUs. An MCU row is a row of MCUs spanning the entire width of the image. Value the number of MCU rows between each restart marker [default: `0` (no restart markers)] Setting this parameter to a non-zero value sets TJPARAM_RESTARTBLOCKS to 0.
TJPARAM_XDENSITY | JPEG horizontal pixel density. Value The JPEG image has (decompression) or will have (compression) the specified horizontal pixel density [default for compression: `1`]. This value is stored in or read from the JPEG header. It does not affect the contents of the JPEG image. Note that this parameter is set by tj3LoadImage8() when loading a Windows BMP file that contains pixel density information, and the value of this parameter is stored to a Windows BMP file by tj3SaveImage8() if the value of TJPARAM_DENSITYUNITS is `2`. This parameter has no effect unless the JPEG colorspace (see TJPARAM_COLORSPACE) is TJCS_YCbCr or TJCS_GRAY. See also TJPARAM_DENSITYUNITS
TJPARAM_YDENSITY | JPEG vertical pixel density. Value The JPEG image has (decompression) or will have (compression) the specified vertical pixel density [default for compression: `1`]. This value is stored in or read from the JPEG header. It does not affect the contents of the JPEG image. Note that this parameter is set by tj3LoadImage8() when loading a Windows BMP file that contains pixel density information, and the value of this parameter is stored to a Windows BMP file by tj3SaveImage8() if the value of TJPARAM_DENSITYUNITS is `2`. This parameter has no effect unless the JPEG colorspace (see TJPARAM_COLORSPACE) is TJCS_YCbCr or TJCS_GRAY. See also TJPARAM_DENSITYUNITS
TJPARAM_DENSITYUNITS | JPEG pixel density units. Value `0` [default for compression] The pixel density of the JPEG image is expressed (decompression) or will be expressed (compression) in unknown units. `1` The pixel density of the JPEG image is expressed (decompression) or will be expressed (compression) in units of pixels/inch. `2` The pixel density of the JPEG image is expressed (decompression) or will be expressed (compression) in units of pixels/cm. This value is stored in or read from the JPEG header. It does not affect the contents of the JPEG image. Note that this parameter is set by tj3LoadImage8() when loading a Windows BMP file that contains pixel density information, and the value of this parameter is stored to a Windows BMP file by tj3SaveImage8() if the value is `2`. This parameter has no effect unless the JPEG colorspace (see TJPARAM_COLORSPACE) is TJCS_YCbCr or TJCS_GRAY. See also TJPARAM_XDENSITY, TJPARAM_YDENSITY
TJPARAM_MAXMEMORY | Memory limit for intermediate buffers. Value the maximum amount of memory (in megabytes) that will be allocated for intermediate buffers, which are used with progressive JPEG compression and decompression, Huffman table optimization, lossless JPEG compression, and lossless transformation [default: `0` (no limit)]
TJPARAM_MAXPIXELS | Image size limit [decompression, lossless transformation, packed-pixel image loading]. Setting this parameter causes the decompression, transform, and image loading functions to return an error if the number of pixels in the source image exceeds the specified limit. This allows security-critical applications to guard against excessive memory consumption. Value maximum number of pixels that the decompression, transform, and image loading functions will process [default: `0` (no limit)]
TJPARAM_SAVEMARKERS | Marker copying behavior [decompression, lossless transformation]. Value [lossless transformation] `0` Do not copy any extra markers (including comments, JFIF thumbnails, Exif data, and ICC profile data) from the source image to the destination image. `1` Do not copy any extra markers, except comment (COM) markers, from the source image to the destination image. `2` [default] Copy all extra markers from the source image to the destination image. `3` Copy all extra markers, except ICC profile data (APP2 markers), from the source image to the destination image. `4` Do not copy any extra markers, except ICC profile data (APP2 markers), from the source image to the destination image. TJXOPT_COPYNONE overrides this parameter for a particular transform. This parameter overrides any ICC profile that was previously associated with the TurboJPEG instance using tj3SetICCProfile(). When decompressing, tj3DecompressHeader() extracts the ICC profile from a JPEG image if this parameter is set to `2` or `4`. tj3GetICCProfile() can then be used to retrieve the profile.

## ◆ TJPF

enum TJPF

Pixel formats.

Enumerator
TJPF_RGB | RGB pixel format. The red, green, and blue components in the image are stored in 3-sample pixels in the order R, G, B from lowest to highest memory address within each pixel.
TJPF_BGR | BGR pixel format. The red, green, and blue components in the image are stored in 3-sample pixels in the order B, G, R from lowest to highest memory address within each pixel.
TJPF_RGBX | RGBX pixel format. The red, green, and blue components in the image are stored in 4-sample pixels in the order R, G, B from lowest to highest memory address within each pixel. The X component is ignored when compressing/encoding and undefined when decompressing/decoding.
TJPF_BGRX | BGRX pixel format. The red, green, and blue components in the image are stored in 4-sample pixels in the order B, G, R from lowest to highest memory address within each pixel. The X component is ignored when compressing/encoding and undefined when decompressing/decoding.
TJPF_XBGR | XBGR pixel format. The red, green, and blue components in the image are stored in 4-sample pixels in the order R, G, B from highest to lowest memory address within each pixel. The X component is ignored when compressing/encoding and undefined when decompressing/decoding.
TJPF_XRGB | XRGB pixel format. The red, green, and blue components in the image are stored in 4-sample pixels in the order B, G, R from highest to lowest memory address within each pixel. The X component is ignored when compressing/encoding and undefined when decompressing/decoding.
TJPF_GRAY | Grayscale pixel format. Each 1-sample pixel represents a luminance (brightness) level from 0 to the maximum sample value (which is, for instance, 255 for 8-bit samples or 4095 for 12-bit samples or 65535 for 16-bit samples.)
TJPF_RGBA | RGBA pixel format. This is the same as TJPF_RGBX, except that when decompressing/decoding, the X component is guaranteed to be equal to the maximum sample value, which can be interpreted as an opaque alpha channel.
TJPF_BGRA | BGRA pixel format. This is the same as TJPF_BGRX, except that when decompressing/decoding, the X component is guaranteed to be equal to the maximum sample value, which can be interpreted as an opaque alpha channel.
TJPF_ABGR | ABGR pixel format. This is the same as TJPF_XBGR, except that when decompressing/decoding, the X component is guaranteed to be equal to the maximum sample value, which can be interpreted as an opaque alpha channel.
TJPF_ARGB | ARGB pixel format. This is the same as TJPF_XRGB, except that when decompressing/decoding, the X component is guaranteed to be equal to the maximum sample value, which can be interpreted as an opaque alpha channel.
TJPF_CMYK | CMYK pixel format. Unlike RGB, which is an additive color model used primarily for display, CMYK (Cyan/Magenta/Yellow/Key) is a subtractive color model used primarily for printing. In the CMYK color model, the value of each color component typically corresponds to an amount of cyan, magenta, yellow, or black ink that is applied to a white background. In order to convert between CMYK and RGB, it is necessary to use a color management system (CMS.) A CMS will attempt to map colors within the printer's gamut to perceptually similar colors in the display's gamut and vice versa, but the mapping is typically not 1:1 or reversible, nor can it be defined with a simple formula. Thus, such a conversion is out of scope for a codec library. However, the TurboJPEG API allows for compressing packed-pixel CMYK images into YCCK JPEG images (see TJCS_YCCK) and decompressing YCCK JPEG images into packed-pixel CMYK images.
TJPF_UNKNOWN | Unknown pixel format. Currently this is only used by tj3LoadImage8(), tj3LoadImage12(), and tj3LoadImage16().

## ◆ TJSAMP

enum TJSAMP

Chrominance subsampling options.

When pixels are converted from RGB to YCbCr (see TJCS_YCbCr) or from CMYK to YCCK (see TJCS_YCCK) as part of the JPEG compression process, some of the Cb and Cr (chrominance) components can be discarded or averaged together to produce a smaller image with little perceptible loss of image quality. (The human eye is more sensitive to small changes in brightness than to small changes in color.) This is called "chrominance subsampling".

Enumerator
TJSAMP_444 | 4:4:4 chrominance subsampling (no chrominance subsampling) The JPEG or YUV image will contain one chrominance component for every pixel in the source image.
TJSAMP_422 | 4:2:2 chrominance subsampling The JPEG or YUV image will contain one chrominance component for every 2x1 block of pixels in the source image.
TJSAMP_420 | 4:2:0 chrominance subsampling The JPEG or YUV image will contain one chrominance component for every 2x2 block of pixels in the source image.
TJSAMP_GRAY | Grayscale. The JPEG or YUV image will contain no chrominance components.
TJSAMP_440 | 4:4:0 chrominance subsampling The JPEG or YUV image will contain one chrominance component for every 1x2 block of pixels in the source image. Note 4:4:0 subsampling is not fully accelerated in libjpeg-turbo.
TJSAMP_411 | 4:1:1 chrominance subsampling The JPEG or YUV image will contain one chrominance component for every 4x1 block of pixels in the source image. All else being equal, a JPEG image with 4:1:1 subsampling is almost exactly the same size as a JPEG image with 4:2:0 subsampling, and in the aggregate, both subsampling methods produce approximately the same perceptual quality. However, 4:1:1 is better able to reproduce sharp horizontal features. Note 4:1:1 subsampling is not fully accelerated in libjpeg-turbo.
TJSAMP_441 | 4:4:1 chrominance subsampling The JPEG or YUV image will contain one chrominance component for every 1x4 block of pixels in the source image. All else being equal, a JPEG image with 4:4:1 subsampling is almost exactly the same size as a JPEG image with 4:2:0 subsampling, and in the aggregate, both subsampling methods produce approximately the same perceptual quality. However, 4:4:1 is better able to reproduce sharp vertical features. Note 4:4:1 subsampling is not fully accelerated in libjpeg-turbo.
TJSAMP_UNKNOWN | Unknown subsampling. The JPEG image uses an unusual type of chrominance subsampling. Such images can be decompressed into packed-pixel images, but they cannot be decompressed into planar YUV images, losslessly transformed if TJXOPT_CROP is specified and TJXOPT_GRAY is not specified, or partially decompressed using a cropping region.

## ◆ TJXOP

enum TJXOP

Transform operations for tj3Transform()

Enumerator
TJXOP_NONE | Do not transform the position of the image pixels.
TJXOP_HFLIP | Flip (mirror) image horizontally. This transform is imperfect if there are any partial iMCUs on the right edge (see TJXOPT_PERFECT.)
TJXOP_VFLIP | Flip (mirror) image vertically. This transform is imperfect if there are any partial iMCUs on the bottom edge (see TJXOPT_PERFECT.)
TJXOP_TRANSPOSE | Transpose image (flip/mirror along upper left to lower right axis.) This transform is always perfect.
TJXOP_TRANSVERSE | Transverse transpose image (flip/mirror along upper right to lower left axis.) This transform is imperfect if there are any partial iMCUs in the image (see TJXOPT_PERFECT.)
TJXOP_ROT90 | Rotate image clockwise by 90 degrees. This transform is imperfect if there are any partial iMCUs on the bottom edge (see TJXOPT_PERFECT.)
TJXOP_ROT180 | Rotate image 180 degrees. This transform is imperfect if there are any partial iMCUs in the image (see TJXOPT_PERFECT.)
TJXOP_ROT270 | Rotate image counter-clockwise by 90 degrees. This transform is imperfect if there are any partial iMCUs on the right edge (see TJXOPT_PERFECT.)

## Function Documentation

## ◆ tj3Alloc()

DLLEXPORT void * tj3Alloc | ( | size_t | bytes | ) |

Allocate a byte buffer for use with TurboJPEG.

You should always use this function to allocate the JPEG destination buffer(s) for the compression and transform functions unless you are disabling automatic buffer (re)allocation (by setting TJPARAM_NOREALLOC.)

Parameters

  bytes | the number of bytes to allocate

Returns
  a pointer to a newly-allocated buffer with the specified number of bytes.

See also
  tj3Free()

## ◆ tj3Compress12()

DLLEXPORT int tj3Compress12 | ( | tjhandle | handle,
|  | const short * | srcBuf,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat,
|  | unsigned char ** | jpegBuf,
|  | size_t * | jpegSize
| ) |  |

Compress a packed-pixel RGB, grayscale, or CMYK image with 9 to 12 bits of data precision per sample into a JPEG image with the same data precision.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for compression
  srcBuf | pointer to a buffer containing a packed-pixel RGB, grayscale, or CMYK source image to be compressed. This buffer should normally be `pitch * height` samples in size. However, you can also use this parameter to compress from a specific region of a larger buffer. The data precision of the source image (from 9 to 12 bits per sample) can be specified using TJPARAM_PRECISION and defaults to 12 if TJPARAM_PRECISION is unset or out of range.
  width | width (in pixels) of the source image
  pitch | samples per row in the source image. Normally this should be `width * tjPixelSize[pixelFormat]`, if the image is unpadded. (Setting this parameter to 0 is the equivalent of setting it to `width * tjPixelSize[pixelFormat]`.) However, you can also use this parameter to specify the row alignment/padding of the source image, to skip rows, or to compress from a specific region of a larger buffer.
  height | height (in pixels) of the source image
  pixelFormat | pixel format of the source image (see Pixel formats.)
  jpegBuf | address of a pointer to a byte buffer that will receive the JPEG image. TurboJPEG has the ability to reallocate the JPEG buffer to accommodate the size of the JPEG image. Thus, you can choose to: pre-allocate the JPEG buffer with an arbitrary size using tj3Alloc() and let TurboJPEG grow the buffer as needed, set `*jpegBuf` to NULL to tell TurboJPEG to allocate the buffer for you, or pre-allocate the buffer to a "worst case" size determined by calling tj3JPEGBufSize() and adding the return value to the size of the ICC profile (if any) that was previously associated with the TurboJPEG instance (see tj3SetICCProfile().) This should ensure that the buffer never has to be re-allocated. (Setting TJPARAM_NOREALLOC guarantees that it won't be.) If you choose option 1 or 3, then `*jpegSize` should be set to the size of your pre-allocated buffer. In any case, unless you have set TJPARAM_NOREALLOC, you should always check `*jpegBuf` upon return from this function, as it may have changed.
  jpegSize | pointer to a size_t variable that holds the size of the JPEG buffer. If `*jpegBuf` points to a pre-allocated buffer, then `*jpegSize` should be set to the size of the buffer. Upon return, `*jpegSize` will contain the size of the JPEG image (in bytes.) If `*jpegBuf` points to a JPEG buffer that is being reused from a previous call to one of the JPEG compression functions, then `*jpegSize` is ignored.

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3Compress16()

DLLEXPORT int tj3Compress16 | ( | tjhandle | handle,
|  | const unsigned short * | srcBuf,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat,
|  | unsigned char ** | jpegBuf,
|  | size_t * | jpegSize
| ) |  |

Compress a packed-pixel RGB, grayscale, or CMYK image with 13 to 16 bits of data precision per sample into a lossless JPEG image with the same data precision.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for compression
  srcBuf | pointer to a buffer containing a packed-pixel RGB, grayscale, or CMYK source image to be compressed. This buffer should normally be `pitch * height` samples in size. However, you can also use this parameter to compress from a specific region of a larger buffer. The data precision of the source image (from 13 to 16 bits per sample) can be specified using TJPARAM_PRECISION and defaults to 16 if TJPARAM_PRECISION is unset or out of range.
  width | width (in pixels) of the source image
  pitch | samples per row in the source image. Normally this should be `width * tjPixelSize[pixelFormat]`, if the image is unpadded. (Setting this parameter to 0 is the equivalent of setting it to `width * tjPixelSize[pixelFormat]`.) However, you can also use this parameter to specify the row alignment/padding of the source image, to skip rows, or to compress from a specific region of a larger buffer.
  height | height (in pixels) of the source image
  pixelFormat | pixel format of the source image (see Pixel formats.)
  jpegBuf | address of a pointer to a byte buffer that will receive the JPEG image. TurboJPEG has the ability to reallocate the JPEG buffer to accommodate the size of the JPEG image. Thus, you can choose to: pre-allocate the JPEG buffer with an arbitrary size using tj3Alloc() and let TurboJPEG grow the buffer as needed, set `*jpegBuf` to NULL to tell TurboJPEG to allocate the buffer for you, or pre-allocate the buffer to a "worst case" size determined by calling tj3JPEGBufSize() and adding the return value to the size of the ICC profile (if any) that was previously associated with the TurboJPEG instance (see tj3SetICCProfile().) This should ensure that the buffer never has to be re-allocated. (Setting TJPARAM_NOREALLOC guarantees that it won't be.) If you choose option 1 or 3, then `*jpegSize` should be set to the size of your pre-allocated buffer. In any case, unless you have set TJPARAM_NOREALLOC, you should always check `*jpegBuf` upon return from this function, as it may have changed.
  jpegSize | pointer to a size_t variable that holds the size of the JPEG buffer. If `*jpegBuf` points to a pre-allocated buffer, then `*jpegSize` should be set to the size of the buffer. Upon return, `*jpegSize` will contain the size of the JPEG image (in bytes.) If `*jpegBuf` points to a JPEG buffer that is being reused from a previous call to one of the JPEG compression functions, then `*jpegSize` is ignored.

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3Compress8()

DLLEXPORT int tj3Compress8 | ( | tjhandle | handle,
|  | const unsigned char * | srcBuf,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat,
|  | unsigned char ** | jpegBuf,
|  | size_t * | jpegSize
| ) |  |

Compress a packed-pixel RGB, grayscale, or CMYK image with 2 to 8 bits of data precision per sample into a JPEG image with the same data precision.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for compression
  srcBuf | pointer to a buffer containing a packed-pixel RGB, grayscale, or CMYK source image to be compressed. This buffer should normally be `pitch * height` samples in size. However, you can also use this parameter to compress from a specific region of a larger buffer. The data precision of the source image (from 2 to 8 bits per sample) can be specified using TJPARAM_PRECISION and defaults to 8 if TJPARAM_PRECISION is unset or out of range.
  width | width (in pixels) of the source image
  pitch | samples per row in the source image. Normally this should be `width * tjPixelSize[pixelFormat]`, if the image is unpadded. (Setting this parameter to 0 is the equivalent of setting it to `width * tjPixelSize[pixelFormat]`.) However, you can also use this parameter to specify the row alignment/padding of the source image, to skip rows, or to compress from a specific region of a larger buffer.
  height | height (in pixels) of the source image
  pixelFormat | pixel format of the source image (see Pixel formats.)
  jpegBuf | address of a pointer to a byte buffer that will receive the JPEG image. TurboJPEG has the ability to reallocate the JPEG buffer to accommodate the size of the JPEG image. Thus, you can choose to: pre-allocate the JPEG buffer with an arbitrary size using tj3Alloc() and let TurboJPEG grow the buffer as needed, set `*jpegBuf` to NULL to tell TurboJPEG to allocate the buffer for you, or pre-allocate the buffer to a "worst case" size determined by calling tj3JPEGBufSize() and adding the return value to the size of the ICC profile (if any) that was previously associated with the TurboJPEG instance (see tj3SetICCProfile().) This should ensure that the buffer never has to be re-allocated. (Setting TJPARAM_NOREALLOC guarantees that it won't be.) If you choose option 1 or 3, then `*jpegSize` should be set to the size of your pre-allocated buffer. In any case, unless you have set TJPARAM_NOREALLOC, you should always check `*jpegBuf` upon return from this function, as it may have changed.
  jpegSize | pointer to a size_t variable that holds the size of the JPEG buffer. If `*jpegBuf` points to a pre-allocated buffer, then `*jpegSize` should be set to the size of the buffer. Upon return, `*jpegSize` will contain the size of the JPEG image (in bytes.) If `*jpegBuf` points to a JPEG buffer that is being reused from a previous call to one of the JPEG compression functions, then `*jpegSize` is ignored.

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3CompressFromYUV8()

DLLEXPORT int tj3CompressFromYUV8 | ( | tjhandle | handle,
|  | const unsigned char * | srcBuf,
|  | int | width,
|  | int | align,
|  | int | height,
|  | unsigned char ** | jpegBuf,
|  | size_t * | jpegSize
| ) |  |

Compress an 8-bit-per-sample unified planar YUV image into an 8-bit-per-sample JPEG image.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for compression
  srcBuf | pointer to a buffer containing a unified planar YUV source image to be compressed. The size of this buffer should match the value returned by tj3YUVBufSize() for the given image width, height, row alignment, and level of chrominance subsampling (see TJPARAM_SUBSAMP.) The Y, U (Cb), and V (Cr) image planes should be stored sequentially in the buffer. (Refer to YUV Image Format Notes.)
  width | width (in pixels) of the source image. If the width is not an even multiple of the iMCU width (see tjMCUWidth), then an intermediate buffer copy will be performed.
  align | row alignment (in bytes) of the source image (must be a power of 2.) Setting this parameter to n indicates that each row in each plane of the source image is padded to the nearest multiple of n bytes (1 = unpadded.)
  height | height (in pixels) of the source image. If the height is not an even multiple of the iMCU height (see tjMCUHeight), then an intermediate buffer copy will be performed.
  jpegBuf | address of a pointer to a byte buffer that will receive the JPEG image. TurboJPEG has the ability to reallocate the JPEG buffer to accommodate the size of the JPEG image. Thus, you can choose to: pre-allocate the JPEG buffer with an arbitrary size using tj3Alloc() and let TurboJPEG grow the buffer as needed, set `*jpegBuf` to NULL to tell TurboJPEG to allocate the buffer for you, or pre-allocate the buffer to a "worst case" size determined by calling tj3JPEGBufSize() and adding the return value to the size of the ICC profile (if any) that was previously associated with the TurboJPEG instance (see tj3SetICCProfile().) This should ensure that the buffer never has to be re-allocated. (Setting TJPARAM_NOREALLOC guarantees that it won't be.) If you choose option 1 or 3, then `*jpegSize` should be set to the size of your pre-allocated buffer. In any case, unless you have set TJPARAM_NOREALLOC, you should always check `*jpegBuf` upon return from this function, as it may have changed.
  jpegSize | pointer to a size_t variable that holds the size of the JPEG buffer. If `*jpegBuf` points to a pre-allocated buffer, then `*jpegSize` should be set to the size of the buffer. Upon return, `*jpegSize` will contain the size of the JPEG image (in bytes.) If `*jpegBuf` points to a JPEG buffer that is being reused from a previous call to one of the JPEG compression functions, then `*jpegSize` is ignored.

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3CompressFromYUVPlanes8()

DLLEXPORT int tj3CompressFromYUVPlanes8 | ( | tjhandle | handle,
|  | const unsigned char *const * | srcPlanes,
|  | int | width,
|  | const int * | strides,
|  | int | height,
|  | unsigned char ** | jpegBuf,
|  | size_t * | jpegSize
| ) |  |

Compress a set of 8-bit-per-sample Y, U (Cb), and V (Cr) image planes into an 8-bit-per-sample JPEG image.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for compression
  srcPlanes | an array of pointers to Y, U (Cb), and V (Cr) image planes (or just a Y plane, if compressing a grayscale image) that contain a YUV source image to be compressed. These planes can be contiguous or non-contiguous in memory. The size of each plane should match the value returned by tj3YUVPlaneSize() for the given image width, height, strides, and level of chrominance subsampling (see TJPARAM_SUBSAMP.) Refer to YUV Image Format Notes for more details.
  width | width (in pixels) of the source image. If the width is not an even multiple of the iMCU width (see tjMCUWidth), then an intermediate buffer copy will be performed.
  strides | an array of integers, each specifying the number of bytes per row in the corresponding plane of the YUV source image. Setting the stride for any plane to 0 is the same as setting it to the plane width (see YUV Image Format Notes.) If `strides` is NULL, then the strides for all planes will be set to their respective plane widths. You can adjust the strides in order to specify an arbitrary amount of row padding in each plane or to create a JPEG image from a subregion of a larger planar YUV image.
  height | height (in pixels) of the source image. If the height is not an even multiple of the iMCU height (see tjMCUHeight), then an intermediate buffer copy will be performed.
  jpegBuf | address of a pointer to a byte buffer that will receive the JPEG image. TurboJPEG has the ability to reallocate the JPEG buffer to accommodate the size of the JPEG image. Thus, you can choose to: pre-allocate the JPEG buffer with an arbitrary size using tj3Alloc() and let TurboJPEG grow the buffer as needed, set `*jpegBuf` to NULL to tell TurboJPEG to allocate the buffer for you, or pre-allocate the buffer to a "worst case" size determined by calling tj3JPEGBufSize() and adding the return value to the size of the ICC profile (if any) that was previously associated with the TurboJPEG instance (see tj3SetICCProfile().) This should ensure that the buffer never has to be re-allocated. (Setting TJPARAM_NOREALLOC guarantees that it won't be.) If you choose option 1 or 3, then `*jpegSize` should be set to the size of your pre-allocated buffer. In any case, unless you have set TJPARAM_NOREALLOC, you should always check `*jpegBuf` upon return from this function, as it may have changed.
  jpegSize | pointer to a size_t variable that holds the size of the JPEG buffer. If `*jpegBuf` points to a pre-allocated buffer, then `*jpegSize` should be set to the size of the buffer. Upon return, `*jpegSize` will contain the size of the JPEG image (in bytes.) If `*jpegBuf` points to a JPEG buffer that is being reused from a previous call to one of the JPEG compression functions, then `*jpegSize` is ignored.

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3DecodeYUV8()

DLLEXPORT int tj3DecodeYUV8 | ( | tjhandle | handle,
|  | const unsigned char * | srcBuf,
|  | int | align,
|  | unsigned char * | dstBuf,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat
| ) |  |

Decode an 8-bit-per-sample unified planar YUV image into an 8-bit-per-sample packed-pixel RGB or grayscale image.

This function performs color conversion (which is accelerated in the libjpeg-turbo implementation) but does not execute any of the other steps in the JPEG decompression process.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for decompression
  srcBuf | pointer to a buffer containing a unified planar YUV source image to be decoded. The size of this buffer should match the value returned by tj3YUVBufSize() for the given image width, height, row alignment, and level of chrominance subsampling (see TJPARAM_SUBSAMP.) The Y, U (Cb), and V (Cr) image planes should be stored sequentially in the source buffer. (Refer to YUV Image Format Notes.)
  align | row alignment (in bytes) of the YUV source image (must be a power of 2.) Setting this parameter to n indicates that each row in each plane of the YUV source image is padded to the nearest multiple of n bytes (1 = unpadded.)
  dstBuf | pointer to a buffer that will receive the packed-pixel decoded image. This buffer should normally be `pitch * height` bytes in size. However, you can also use this parameter to decode into a specific region of a larger buffer.
  width | width (in pixels) of the source and destination images
  pitch | bytes per row in the destination image. Normally this should be set to `width * tjPixelSize[pixelFormat]`, if the destination image should be unpadded. (Setting this parameter to 0 is the equivalent of setting it to `width * tjPixelSize[pixelFormat]`.) However, you can also use this parameter to specify the row alignment/padding of the destination image, to skip rows, or to decode into a specific region of a larger buffer.
  height | height (in pixels) of the source and destination images
  pixelFormat | pixel format of the destination image (see Pixel formats.)

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3DecodeYUVPlanes8()

DLLEXPORT int tj3DecodeYUVPlanes8 | ( | tjhandle | handle,
|  | const unsigned char *const * | srcPlanes,
|  | const int * | strides,
|  | unsigned char * | dstBuf,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat
| ) |  |

Decode a set of 8-bit-per-sample Y, U (Cb), and V (Cr) image planes into an 8-bit-per-sample packed-pixel RGB or grayscale image.

This function performs color conversion (which is accelerated in the libjpeg-turbo implementation) but does not execute any of the other steps in the JPEG decompression process.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for decompression
  srcPlanes | an array of pointers to Y, U (Cb), and V (Cr) image planes (or just a Y plane, if decoding a grayscale image) that contain a YUV image to be decoded. These planes can be contiguous or non-contiguous in memory. The size of each plane should match the value returned by tj3YUVPlaneSize() for the given image width, height, strides, and level of chrominance subsampling (see TJPARAM_SUBSAMP.) Refer to YUV Image Format Notes for more details.
  strides | an array of integers, each specifying the number of bytes per row in the corresponding plane of the YUV source image. Setting the stride for any plane to 0 is the same as setting it to the plane width (see YUV Image Format Notes.) If `strides` is NULL, then the strides for all planes will be set to their respective plane widths. You can adjust the strides in order to specify an arbitrary amount of row padding in each plane or to decode a subregion of a larger planar YUV image.
  dstBuf | pointer to a buffer that will receive the packed-pixel decoded image. This buffer should normally be `pitch * height` bytes in size. However, you can also use this parameter to decode into a specific region of a larger buffer.
  width | width (in pixels) of the source and destination images
  pitch | bytes per row in the destination image. Normally this should be set to `width * tjPixelSize[pixelFormat]`, if the destination image should be unpadded. (Setting this parameter to 0 is the equivalent of setting it to `width * tjPixelSize[pixelFormat]`.) However, you can also use this parameter to specify the row alignment/padding of the destination image, to skip rows, or to decode into a specific region of a larger buffer.
  height | height (in pixels) of the source and destination images
  pixelFormat | pixel format of the destination image (see Pixel formats.)

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3Decompress12()

DLLEXPORT int tj3Decompress12 | ( | tjhandle | handle,
|  | const unsigned char * | jpegBuf,
|  | size_t | jpegSize,
|  | short * | dstBuf,
|  | int | pitch,
|  | int | pixelFormat
| ) |  |

Decompress a JPEG image with 9 to 12 bits of data precision per sample into a packed-pixel RGB, grayscale, or CMYK image with the same data precision.

The parameters that describe the JPEG image will be set when this function returns.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for decompression
  jpegBuf | pointer to a byte buffer containing the JPEG image to decompress
  jpegSize | size of the JPEG image (in bytes)
  dstBuf | pointer to a buffer that will receive the packed-pixel decompressed image. This buffer should normally be `pitch * destinationHeight` samples in size. However, you can also use this parameter to decompress into a specific region of a larger buffer. NOTE: If the JPEG image is lossy, then `destinationHeight` is either the scaled JPEG height (see TJSCALED(), TJPARAM_JPEGHEIGHT, and tj3SetScalingFactor()) or the height of the cropping region (see tj3SetCroppingRegion().) If the JPEG image is lossless, then `destinationHeight` is the JPEG height.
  pitch | samples per row in the destination image. Normally this should be set to `destinationWidth * tjPixelSize[pixelFormat]`, if the destination image should be unpadded. (Setting this parameter to 0 is the equivalent of setting it to `destinationWidth * tjPixelSize[pixelFormat]`.) However, you can also use this parameter to specify the row alignment/padding of the destination image, to skip rows, or to decompress into a specific region of a larger buffer. NOTE: If the JPEG image is lossy, then `destinationWidth` is either the scaled JPEG width (see TJSCALED(), TJPARAM_JPEGWIDTH, and tj3SetScalingFactor()) or the width of the cropping region (see tj3SetCroppingRegion().) If the JPEG image is lossless, then `destinationWidth` is the JPEG width.
  pixelFormat | pixel format of the destination image (see Pixel formats.)

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3Decompress16()

DLLEXPORT int tj3Decompress16 | ( | tjhandle | handle,
|  | const unsigned char * | jpegBuf,
|  | size_t | jpegSize,
|  | unsigned short * | dstBuf,
|  | int | pitch,
|  | int | pixelFormat
| ) |  |

Decompress a lossless JPEG image with 13 to 16 bits of data precision per sample into a packed-pixel RGB, grayscale, or CMYK image with the same data precision.

The parameters that describe the JPEG image will be set when this function returns.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for decompression
  jpegBuf | pointer to a byte buffer containing the JPEG image to decompress
  jpegSize | size of the JPEG image (in bytes)
  dstBuf | pointer to a buffer that will receive the packed-pixel decompressed image. This buffer should normally be `pitch * destinationHeight` samples in size. However, you can also use this parameter to decompress into a specific region of a larger buffer. NOTE: If the JPEG image is lossy, then `destinationHeight` is either the scaled JPEG height (see TJSCALED(), TJPARAM_JPEGHEIGHT, and tj3SetScalingFactor()) or the height of the cropping region (see tj3SetCroppingRegion().) If the JPEG image is lossless, then `destinationHeight` is the JPEG height.
  pitch | samples per row in the destination image. Normally this should be set to `destinationWidth * tjPixelSize[pixelFormat]`, if the destination image should be unpadded. (Setting this parameter to 0 is the equivalent of setting it to `destinationWidth * tjPixelSize[pixelFormat]`.) However, you can also use this parameter to specify the row alignment/padding of the destination image, to skip rows, or to decompress into a specific region of a larger buffer. NOTE: If the JPEG image is lossy, then `destinationWidth` is either the scaled JPEG width (see TJSCALED(), TJPARAM_JPEGWIDTH, and tj3SetScalingFactor()) or the width of the cropping region (see tj3SetCroppingRegion().) If the JPEG image is lossless, then `destinationWidth` is the JPEG width.
  pixelFormat | pixel format of the destination image (see Pixel formats.)

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3Decompress8()

DLLEXPORT int tj3Decompress8 | ( | tjhandle | handle,
|  | const unsigned char * | jpegBuf,
|  | size_t | jpegSize,
|  | unsigned char * | dstBuf,
|  | int | pitch,
|  | int | pixelFormat
| ) |  |

Decompress a JPEG image with 2 to 8 bits of data precision per sample into a packed-pixel RGB, grayscale, or CMYK image with the same data precision.

The parameters that describe the JPEG image will be set when this function returns.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for decompression
  jpegBuf | pointer to a byte buffer containing the JPEG image to decompress
  jpegSize | size of the JPEG image (in bytes)
  dstBuf | pointer to a buffer that will receive the packed-pixel decompressed image. This buffer should normally be `pitch * destinationHeight` samples in size. However, you can also use this parameter to decompress into a specific region of a larger buffer. NOTE: If the JPEG image is lossy, then `destinationHeight` is either the scaled JPEG height (see TJSCALED(), TJPARAM_JPEGHEIGHT, and tj3SetScalingFactor()) or the height of the cropping region (see tj3SetCroppingRegion().) If the JPEG image is lossless, then `destinationHeight` is the JPEG height.
  pitch | samples per row in the destination image. Normally this should be set to `destinationWidth * tjPixelSize[pixelFormat]`, if the destination image should be unpadded. (Setting this parameter to 0 is the equivalent of setting it to `destinationWidth * tjPixelSize[pixelFormat]`.) However, you can also use this parameter to specify the row alignment/padding of the destination image, to skip rows, or to decompress into a specific region of a larger buffer. NOTE: If the JPEG image is lossy, then `destinationWidth` is either the scaled JPEG width (see TJSCALED(), TJPARAM_JPEGWIDTH, and tj3SetScalingFactor()) or the width of the cropping region (see tj3SetCroppingRegion().) If the JPEG image is lossless, then `destinationWidth` is the JPEG width.
  pixelFormat | pixel format of the destination image (see Pixel formats.)

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3DecompressHeader()

DLLEXPORT int tj3DecompressHeader | ( | tjhandle | handle,
|  | const unsigned char * | jpegBuf,
|  | size_t | jpegSize
| ) |  |

Retrieve information about a JPEG image without decompressing it, or prime the decompressor with quantization and Huffman tables.

If a JPEG image is passed to this function, then the parameters that describe the JPEG image will be set when the function returns. If a JPEG image is passed to this function and TJPARAM_SAVEMARKERS is set to `2` or `4`, then the ICC profile (if any) will be extracted from the JPEG image. (tj3GetICCProfile() can then be used to retrieve the profile.)

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for decompression
  jpegBuf | pointer to a byte buffer containing a JPEG image or an "abbreviated table specification" (AKA "tables-only") datastream. Passing a tables-only datastream to this function primes the decompressor with quantization and Huffman tables that can be used when decompressing subsequent "abbreviated image" datastreams. This is useful, for instance, when decompressing video streams in which all frames share the same quantization and Huffman tables.
  jpegSize | size of the JPEG image or tables-only datastream (in bytes)

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3DecompressToYUV8()

DLLEXPORT int tj3DecompressToYUV8 | ( | tjhandle | handle,
|  | const unsigned char * | jpegBuf,
|  | size_t | jpegSize,
|  | unsigned char * | dstBuf,
|  | int | align
| ) |  |

Decompress an 8-bit-per-sample JPEG image into an 8-bit-per-sample unified planar YUV image.

This function performs JPEG decompression but leaves out the color conversion step, so a planar YUV image is generated instead of a packed-pixel image. The parameters that describe the JPEG image will be set when this function returns.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for decompression
  jpegBuf | pointer to a byte buffer containing the JPEG image to decompress
  jpegSize | size of the JPEG image (in bytes)
  dstBuf | pointer to a buffer that will receive the unified planar YUV decompressed image. Use tj3YUVBufSize() to determine the appropriate size for this buffer based on the scaled JPEG width and height (see TJSCALED(), TJPARAM_JPEGWIDTH, TJPARAM_JPEGHEIGHT, and tj3SetScalingFactor()), row alignment, and level of chrominance subsampling (see TJPARAM_SUBSAMP.) The Y, U (Cb), and V (Cr) image planes will be stored sequentially in the buffer. (Refer to YUV Image Format Notes.)
  align | row alignment (in bytes) of the YUV image (must be a power of 2.) Setting this parameter to n will cause each row in each plane of the YUV image to be padded to the nearest multiple of n bytes (1 = unpadded.) To generate images suitable for X Video, `align` should be set to 4.

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3DecompressToYUVPlanes8()

DLLEXPORT int tj3DecompressToYUVPlanes8 | ( | tjhandle | handle,
|  | const unsigned char * | jpegBuf,
|  | size_t | jpegSize,
|  | unsigned char ** | dstPlanes,
|  | int * | strides
| ) |  |

Decompress an 8-bit-per-sample JPEG image into separate 8-bit-per-sample Y, U (Cb), and V (Cr) image planes.

This function performs JPEG decompression but leaves out the color conversion step, so a planar YUV image is generated instead of a packed-pixel image. The parameters that describe the JPEG image will be set when this function returns.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for decompression
  jpegBuf | pointer to a byte buffer containing the JPEG image to decompress
  jpegSize | size of the JPEG image (in bytes)
  dstPlanes | an array of pointers to Y, U (Cb), and V (Cr) image planes (or just a Y plane, if decompressing a grayscale image) that will receive the decompressed image. These planes can be contiguous or non-contiguous in memory. Use tj3YUVPlaneSize() to determine the appropriate size for each plane based on the scaled JPEG width and height (see TJSCALED(), TJPARAM_JPEGWIDTH, TJPARAM_JPEGHEIGHT, and tj3SetScalingFactor()), strides, and level of chrominance subsampling (see TJPARAM_SUBSAMP.) Refer to YUV Image Format Notes for more details.
  strides | an array of integers, each specifying the number of bytes per row in the corresponding plane of the YUV image. Setting the stride for any plane to 0 is the same as setting it to the scaled plane width (see YUV Image Format Notes.) If `strides` is NULL, then the strides for all planes will be set to their respective scaled plane widths. You can adjust the strides in order to add an arbitrary amount of row padding to each plane or to decompress the JPEG image into a subregion of a larger planar YUV image.

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3Destroy()

DLLEXPORT void tj3Destroy | ( | tjhandle | handle | ) |

Destroy a TurboJPEG instance.

Parameters

  handle | handle to a TurboJPEG instance. If the handle is NULL, then this function has no effect.

## ◆ tj3EncodeYUV8()

DLLEXPORT int tj3EncodeYUV8 | ( | tjhandle | handle,
|  | const unsigned char * | srcBuf,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat,
|  | unsigned char * | dstBuf,
|  | int | align
| ) |  |

Encode an 8-bit-per-sample packed-pixel RGB or grayscale image into an 8-bit-per-sample unified planar YUV image.

This function performs color conversion (which is accelerated in the libjpeg-turbo implementation) but does not execute any of the other steps in the JPEG compression process.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for compression
  srcBuf | pointer to a buffer containing a packed-pixel RGB or grayscale source image to be encoded. This buffer should normally be `pitch * height` bytes in size. However, you can also use this parameter to encode from a specific region of a larger buffer.
  width | width (in pixels) of the source image
  pitch | bytes per row in the source image. Normally this should be `width * tjPixelSize[pixelFormat]`, if the image is unpadded. (Setting this parameter to 0 is the equivalent of setting it to `width * tjPixelSize[pixelFormat]`.) However, you can also use this parameter to specify the row alignment/padding of the source image, to skip rows, or to encode from a specific region of a larger packed-pixel image.
  height | height (in pixels) of the source image
  pixelFormat | pixel format of the source image (see Pixel formats.)
  dstBuf | pointer to a buffer that will receive the unified planar YUV image. Use tj3YUVBufSize() to determine the appropriate size for this buffer based on the image width, height, row alignment, and level of chrominance subsampling (see TJPARAM_SUBSAMP.) The Y, U (Cb), and V (Cr) image planes will be stored sequentially in the buffer. (Refer to YUV Image Format Notes.)
  align | row alignment (in bytes) of the YUV image (must be a power of 2.) Setting this parameter to n will cause each row in each plane of the YUV image to be padded to the nearest multiple of n bytes (1 = unpadded.) To generate images suitable for X Video, `align` should be set to 4.

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3EncodeYUVPlanes8()

DLLEXPORT int tj3EncodeYUVPlanes8 | ( | tjhandle | handle,
|  | const unsigned char * | srcBuf,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat,
|  | unsigned char ** | dstPlanes,
|  | int * | strides
| ) |  |

Encode an 8-bit-per-sample packed-pixel RGB or grayscale image into separate 8-bit-per-sample Y, U (Cb), and V (Cr) image planes.

This function performs color conversion (which is accelerated in the libjpeg-turbo implementation) but does not execute any of the other steps in the JPEG compression process.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for compression
  srcBuf | pointer to a buffer containing a packed-pixel RGB or grayscale source image to be encoded. This buffer should normally be `pitch * height` bytes in size. However, you can also use this parameter to encode from a specific region of a larger buffer.
  width | width (in pixels) of the source image
  pitch | bytes per row in the source image. Normally this should be `width * tjPixelSize[pixelFormat]`, if the image is unpadded. (Setting this parameter to 0 is the equivalent of setting it to `width * tjPixelSize[pixelFormat]`.) However, you can also use this parameter to specify the row alignment/padding of the source image, to skip rows, or to encode from a specific region of a larger packed-pixel image.
  height | height (in pixels) of the source image
  pixelFormat | pixel format of the source image (see Pixel formats.)
  dstPlanes | an array of pointers to Y, U (Cb), and V (Cr) image planes (or just a Y plane, if generating a grayscale image) that will receive the encoded image. These planes can be contiguous or non-contiguous in memory. Use tj3YUVPlaneSize() to determine the appropriate size for each plane based on the image width, height, strides, and level of chrominance subsampling (see TJPARAM_SUBSAMP.) Refer to YUV Image Format Notes for more details.
  strides | an array of integers, each specifying the number of bytes per row in the corresponding plane of the YUV image. Setting the stride for any plane to 0 is the same as setting it to the plane width (see YUV Image Format Notes.) If `strides` is NULL, then the strides for all planes will be set to their respective plane widths. You can adjust the strides in order to add an arbitrary amount of row padding to each plane or to encode an RGB or grayscale image into a subregion of a larger planar YUV image.

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3Free()

DLLEXPORT void tj3Free | ( | void * | buffer | ) |

Free a byte buffer previously allocated by TurboJPEG.

You should always use this function to free JPEG destination buffer(s) that were automatically (re)allocated by the compression and transform functions or that were manually allocated using tj3Alloc().

Parameters

  buffer | address of the buffer to free. If the address is NULL, then this function has no effect.

See also
  tj3Alloc()

## ◆ tj3Get()

DLLEXPORT int tj3Get | ( | tjhandle | handle,
|  | int | param
| ) |  |

Get the value of a parameter.

Parameters

  handle | handle to a TurboJPEG instance
  param | one of the parameters

Returns
  the value of the specified parameter, or -1 if the value is unknown.

## ◆ tj3GetErrorCode()

DLLEXPORT int tj3GetErrorCode | ( | tjhandle | handle | ) |

Returns a code indicating the severity of the last error.

See Error codes.

Parameters

  handle | handle to a TurboJPEG instance

Returns
  a code indicating the severity of the last error. See Error codes.

## ◆ tj3GetErrorStr()

DLLEXPORT char * tj3GetErrorStr | ( | tjhandle | handle | ) |

Returns a descriptive error message explaining why the last command failed.

Parameters

  handle | handle to a TurboJPEG instance, or NULL if the error was generated by a global function (but note that retrieving the error message for a global function is thread-safe only on platforms that support thread-local storage.)

Returns
  a descriptive error message explaining why the last command failed.

## ◆ tj3GetICCProfile()

DLLEXPORT int tj3GetICCProfile | ( | tjhandle | handle,
|  | unsigned char ** | iccBuf,
|  | size_t * | iccSize
| ) |  |

Retrieve the ICC (International Color Consortium) color management profile (if any) that was previously extracted from a JPEG image.

Note
  To extract the ICC profile from a JPEG image, call tj3DecompressHeader() with TJPARAM_SAVEMARKERS set to `2` or `4`. Once the ICC profile is retrieved, it must be re-extracted before it can be retrieved again.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for decompression
  iccBuf | address of a pointer to a byte buffer. Upon return: If `iccBuf` is not NULL and there is an ICC profile to retrieve, then `*iccBuf` will point to a byte buffer containing the ICC profile. This buffer should be freed using tj3Free(). If `iccBuf` is not NULL and there is no ICC profile to retrieve, then `*iccBuf` will be NULL. If `iccBuf` is NULL, then only the ICC profile size will be retrieved, and the ICC profile can be retrieved later.
  iccSize | address of a size_t variable. Upon return, the variable will contain the ICC profile size (or 0 if there is no ICC profile to retrieve.)

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3GetScalingFactors()

DLLEXPORT tjscalingfactor * tj3GetScalingFactors | ( | int * | numScalingFactors | ) |

Returns a list of fractional scaling factors that the JPEG decompressor supports.

Parameters

  numScalingFactors | pointer to an integer variable that will receive the number of elements in the list

Returns
  a pointer to a list of fractional scaling factors, or NULL if an error is encountered (see tj3GetErrorStr().)

## ◆ tj3Init()

DLLEXPORT tjhandle tj3Init | ( | int | initType | ) |

Create a new TurboJPEG instance.

Parameters

  initType | one of the initialization options

Returns
  a handle to the newly-created instance, or NULL if an error occurred (see tj3GetErrorStr().)

## ◆ tj3JPEGBufSize()

DLLEXPORT size_t tj3JPEGBufSize | ( | int | width,
|  | int | height,
|  | int | jpegSubsamp
| ) |  |

The maximum size of the buffer (in bytes) required to hold a JPEG image with the given parameters.

The number of bytes returned by this function is larger than the size of the uncompressed source image. The reason for this is that the JPEG format uses 16-bit coefficients, so it is possible for a very high-quality source image with very high-frequency content to expand rather than compress when converted to the JPEG format. Such images represent very rare corner cases, but since there is no way to predict the size of a JPEG image prior to compression, the corner cases have to be handled.

Parameters

  width | width (in pixels) of the image
  height | height (in pixels) of the image
  jpegSubsamp | the level of chrominance subsampling to be used when generating the JPEG image (see Chrominance subsampling options.) TJSAMP_UNKNOWN is treated like TJSAMP_444, since a buffer large enough to hold a JPEG image with no subsampling should also be large enough to hold a JPEG image with an arbitrary level of subsampling. Note that lossless JPEG images always use TJSAMP_444.

Returns
  the maximum size of the buffer (in bytes) required to hold the image, or 0 if the arguments are out of bounds.

## ◆ tj3LoadImage12()

DLLEXPORT short * tj3LoadImage12 | ( | tjhandle | handle,
|  | const char * | filename,
|  | int * | width,
|  | int | align,
|  | int * | height,
|  | int * | pixelFormat
| ) |  |

Load a packed-pixel image with 9 to 12 bits of data precision per sample from disk into memory.

Parameters

  handle | handle to a TurboJPEG instance
  filename | name of a file containing a packed-pixel image in PBMPLUS (PPM/PGM) format. The target data precision (from 9 to 12 bits per sample) can be specified using TJPARAM_PRECISION and defaults to 12 if TJPARAM_PRECISION is unset or out of range. If the data precision of the PBMPLUS file does not match the target data precision, then upconverting or downconverting will be performed.
  width | pointer to an integer variable that will receive the width (in pixels) of the packed-pixel image
  align | row alignment (in samples) of the packed-pixel buffer to be returned (must be a power of 2.) Setting this parameter to n will cause all rows in the buffer to be padded to the nearest multiple of n samples (1 = unpadded.)
  height | pointer to an integer variable that will receive the height (in pixels) of the packed-pixel image
  pixelFormat | pointer to an integer variable that specifies or will receive the pixel format of the packed-pixel buffer. The behavior of this function will vary depending on the value of `*pixelFormat` passed to the function: TJPF_UNKNOWN : The packed-pixel buffer returned by this function will use the most optimal pixel format for the file type, and `*pixelFormat` will contain the ID of that pixel format upon successful return from this function. TJPF_GRAY : Only PGM files can be loaded. TJPF_CMYK : The RGB or grayscale pixels stored in the file will be converted using a quick & dirty algorithm that is suitable only for testing purposes. (Proper conversion between CMYK and other formats requires a color management system.) Other pixel formats : The packed-pixel buffer will use the specified pixel format, and pixel format conversion will be performed if necessary.

Returns
  a pointer to a newly-allocated buffer containing the packed-pixel image, converted to the chosen pixel format and with the chosen row alignment, or NULL if an error occurred (see tj3GetErrorStr().) This buffer should be freed using tj3Free().

## ◆ tj3LoadImage16()

DLLEXPORT unsigned short * tj3LoadImage16 | ( | tjhandle | handle,
|  | const char * | filename,
|  | int * | width,
|  | int | align,
|  | int * | height,
|  | int * | pixelFormat
| ) |  |

Load a packed-pixel image with 13 to 16 bits of data precision per sample from disk into memory.

Parameters

  handle | handle to a TurboJPEG instance
  filename | name of a file containing a packed-pixel image in PBMPLUS (PPM/PGM) format. The target data precision (from 13 to 16 bits per sample) can be specified using TJPARAM_PRECISION and defaults to 16 if TJPARAM_PRECISION is unset or out of range. If the data precision of the PBMPLUS file does not match the target data precision, then upconverting or downconverting will be performed.
  width | pointer to an integer variable that will receive the width (in pixels) of the packed-pixel image
  align | row alignment (in samples) of the packed-pixel buffer to be returned (must be a power of 2.) Setting this parameter to n will cause all rows in the buffer to be padded to the nearest multiple of n samples (1 = unpadded.)
  height | pointer to an integer variable that will receive the height (in pixels) of the packed-pixel image
  pixelFormat | pointer to an integer variable that specifies or will receive the pixel format of the packed-pixel buffer. The behavior of this function will vary depending on the value of `*pixelFormat` passed to the function: TJPF_UNKNOWN : The packed-pixel buffer returned by this function will use the most optimal pixel format for the file type, and `*pixelFormat` will contain the ID of that pixel format upon successful return from this function. TJPF_GRAY : Only PGM files can be loaded. TJPF_CMYK : The RGB or grayscale pixels stored in the file will be converted using a quick & dirty algorithm that is suitable only for testing purposes. (Proper conversion between CMYK and other formats requires a color management system.) Other pixel formats : The packed-pixel buffer will use the specified pixel format, and pixel format conversion will be performed if necessary.

Returns
  a pointer to a newly-allocated buffer containing the packed-pixel image, converted to the chosen pixel format and with the chosen row alignment, or NULL if an error occurred (see tj3GetErrorStr().) This buffer should be freed using tj3Free().

## ◆ tj3LoadImage8()

DLLEXPORT unsigned char * tj3LoadImage8 | ( | tjhandle | handle,
|  | const char * | filename,
|  | int * | width,
|  | int | align,
|  | int * | height,
|  | int * | pixelFormat
| ) |  |

Load a packed-pixel image with 2 to 8 bits of data precision per sample from disk into memory.

Parameters

  handle | handle to a TurboJPEG instance
  filename | name of a file containing a packed-pixel image in Windows BMP or PBMPLUS (PPM/PGM) format. Windows BMP files require 8-bit-per-sample data precision. When loading a PBMPLUS file, the target data precision (from 2 to 8 bits per sample) can be specified using TJPARAM_PRECISION and defaults to 8 if TJPARAM_PRECISION is unset or out of range. If the data precision of the PBMPLUS file does not match the target data precision, then upconverting or downconverting will be performed.
  width | pointer to an integer variable that will receive the width (in pixels) of the packed-pixel image
  align | row alignment (in samples) of the packed-pixel buffer to be returned (must be a power of 2.) Setting this parameter to n will cause all rows in the buffer to be padded to the nearest multiple of n samples (1 = unpadded.)
  height | pointer to an integer variable that will receive the height (in pixels) of the packed-pixel image
  pixelFormat | pointer to an integer variable that specifies or will receive the pixel format of the packed-pixel buffer. The behavior of this function varies depending on the value of `*pixelFormat` passed to the function: TJPF_UNKNOWN : The packed-pixel buffer returned by this function will use the most optimal pixel format for the file type, and `*pixelFormat` will contain the ID of that pixel format upon successful return from this function. TJPF_GRAY : Only PGM files and 8-bit-per-pixel BMP files with a grayscale colormap can be loaded. TJPF_CMYK : The RGB or grayscale pixels stored in the file will be converted using a quick & dirty algorithm that is suitable only for testing purposes. (Proper conversion between CMYK and other formats requires a color management system.) Other pixel formats : The packed-pixel buffer will use the specified pixel format, and pixel format conversion will be performed if necessary.

Returns
  a pointer to a newly-allocated buffer containing the packed-pixel image, converted to the chosen pixel format and with the chosen row alignment, or NULL if an error occurred (see tj3GetErrorStr().) This buffer should be freed using tj3Free().

## ◆ tj3SaveImage12()

DLLEXPORT int tj3SaveImage12 | ( | tjhandle | handle,
|  | const char * | filename,
|  | const short * | buffer,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat
| ) |  |

Save a packed-pixel image with 9 to 12 bits of data precision per sample from memory to disk.

Parameters

  handle | handle to a TurboJPEG instance
  filename | name of a file to which to save the packed-pixel image, which will be stored in PBMPLUS (PPM/PGM) format. The source data precision (from 9 to 12 bits per sample) can be specified using TJPARAM_PRECISION and defaults to 12 if TJPARAM_PRECISION is unset or out of range.
  buffer | pointer to a buffer containing a packed-pixel RGB, grayscale, or CMYK image to be saved
  width | width (in pixels) of the packed-pixel image
  pitch | samples per row in the packed-pixel image. Setting this parameter to 0 is the equivalent of setting it to `width * tjPixelSize[pixelFormat]`.
  height | height (in pixels) of the packed-pixel image
  pixelFormat | pixel format of the packed-pixel image (see Pixel formats.) If this parameter is set to TJPF_GRAY, then the image will be stored in PGM format. Otherwise, the image will be stored in PPM format. If this parameter is set to TJPF_CMYK, then the CMYK pixels will be converted to RGB using a quick & dirty algorithm that is suitable only for testing purposes. (Proper conversion between CMYK and other formats requires a color management system.)

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr().)

## ◆ tj3SaveImage16()

DLLEXPORT int tj3SaveImage16 | ( | tjhandle | handle,
|  | const char * | filename,
|  | const unsigned short * | buffer,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat
| ) |  |

Save a packed-pixel image with 13 to 16 bits of data precision per sample from memory to disk.

Parameters

  handle | handle to a TurboJPEG instance
  filename | name of a file to which to save the packed-pixel image, which will be stored in PBMPLUS (PPM/PGM) format. The source data precision (from 13 to 16 bits per sample) can be specified using TJPARAM_PRECISION and defaults to 16 if TJPARAM_PRECISION is unset or out of range.
  buffer | pointer to a buffer containing a packed-pixel RGB, grayscale, or CMYK image to be saved
  width | width (in pixels) of the packed-pixel image
  pitch | samples per row in the packed-pixel image. Setting this parameter to 0 is the equivalent of setting it to `width * tjPixelSize[pixelFormat]`.
  height | height (in pixels) of the packed-pixel image
  pixelFormat | pixel format of the packed-pixel image (see Pixel formats.) If this parameter is set to TJPF_GRAY, then the image will be stored in PGM format. Otherwise, the image will be stored in PPM format. If this parameter is set to TJPF_CMYK, then the CMYK pixels will be converted to RGB using a quick & dirty algorithm that is suitable only for testing purposes. (Proper conversion between CMYK and other formats requires a color management system.)

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr().)

## ◆ tj3SaveImage8()

DLLEXPORT int tj3SaveImage8 | ( | tjhandle | handle,
|  | const char * | filename,
|  | const unsigned char * | buffer,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat
| ) |  |

Save a packed-pixel image with 2 to 8 bits of data precision per sample from memory to disk.

Parameters

  handle | handle to a TurboJPEG instance
  filename | name of a file to which to save the packed-pixel image. The image will be stored in Windows BMP or PBMPLUS (PPM/PGM) format, depending on the file extension. Windows BMP files require 8-bit-per-sample data precision. When saving a PBMPLUS file, the source data precision (from 2 to 8 bits per sample) can be specified using TJPARAM_PRECISION and defaults to 8 if TJPARAM_PRECISION is unset or out of range.
  buffer | pointer to a buffer containing a packed-pixel RGB, grayscale, or CMYK image to be saved
  width | width (in pixels) of the packed-pixel image
  pitch | samples per row in the packed-pixel image. Setting this parameter to 0 is the equivalent of setting it to `width * tjPixelSize[pixelFormat]`.
  height | height (in pixels) of the packed-pixel image
  pixelFormat | pixel format of the packed-pixel image (see Pixel formats.) If this parameter is set to TJPF_GRAY, then the image will be stored in PGM or 8-bit-per-pixel (indexed color) BMP format. Otherwise, the image will be stored in PPM or 24-bit-per-pixel BMP format. If this parameter is set to TJPF_CMYK, then the CMYK pixels will be converted to RGB using a quick & dirty algorithm that is suitable only for testing purposes. (Proper conversion between CMYK and other formats requires a color management system.)

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr().)

## ◆ tj3Set()

DLLEXPORT int tj3Set | ( | tjhandle | handle,
|  | int | param,
|  | int | value
| ) |  |

Set the value of a parameter.

Parameters

  handle | handle to a TurboJPEG instance
  param | one of the parameters
  value | value of the parameter (refer to parameter documentation)

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr().)

## ◆ tj3SetCroppingRegion()

DLLEXPORT int tj3SetCroppingRegion | ( | tjhandle | handle,
|  | tjregion | croppingRegion
| ) |  |

Set the cropping region for partially decompressing a lossy JPEG image into a packed-pixel image.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for decompression
  croppingRegion | tjregion structure that specifies a subregion of the JPEG image to decompress, or `TJUNCROPPED` for no cropping. The left boundary of the cropping region must be evenly divisible by the scaled iMCU width– `TJSCALED(tjMCUWidth[subsamp], scalingFactor)`, where `subsamp` is the level of chrominance subsampling in the JPEG image (see TJPARAM_SUBSAMP) and `scalingFactor` is the decompression scaling factor (see tj3SetScalingFactor().) The cropping region should be specified relative to the scaled image dimensions. Unless `croppingRegion` is `TJUNCROPPED`, the JPEG header must be read (see tj3DecompressHeader()) prior to calling this function.

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr().)

## ◆ tj3SetICCProfile()

DLLEXPORT int tj3SetICCProfile | ( | tjhandle | handle,
|  | unsigned char * | iccBuf,
|  | size_t | iccSize
| ) |  |

Embed an ICC (International Color Consortium) color management profile in JPEG images generated by subsequent compression and lossless transformation operations.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for compression
  iccBuf | pointer to a byte buffer containing an ICC profile. A copy is made of the ICC profile, so this buffer can be freed or reused as soon as this function returns. Setting this parameter to NULL or setting `iccSize` to 0 removes any ICC profile that was previously associated with the TurboJPEG instance.
  iccSize | size of the ICC profile (in bytes.) Setting this parameter to 0 or setting `iccBuf` to NULL removes any ICC profile that was previously associated with the TurboJPEG instance.

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr().)

## ◆ tj3SetScalingFactor()

DLLEXPORT int tj3SetScalingFactor | ( | tjhandle | handle,
|  | tjscalingfactor | scalingFactor
| ) |  |

Set the scaling factor for subsequent lossy decompression operations.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for decompression
  scalingFactor | tjscalingfactor structure that specifies a fractional scaling factor that the decompressor supports (see tj3GetScalingFactors()), or `TJUNSCALED` for no scaling. Decompression scaling is a function of the IDCT algorithm, so scaling factors are generally limited to multiples of 1/8. If the entire JPEG image will be decompressed, then the width and height of the scaled destination image can be determined by calling TJSCALED() with the JPEG width and height (see TJPARAM_JPEGWIDTH and TJPARAM_JPEGHEIGHT) and the specified scaling factor. When decompressing into a planar YUV image, an intermediate buffer copy will be performed if the width or height of the scaled destination image is not an even multiple of the iMCU size (see tjMCUWidth and tjMCUHeight.) Note that decompression scaling is not available (and the specified scaling factor is ignored) when decompressing lossless JPEG images (see TJPARAM_LOSSLESS), since the IDCT algorithm is not used with those images. Note also that TJPARAM_FASTDCT is ignored when decompression scaling is enabled.

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr().)

## ◆ tj3Transform()

DLLEXPORT int tj3Transform | ( | tjhandle | handle,
|  | const unsigned char * | jpegBuf,
|  | size_t | jpegSize,
|  | int | n,
|  | unsigned char ** | dstBufs,
|  | size_t * | dstSizes,
|  | const tjtransform * | transforms
| ) |  |

Losslessly transform a JPEG image into another JPEG image.

Lossless transforms work by moving the raw DCT coefficients from one JPEG image structure to another without altering the values of the coefficients. While this is typically faster than decompressing the image, transforming it, and re-compressing it, lossless transforms are not free. Each lossless transform requires reading and performing entropy decoding on all of the coefficients in the source image, regardless of the size of the destination image. Thus, this function provides a means of generating multiple transformed images from the same source or applying multiple transformations simultaneously, in order to eliminate the need to read the source coefficients multiple times.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for lossless transformation
  jpegBuf | pointer to a byte buffer containing the JPEG source image to transform
  jpegSize | size of the JPEG source image (in bytes)
  n | the number of transformed JPEG images to generate
  dstBufs | pointer to an array of n byte buffers. `dstBufs[i]` will receive a JPEG image that has been transformed using the parameters in `transforms[i]`. TurboJPEG has the ability to reallocate the JPEG destination buffer to accommodate the size of the transformed JPEG image. Thus, you can choose to: pre-allocate the JPEG destination buffer with an arbitrary size using tj3Alloc() and let TurboJPEG grow the buffer as needed, set `dstBufs[i]` to NULL to tell TurboJPEG to allocate the buffer for you, or pre-allocate the buffer to a "worst case" size determined by calling tj3TransformBufSize(). Under normal circumstances, this should ensure that the buffer never has to be re-allocated. (Setting TJPARAM_NOREALLOC guarantees that it won't be.) Note, however, that there are some rare cases (such as transforming images with a large amount of embedded Exif data) in which the transformed JPEG image will be larger than the worst-case size, and TJPARAM_NOREALLOC cannot be used in those cases unless the embedded data is discarded using TJXOPT_COPYNONE or TJPARAM_SAVEMARKERS. If you choose option 1 or 3, then `dstSizes[i]` should be set to the size of your pre-allocated buffer. In any case, unless you have set TJPARAM_NOREALLOC, you should always check `dstBufs[i]` upon return from this function, as it may have changed.
  dstSizes | pointer to an array of n size_t variables that will receive the actual sizes (in bytes) of each transformed JPEG image. If `dstBufs[i]` points to a pre-allocated buffer, then `dstSizes[i]` should be set to the size of the buffer. Upon return, `dstSizes[i]` will contain the size of the transformed JPEG image (in bytes.)
  transforms | pointer to an array of n tjtransform structures, each of which specifies the transform parameters and/or cropping region for the corresponding transformed JPEG image.

Returns
  0 if successful, or -1 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3TransformBufSize()

DLLEXPORT size_t tj3TransformBufSize | ( | tjhandle | handle,
|  | const tjtransform * | transform
| ) |  |

The maximum size of the buffer (in bytes) required to hold a JPEG image transformed with the given transform parameters and/or cropping region.

This function is a wrapper for tj3JPEGBufSize() that takes into account cropping, transposition of the width and height (which affects the destination image dimensions and level of chrominance subsampling), grayscale conversion, and the ICC profile (if any) that was previously associated with the TurboJPEG instance (see tj3SetICCProfile()) or extracted from the source image (see tj3GetICCProfile() and TJPARAM_SAVEMARKERS.) The JPEG header must be read (see tj3DecompressHeader()) prior to calling this function.

Parameters

  handle | handle to a TurboJPEG instance that has been initialized for lossless transformation
  transform | pointer to a tjtransform structure that specifies the transform parameters and/or cropping region for the JPEG image.

Returns
  the maximum size of the buffer (in bytes) required to hold the transformed image, or 0 if an error occurred (see tj3GetErrorStr() and tj3GetErrorCode().)

## ◆ tj3YUVBufSize()

DLLEXPORT size_t tj3YUVBufSize | ( | int | width,
|  | int | align,
|  | int | height,
|  | int | subsamp
| ) |  |

The size of the buffer (in bytes) required to hold a unified planar YUV image with the given parameters.

Parameters

  width | width (in pixels) of the image
  align | row alignment (in bytes) of the image (must be a power of 2.) Setting this parameter to n specifies that each row in each plane of the image will be padded to the nearest multiple of n bytes (1 = unpadded.)
  height | height (in pixels) of the image
  subsamp | level of chrominance subsampling in the image (see Chrominance subsampling options.)

Returns
  the size of the buffer (in bytes) required to hold the image, or 0 if the arguments are out of bounds.

## ◆ tj3YUVPlaneHeight()

DLLEXPORT int tj3YUVPlaneHeight | ( | int | componentID,
|  | int | height,
|  | int | subsamp
| ) |  |

The plane height of a YUV image plane with the given parameters.

Refer to YUV Image Format Notes for a description of plane height.

Parameters

  componentID | ID number of the image plane (0 = Y, 1 = U/Cb, 2 = V/Cr)
  height | height (in pixels) of the YUV image
  subsamp | level of chrominance subsampling in the image (see Chrominance subsampling options.)

Returns
  the plane height of a YUV image plane with the given parameters, or 0 if the arguments are out of bounds.

## ◆ tj3YUVPlaneSize()

DLLEXPORT size_t tj3YUVPlaneSize | ( | int | componentID,
|  | int | width,
|  | int | stride,
|  | int | height,
|  | int | subsamp
| ) |  |

The size of the buffer (in bytes) required to hold a YUV image plane with the given parameters.

Parameters

  componentID | ID number of the image plane (0 = Y, 1 = U/Cb, 2 = V/Cr)
  width | width (in pixels) of the YUV image. NOTE: This is the width of the whole image, not the plane width.
  stride | bytes per row in the image plane. Setting this to 0 is the equivalent of setting it to the plane width.
  height | height (in pixels) of the YUV image. NOTE: This is the height of the whole image, not the plane height.
  subsamp | level of chrominance subsampling in the image (see Chrominance subsampling options.)

Returns
  the size of the buffer (in bytes) required to hold the YUV image plane, or 0 if the arguments are out of bounds.

## ◆ tj3YUVPlaneWidth()

DLLEXPORT int tj3YUVPlaneWidth | ( | int | componentID,
|  | int | width,
|  | int | subsamp
| ) |  |

The plane width of a YUV image plane with the given parameters.

Refer to YUV Image Format Notes for a description of plane width.

Parameters

  componentID | ID number of the image plane (0 = Y, 1 = U/Cb, 2 = V/Cr)
  width | width (in pixels) of the YUV image
  subsamp | level of chrominance subsampling in the image (see Chrominance subsampling options.)

Returns
  the plane width of a YUV image plane with the given parameters, or 0 if the arguments are out of bounds.

## Variable Documentation

## ◆ tjAlphaOffset

const int tjAlphaOffset[TJ_NUMPF]
| static

Alpha offset (in samples) for a given pixel format.

This specifies the number of samples that the alpha component is offset from the start of the pixel. For instance, if an 8-bit-per-component pixel of format TJPF_BGRA is stored in `unsigned char pixel[]`, then the alpha component is `pixel[tjAlphaOffset[TJPF_BGRA]]`. The offset is -1 if the pixel format does not have an alpha component.

## ◆ tjBlueOffset

const int tjBlueOffset[TJ_NUMPF]
| static

Blue offset (in samples) for a given pixel format.

This specifies the number of samples that the blue component is offset from the start of the pixel. For instance, if an 8-bit-per-component pixel of format TJPF_BGRX is stored in `unsigned char pixel[]`, then the blue component is `pixel[tjBlueOffset[TJPF_BGRX]]`. The offset is -1 if the pixel format does not have a blue component.

## ◆ tjGreenOffset

const int tjGreenOffset[TJ_NUMPF]
| static

Green offset (in samples) for a given pixel format.

This specifies the number of samples that the green component is offset from the start of the pixel. For instance, if an 8-bit-per-component pixel of format TJPF_BGRX is stored in `unsigned char pixel[]`, then the green component is `pixel[tjGreenOffset[TJPF_BGRX]]`. The offset is -1 if the pixel format does not have a green component.

## ◆ tjMCUHeight

const int tjMCUHeight[TJ_NUMSAMP]
| static

iMCU height (in pixels) for a given level of chrominance subsampling

In a typical lossy JPEG image, 8x8 blocks of DCT coefficients for each component are interleaved in a single scan. If the image uses chrominance subsampling, then multiple luminance blocks are stored together, followed by a single block for each chrominance component. The minimum set of full-resolution luminance block(s) and corresponding (possibly subsampled) chrominance blocks necessary to represent at least one DCT block per component is called a "Minimum Coded Unit" or "MCU". (For example, an MCU in an interleaved lossy JPEG image that uses 4:2:2 subsampling consists of two luminance blocks followed by one block for each chrominance component.) In a non-interleaved lossy JPEG image, each component is stored in a separate scan, and an MCU is a single DCT block, so we use the term "iMCU" (interleaved MCU) to refer to the equivalent of an MCU in an interleaved JPEG image. For the common case of interleaved JPEG images, an iMCU is the same as an MCU.

iMCU sizes:

- 8x8 for no subsampling or grayscale
- 16x8 for 4:2:2
- 8x16 for 4:4:0
- 16x16 for 4:2:0
- 32x8 for 4:1:1
- 8x32 for 4:4:1

## ◆ tjMCUWidth

const int tjMCUWidth[TJ_NUMSAMP]
| static

iMCU width (in pixels) for a given level of chrominance subsampling

In a typical lossy JPEG image, 8x8 blocks of DCT coefficients for each component are interleaved in a single scan. If the image uses chrominance subsampling, then multiple luminance blocks are stored together, followed by a single block for each chrominance component. The minimum set of full-resolution luminance block(s) and corresponding (possibly subsampled) chrominance blocks necessary to represent at least one DCT block per component is called a "Minimum Coded Unit" or "MCU". (For example, an MCU in an interleaved lossy JPEG image that uses 4:2:2 subsampling consists of two luminance blocks followed by one block for each chrominance component.) In a non-interleaved lossy JPEG image, each component is stored in a separate scan, and an MCU is a single DCT block, so we use the term "iMCU" (interleaved MCU) to refer to the equivalent of an MCU in an interleaved JPEG image. For the common case of interleaved JPEG images, an iMCU is the same as an MCU.

iMCU sizes:

- 8x8 for no subsampling or grayscale
- 16x8 for 4:2:2
- 8x16 for 4:4:0
- 16x16 for 4:2:0
- 32x8 for 4:1:1
- 8x32 for 4:4:1

## ◆ tjPixelSize

const int tjPixelSize[TJ_NUMPF]
| static

Pixel size (in samples) for a given pixel format.

## ◆ tjRedOffset

const int tjRedOffset[TJ_NUMPF]
| static

Red offset (in samples) for a given pixel format.

This specifies the number of samples that the red component is offset from the start of the pixel. For instance, if an 8-bit-per-component pixel of format TJPF_BGRX is stored in `unsigned char pixel[]`, then the red component is `pixel[tjRedOffset[TJPF_BGRX]]`. The offset is -1 if the pixel format does not have a red component.

## ◆ TJUNCROPPED

const tjregion TJUNCROPPED
| static

A tjregion structure that specifies no cropping.

## ◆ TJUNSCALED

const tjscalingfactor TJUNSCALED
| static

A tjscalingfactor structure that specifies a scaling factor of 1/1 (no scaling)