libmtp version: 0.1.5

Attempting to connect device(s)
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0e79
   idProduct: 1307
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000002
Device info:
   Manufacturer: ARCHOS
   Model: a504
   Device version: 1.6.20  
   Serial number: C5B8X71AC13UGG
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 10.0;
Supported operations:
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   1001: get device info
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   100f: Format storage
   1010: Reset device
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100c: Send object info
   100d: Send object
   100b: Delete object
   1019: Move object
   101a: Copy object
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9807: Get interdependent property description
   9808: Send object property list
   9810: Get object references
   9811: Set object references
   101b: Get partial object
   9201: Report Added/Deleted Items
Events supported:
   0x4001
   0x4004
   0x4005
   0x400a
Device Properties Supported:
   0xd101: Secure Time
   0xd102: Device Certificate
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Device Friendly Name
Playable File (Object) Types and Object Properties Supported:
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 1 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1000, MAX 327680, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 85,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 1 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 353,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   3008: MS Wave
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 1 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 64000, MAX 3072000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 1, 17,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   b903: AAC
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 1 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 255,  READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   300a: MS AVI
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 720, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 576, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 1 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 3072000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 1, 17, 85, 353,  READ ONLY
      de9c: VideoBitRate UINT32 data type range: MIN 10240, MAX 5120000, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 1482049860, 808802372, 1395937357, 1145656920,  GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 10240, MAX 8192000, STEP 1 READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 1, MAX 30000, STEP 1 GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 1, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   b981: WMV
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 720, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 576, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 1 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 3072000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 1, 17, 85, 353,  READ ONLY
      de9c: VideoBitRate UINT32 data type range: MIN 10240, MAX 10240000, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911,  GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 10240, MAX 13312000, STEP 1 READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 1, MAX 30000, STEP 1 GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 1, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   300c: ASF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 720, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 576, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 1 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 3072000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 1, 17, 85, 353,  READ ONLY
      de9c: VideoBitRate UINT32 data type range: MIN 10240, MAX 10240000, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911, 1482049860, 808802372, 1395937357, 1145656920,  GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 10240, MAX 13312000, STEP 1 READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 1, MAX 30000, STEP 1 GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 1, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   300b: MPEG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 720, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 576, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 1 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 3072000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 80,  READ ONLY
      de9c: VideoBitRate UINT32 data type range: MIN 10240, MAX 10240000, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 826757197, 843534413,  GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 10240, MAX 13312000, STEP 1 READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 1, MAX 30000, STEP 1 GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 1, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   b982: MP4
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 720, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 576, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 1 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 3072000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 255,  READ ONLY
      de9c: VideoBitRate UINT32 data type range: MIN 10240, MAX 5120000, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 875967048, 1129726276, 826496577, 875967064,  GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 10240, MAX 8192000, STEP 1 READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 1, MAX 30000, STEP 1 GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 1, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   3801: JPEG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   3808: JFIF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   3804: BMP
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   380b: PNG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   ba03: Abstract Audio Album
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,  GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 1, MAX 1024, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 1, MAX 1024, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 1, MAX -1, STEP 1 GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: DateCreated STRING data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 79818866688
      FreeSpaceInBytes: 67965894656
      FreeSpaceInObjects: 4294967295
      StorageDescription: Internal HardDisk
      VolumeIdentifier: HKA540AMC8R3LL
Special directories:
   Default music folder: 0x00000004
   Default playlist folder: 0x0000006a
   Default picture folder: 0x00000014
   Default video folder: 0x0000007c
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000118
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: (NULL)
   Synchronization partner: (NULL)
   Battery level 0 of 3 (0%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   RIFF WAVE file
   Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
   Audio Video Interleave
   Microsoft Windows Media Video
   Microsoft Advanced Systems Format
   MPEG video stream
   MPEG-4 Part 14 Container Format (Audio+Video Empahsis)
   JPEG file
   JFIF file
   BMP bitmap file
   Portable Network Graphics

Secure Time:
<DRMCLOCK type="status"><VALUE>#20060522 12:13:29Z#</VALUE><FLAG>DRM_CLK_NOT_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">C5B8X71AC13UGG</UNIQUEID><PUBLICKEY private="1">efVfIxK3Munlf5HdwwNFJc3e1Wa2t0dyzhgNjXJ2KK8Jv1E0e/L4QQ==</PUBLICKEY><KEYDATA>VXUlmdHQSU+hy+q8cUn04bcfezw=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>3VHCHxifwOjtdNIMFeNItuMZqHGgjnhQxy9PXKw7s5xybRzIjPkTGQ==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>jyVXx/t+NOmMmdIRqYDTpRXF4/E=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.104.115</SECURITYVERSION><CERTIFICATE private="1">efVfIxK3Munlf5HdwwNFJc3e1Wa2t0dyzhgNjXJ2KK8Jv1E0e/L4QQIEaHPMNpKrP09P1Me4nkx7VPHPjxreU0o3RQK1hdL9mYjQi195ibK8BOJg</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>A504</NAME>
    <MANUFACTURER>Archos</MANUFACTURER>
    <MAKE>A504</MAKE>
    <DISTRIBUTOR>Archos</DISTRIBUTOR>
    <MODEL>A504</MODEL>
    <SECURITYLEVEL>2000</SECURITYLEVEL>
    <HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
    <HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR>
    <FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR>
    <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
    <FEATURES>
        <CLOCK>2</CLOCK>
        <SECURECLOCK>
            <URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
            <PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY>
        </SECURECLOCK>
        <METERING>1</METERING>
        <LICENSE_ACQ>1</LICENSE_ACQ>
        <LICENSE_SYNC>1</LICENSE_SYNC>
        <ENCRYPTION>1</ENCRYPTION>
        <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
    </FEATURES>
    <LIMITS>
        <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
        <MAXLICENSESIZE>10240</MAXLICENSESIZE>
        <MAXHEADERSIZE>5120</MAXHEADERSIZE>
    </LIMITS><PUBLICKEY>7KiDPsl9CZB/GYmnMNp4uy50pTCLEvjNZSrm2QajhPAQPli1ccLhNQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>/edeqZJclq5G6KuHDjMjcPU9NHeT9bbFYGCkBn1GQVhc9pKBWqZKaQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>983</AUTH_ID><PUBLICKEY>2KqzhyuwjFtjObyu99qx/Z9IYEbxvz+r4Cnui049xqxMHCdPDwYDJg==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>fKmq5LLr+r7rGhA3M4hE8BV8+GLeV7K09RUbofEYTdJ9iI1D2Q7kIw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>l5TRtNPfdxdretk8bTlY1XGiaFmaevtJuwErqrwpXL82hScj6cjlDg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>

Device description WMPInfo.xml file:
<DeviceInfo>
    <WMP DeviceID="{4287E9BD-3B39-4BFD-A5AD-FFDCB8B796C8}" RelationshipID="{6870ED09-423F-4172-94B4-FE3AF8069649}"/>
</DeviceInfo>

OK.
