Unable to open ~/.mtpz-data for reading, MTPZ disabled.libmtp version: 1.1.5

Listing raw device(s)
   Found 1 device(s):
   Motorola: Atrix MB860 (MTP mode) (22b8:7088) @ bus 4, dev 71
Attempting to connect device(s)
USB low-level info:
   Interface has a kernel driver attached.
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 22b8
   idProduct: 7088
   IN endpoint maxpacket: 64 bytes
   OUT endpoint maxpacket: 64 bytes
   Raw device info:
      Bus location: 4
      Device number: 71
      Device entry info:
         Vendor: Motorola
         Vendor id: 0x22b8
         Product: Atrix MB860 (MTP mode)
         Vendor id: 0x7088
         Device flags: 0x08008106
Configuration 0, interface 0, altsetting 0:
   Interface description contains the string "MTP"
   Device recognized as MTP, no further probing.
Device info:
   Manufacturer: Motorola
   Model: MB860
   Device version: V1.1
   Serial number: 12345678901234561234567890123456
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com/WMPPD: 10.0; microsoft.com/DeviceServices:1.0;
   Detected object size: 64 bits
   Extensions:
        microsoft.com/WMPPD: 10.0
        microsoft.com/DeviceServices: 1.0
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1010: Reset device
   1012: Set object protection
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   101b: Get partial object
   9810: Get object references
   9811: Set object references
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9807: Get interdependent property description
   9301: Unknown (9301)
   9302: Unknown (9302)
   9303: Unknown (9303)
   9304: Unknown (9304)
   9305: Unknown (9305)
   9306: Unknown (9306)
   9307: Unknown (9307)
   9308: Unknown (9308)
   9309: Unknown (9309)
   100a: Get thumbnail
Events supported:
   0x4001
   0x4004
   0x4005
   0x400a
   0x400b
   0xc303
Device Properties Supported:
   0x5011: Date & Time
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd405: Device Icon
   0x5001: Battery Level
Playable File (Object) Types and Object Properties Supported:
   300c: ASF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 864000000, STEP 1 READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 352, 353, 384, 41222, 85,  READ ONLY
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 320000, STEP 1 READ ONLY
      de97: Scan Depth UINT16 data type enumeration: 0,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 720, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 859189832, 959853128, 1195724877, 827739479, 844516695, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 1000, MAX 2048000, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 1000, MAX 30000, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type GET/SET
   b981: WMV
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 864000000, STEP 1 READ ONLY
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 352, 353, 384, 41222, 85,  READ ONLY
      de97: Scan Depth UINT16 data type enumeration: 0,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 720, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type range: MIN 1, MAX 48000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 384000, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 859189832, 959853128, 1195724877, 827739479, 844516695, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 1000, MAX 2048000, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 1000, MAX 30000, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type GET/SET
   3009: MP3
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 864000000, STEP 1 READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 352, 353, 384, 41222, 85,  READ ONLY
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 320000, STEP 1 READ ONLY
   3008: MS Wave
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 864000000, STEP 1 READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 352, 353, 384, 41222, 85,  READ ONLY
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 320000, STEP 1 READ ONLY
   b901: WMA
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 864000000, STEP 1 READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 352, 353, 384, 41222, 85,  READ ONLY
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 320000, STEP 1 READ ONLY
   ba03: Abstract Audio Album
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1200, STEP 1 GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1600, STEP 1 GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
   ba05: Abstract Audio Video Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
   3001: Association/Directory
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc06: Association Desc UINT32 data type ANY 32BIT VALUE form GET/SET
   3801: JPEG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 1, MAX 4920, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 1, MAX 4920, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1200, STEP 1 GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1600, STEP 1 GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 4194304, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  READ ONLY
   3807: GIF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 4920, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 4920, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1200, STEP 1 GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1600, STEP 1 GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 4194304, STEP 1 READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  READ ONLY
   3804: BMP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 1, MAX 4920, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 1, MAX 4920, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1200, STEP 1 GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1600, STEP 1 GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 4194304, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 4194304, STEP 1 READ ONLY
   380b: PNG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 1, MAX 4920, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 1, MAX 4920, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1200, STEP 1 GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1600, STEP 1 GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 4194304, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  READ ONLY
   3800: Defined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
   b984: 3GP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 864000000, STEP 1 READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 352, 353, 384, 41222, 85,  READ ONLY
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 320000, STEP 1 READ ONLY
      de97: Scan Depth UINT16 data type enumeration: 0,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 720, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 859189832, 959853128, 1195724877, 827739479, 844516695, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 1000, MAX 2048000, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 1000, MAX 30000, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type GET/SET
   b982: MP4
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 864000000, STEP 1 READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 352, 353, 384, 41222, 85,  READ ONLY
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 320000, STEP 1 READ ONLY
      de97: Scan Depth UINT16 data type enumeration: 0,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 720, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 859189832, 959853128, 1195724877, 827739479, 844516695, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 1000, MAX 2048000, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 1000, MAX 30000, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type GET/SET
   b903: AAC
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 864000000, STEP 1 READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 352, 353, 384, 41222, 85,  READ ONLY
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 320000, STEP 1 READ ONLY
   3000: Undefined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
Storage Devices:
   StorageID: 0x00020001
      StorageType: 0x0004 removable RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 13541736448
      FreeSpaceInBytes: 4892884992
      FreeSpaceInObjects: 4294967295
      StorageDescription: Removable Storage
      VolumeIdentifier: 954733058
Special directories:
   Default music folder: 0xffffffff
   Default playlist folder: 0x0000057b
   Default picture folder: 0x0000059f
   Default video folder: 0xffffffff
   Default organizer folder: 0xffffffff
   Default zencast folder: 0xffffffff
   Default album folder: 0x0000057d
   Default text folder: 0xffffffff
MTP-specific device properties:
   Friendly name: MB860
   Synchronization partner: Moto Media Sync Engine
   Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
   Microsoft Advanced Systems Format
   Microsoft Windows Media Video
   ISO MPEG-1 Audio Layer 3
   RIFF WAVE file
   Microsoft Windows Media Audio
   Abstract Album file
   Abstract Playlist file
   Folder
   JPEG file
   GIF bitmap file
   BMP bitmap file
   Portable Network Graphics
   MPEG-4 Part 14 Container Format (Audio+Video Emphasis)
   Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3

WMPInfo.xml file contents:
<DeviceInfo>
    <WMP DeviceID="{69AE1F11-EB18-49A3-B232-F50177CEC050}" RelationshipID="{00000000-0000-0000-0000-000000000000}"/>
</DeviceInfo>

OK.
