libmtp version: 0.2.1

Attempting to connect device(s)
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0471
   idProduct: 084e
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000002
Microsoft device descriptor 0xee:
       0000: 1203 4d00 5300 4600 5400 3100 3000 3000   ..M.S.F.T.1.0.0.
       0010: 0100                                      ..
Device info:
   Manufacturer: Philips
   Model: Philips GoGear SA60XX
   Device version: PH03010D02
   Serial number: 0000000EA6570F9F0706141006181631
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com/WMDRMPD: 10.1;audible.com: 1.0;
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1010: Reset device
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   9810: Get object references
   9811: Set object references
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   101b: Get partial object
   9201: Report Added/Deleted Items
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
Events supported:
   0x4004
   0x4005
Device Properties Supported:
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Device Friendly Name
   0xd101: Secure Time
   0xd102: Device Certificate
   0xd103: RevocationInfo
Playable File (Object) Types and Object Properties Supported:
   3009: MP3
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
   b901: WMA
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
   3008: MS Wave
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
   3801: JPEG
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc87: Width UINT32 data type range: MIN 1, MAX 320, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 1, MAX 240, STEP 1 GET/SET
   300a: MS AVI
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc87: Width UINT32 data type range: MIN 1, MAX 320, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 1, MAX 240, STEP 1 GET/SET
      de97: ScanDepth UINT16 data type enumeration: 1,  READ ONLY
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 1195724877, 861293911,  GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 1000, MAX 10000, STEP 1 GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 32768, MAX 2048000, STEP 1 GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      dea1: EncodingProfile STRING data type GET/SET
   b981: WMV
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc87: Width UINT32 data type range: MIN 1, MAX 320, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 1, MAX 240, STEP 1 GET/SET
      de97: ScanDepth UINT16 data type enumeration: 1,  READ ONLY
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 1195724877, 861293911,  GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 1000, MAX 10000, STEP 1 GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 32768, MAX 2048000, STEP 1 GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      dea1: EncodingProfile STRING data type GET/SET
   300c: ASF
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc87: Width UINT32 data type range: MIN 1, MAX 320, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 1, MAX 240, STEP 1 GET/SET
      de97: ScanDepth UINT16 data type enumeration: 1,  READ ONLY
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 1195724877, 861293911,  GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 1000, MAX 10000, STEP 1 GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 32768, MAX 2048000, STEP 1 GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      dea1: EncodingProfile STRING data type GET/SET
   3001: Association/Directory
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
   ba05: Abstract Audio Video Playlist
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
   3000: Undefined Type
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
   b802: Firmware
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
   ba03: Abstract Audio Album
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,  READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc9b: AlbumArtist STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 4003463168
      FreeSpaceInBytes: 2491481457
      FreeSpaceInObjects: 5419
      StorageDescription: Internal Storage
      VolumeIdentifier: 0000000EA6570F9F0706141006181631
Special directories:
   Default music folder: 0x20000004
   Default playlist folder: 0x20000019
   Default picture folder: 0x20000018
   Default video folder: 0x20000016
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: Philips GoGear SA60XX
   Synchronization partner: Longhorn Sync Engine
   Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   RIFF WAVE file
   JPEG file
   Audio Video Interleave
   Microsoft Windows Media Video
   Microsoft Advanced Systems Format
   Firmware file

Secure Time:
<DRMCLOCK type="status"><VALUE>#20070511
07:42:09Z#</VALUE><FLAG>DRM_CLK_NEEDS_REFRESH</FLAG></DRMCLOCK>AG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID
private="1">AAAADqZXD58HBhQQBhgWMQAAAAA=</UNIQUEID><PUBLICKEY
private="1">lb+TWhA19FA+sD+8fEw8PAaJamIZIWURWRZ4x8z5tZ1cKDzwwQiVNg==</PUBLICKEY><KEYDATA>Jy23mPedTghHJBvHK0oxHi92L0U=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>3ZpQV/dynAhxFjt2SFd1WBnuNTptTfR0nCBLFRQE1AJ08DjerYP9dA==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>QAMvSPcyOA1DapTTXBVLY9xurLs=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.107.107</SECURITYVERSION><CERTIFICATE
private="1">lb+TWhA19FA+sD+8fEw8PAaJamIZIWURWRZ4x8z5tZ1cKDzwwQiVNgIEa2vAdAIRpqxdInYSUyr7KfBg4sZaQiLnlLMg+Ur7sQkFCesrqKdQQ81e</CERTIFICATE></FALLBACK><CERTIFICATE
type="GROUP"><DATA><NAME>SA60xx</NAME>
    <MANUFACTURER>Perception Digital Ltd</MANUFACTURER>
    <MAKE>Philips Audio & Multi Media Applications</MAKE>
    <DISTRIBUTOR>Koninklijke Philips Electronics N.V.</DISTRIBUTOR>
    <MODEL>00</MODEL>
    <SECURITYLEVEL>2000</SECURITYLEVEL>
    <HARDWARE_VER_MAJOR>02</HARDWARE_VER_MAJOR>
    <HARDWARE_VER_MINOR>00</HARDWARE_VER_MINOR>
    <FIRMWARE_VER_MAJOR>08</FIRMWARE_VER_MAJOR>
    <FIRMWARE_VER_MINOR>00</FIRMWARE_VER_MINOR>
    <FEATURES>
        <CLOCK>2</CLOCK>
        <SECURECLOCK>
            <URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>

<PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY>
        </SECURECLOCK>
        <METERING>1</METERING>
        <LICENSE_ACQ>0</LICENSE_ACQ>
        <LICENSE_SYNC>1</LICENSE_SYNC>
        <ENCRYPTION>1</ENCRYPTION>
        <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
    </FEATURES>
    <LIMITS>
        <MAXCHAINDEPTH>5</MAXCHAINDEPTH>
        <MAXLICENSESIZE>10240</MAXLICENSESIZE>
        <MAXHEADERSIZE>5120</MAXHEADERSIZE>

</LIMITS><PUBLICKEY>O/xY2BVO97/4QEvlk+ETiHxn13rWyg5HsWO/Uy3DHCQg7rowMRF0gw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>vgUBFIcCPVuNuYhGWODMqCH8XiNw83pAwS9S8KWZckb7T99BX4i+OQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>1743</AUTH_ID><PUBLICKEY>Q5qnbSHxftMJXBVdgoi0Ds8CrUgXgToCUcmJIz4LSDcycDSj2n5FfQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>cdq3bQ3V+qGBJXT52FXvDw4jVzret3LRWnpa6q7bMHiSeyZWfRuQMg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>s9lZMSUkYRzjmE8Ju5CtPS6lclfC1BG7Np/QWoLoOXDlt4gYBywCdw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>

Device description WMPInfo.xml file:
<DeviceInfo>
    <WMP DeviceID="{67F39E4A-BE30-4778-8A0B-0B4196AB747A}"
RelationshipID="{4252D0B8-109A-4B34-BE69-CF79F3357D11}"/>
</DeviceInfo>

OK.
