


---

** [bugs:#1410] unknown device - Archos 48 Internet Tablet 500GB**

**Status:** open
**Group:** 1.1.9
**Created:** Fri Sep 11, 2015 05:29 PM UTC by Anonymous
**Last Updated:** Fri Sep 11, 2015 05:29 PM UTC
**Owner:** nobody


I have an Archos 48 Internet Tablet, a device with a 500 GB hard drive I use as music player. This is the output of mtp-detect

libmtp version: 1.1.9

Listing raw device(s)
Device 0 (VID=0e79 and PID=1421) is UNKNOWN.
Please report this VID/PID and the device model to the libmtp development team
   Found 1 device(s):
   0e79:1421 @ bus 4, dev 14
Attempting to connect device(s)
USB low-level info:
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 255
   bDeviceProtocol: 255
   idVendor: 0e79
   idProduct: 1421
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 4
      Device number: 14
      Device entry info:
         Vendor: (null)
         Vendor id: 0x0e79
         Product: (null)
         Vendor id: 0x1421
         Device flags: 0x00000000
Microsoft device descriptor 0xee:
	0000: 1203 4d00 5300 4600 5400 3100 3000 3000	..M.S.F.T.1.0.0.
	0010: fe00                                   	..
Microsoft device response to control message 1, CMD 0xfe:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Microsoft device response to control message 2, CMD 0xfe:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Device responds to control message 2 with some data.
Device info:
   Manufacturer: ARCHOS
   Model: Archos 48
   Device version: 2.0.45  
   Serial number: JG661EBPEA3BLL
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 10.0;
   Detected object size: 64 bits
   Extensions:
        microsoft.com: 1.0
        microsoft.com/WMDRMPD: 10.1
        microsoft.com/WMPPD: 10.0
Supported operations:
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   1001: get device info
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1010: Reset device
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100c: Send object info
   100d: Send object
   100b: Delete object
   1019: Move object
   101a: Copy object
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9807: Get interdependent property description
   9808: Send object property list
   9810: Get object references
   9811: Set object references
   101b: Get partial object
   9201: Report Added/Deleted Items
Events supported:
   0x4001
   0x4004
   0x4005
   0x400a
Device Properties Supported:
   0xd101: Secure Time
   0xd102: Device Certificate
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
Playable File (Object) Types and Object Properties Supported:
   3000: Undefined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
   3009: MP3
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1000, MAX 327680, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 85,  READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   b901: WMA
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 320000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 353,  READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   3008: MS Wave
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 96000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 64000, MAX 3072000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 1, 17,  READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   b903: AAC
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 96000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 255,  READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   300a: MS AVI
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 1280, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 720, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 96000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 8000, MAX 3072000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 1, 17, 85, 353,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 10240, MAX 8192000, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 1482049860, 808802372, 1395937357, 1145656920,  GET/SET
      dea1: Encoding Profile STRING data type GET/SET
      de91: Total Bit Rate UINT32 data type range: MIN 10240, MAX 11264000, STEP 1 READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de97: Scan Depth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 1, MAX 30000, STEP 1 GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 1, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   b981: WMV
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 1280, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 720, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 96000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 8000, MAX 3072000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 1, 17, 85, 353,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 10240, MAX 10240000, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 861293911,  GET/SET
      dea1: Encoding Profile STRING data type GET/SET
      de91: Total Bit Rate UINT32 data type range: MIN 10240, MAX 13312000, STEP 1 READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      de97: Scan Depth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 1, MAX 30000, STEP 1 GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 1, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   300c: ASF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 1280, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 720, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 96000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 8000, MAX 3072000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 1, 17, 85, 353,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 10240, MAX 10240000, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 861293911, 1482049860, 808802372, 1395937357, 1145656920,  GET/SET
      dea1: Encoding Profile STRING data type GET/SET
      de91: Total Bit Rate UINT32 data type range: MIN 10240, MAX 13312000, STEP 1 READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de97: Scan Depth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 1, MAX 30000, STEP 1 GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 1, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   300b: MPEG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 720, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 576, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 96000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 8000, MAX 3072000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 80,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 10240, MAX 10240000, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 826757197, 843534413,  GET/SET
      dea1: Encoding Profile STRING data type GET/SET
      de91: Total Bit Rate UINT32 data type range: MIN 10240, MAX 13312000, STEP 1 READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de97: Scan Depth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 1, MAX 30000, STEP 1 GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 1, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   b982: MP4
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 1280, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 720, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 96000, STEP 1 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 8000, MAX 3072000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 255,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 10240, MAX 5120000, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 875967048, 1129726276, 826496577, 875967064,  GET/SET
      dea1: Encoding Profile STRING data type GET/SET
      de91: Total Bit Rate UINT32 data type range: MIN 10240, MAX 8192000, STEP 1 READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de97: Scan Depth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 1, MAX 30000, STEP 1 GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 1, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   3801: JPEG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   3808: JFIF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   3804: BMP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   380b: PNG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc87: Width UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   ba03: Abstract Audio Album
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 1, MAX 1024, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 1, MAX 1024, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 1, MAX -1, STEP 1 GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   3001: Association/Directory
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 495526760448
      FreeSpaceInBytes: 414964207616
      FreeSpaceInObjects: 4294967295
      StorageDescription: Internal Hard Drive
      VolumeIdentifier: (null)
Special directories:
   Default music folder: 0x000000c6
   Default playlist folder: 0xffffffff
   Default picture folder: 0x00000f56
   Default video folder: 0x00000f4b
   Default organizer folder: 0xffffffff
   Default zencast folder: 0xffffffff
   Default album folder: 0xffffffff
   Default text folder: 0xffffffff
MTP-specific device properties:
   Friendly name: Archie
   Synchronization partner: (NULL)
   Battery level 1 of 3 (33%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   RIFF WAVE file
   Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
   Audio Video Interleave
   Microsoft Windows Media Video
   Microsoft Advanced Systems Format
   MPEG video stream
   MPEG-4 Part 14 Container Format (Audio+Video Emphasis)
   JPEG file
   JFIF file
   BMP bitmap file
   Portable Network Graphics
   Abstract Album file
   Abstract Playlist file
   Folder

Secure Time:
<DRMCLOCK type="status"><VALUE>#19700131 22:30:51Z#</VALUE><FLAG>DRM_CLK_NOT_SET</FLAG></DRMCLOCK>
OK.


---

Sent from sourceforge.net because you indicated interest in <https://sourceforge.net/p/libmtp/bugs/1410/>



To unsubscribe from further messages, please visit <https://sourceforge.net/auth/subscriptions/>