libmtp version: 0.3.0

Listing raw device(s)
Device 0 (VID=1004 and PID=6132) is UNKNOWN.
Please report this VID/PID and the device model to the libmtp development
team
Found 1 device(s):
1004:6132 @ bus 0, dev 14
Attempting to connect device(s)
PTP: Opening session
USB low-level info:
Using kernel interface "usbfs"
bcdUSB: 512
bDeviceClass: 0
bDeviceSubClass: 0
bDeviceProtocol: 0
idVendor: 1004
idProduct: 6132
IN endpoint maxpacket: 512 bytes
OUT endpoint maxpacket: 512 bytes
Raw device info:
Bus location: 0
Device number: 14
Device entry info:
Vendor: (null)
Vendor id: 0x1004
Product: (null)
Vendor id: 0x6132
Device flags: 0x00000000
Microsoft device descriptor 0xee:
0000: 1203 4d00 5300 4600 5400 3100 3000 3000 ..M.S.F.T.1.0.0.
0010: fa00 ..
Microsoft device response to control message 1, CMD 0xfa:
0000: 2800 0000 0001 0400 0100 0000 0000 0000 (...............
0010: 0001 4d54 5000 0000 0000 3034 0000 0000 ..MTP.....04....
0020: 0000 0000 0000 0000 ........
Microsoft device response to control message 2, CMD 0xfa:
0000: 2800 0000 0001 0400 0100 0000 0000 0000 (...............
0010: 0001 4d54 5000 0000 0000 3034 0000 0000 ..MTP.....04....
0020: 0000 0000 0000 0000 ........
Device info:
Manufacturer: LG Electronics
Model: ����0Mu
Device version: Sync Pla
Serial number: : <[EDIT]deleted garbled info[/EDIT]>
Vendor extension ID: 0x00000006
Vendor extension description: microsoft.com/WMPPD: 10.0;
LGElectronics.com/Dispatcher: 0.0a; microsoft.com/WMPPD: 11.0;
vodafone.com/omadrmv2: 1.0;
Detected object size: 64 bits
Supported operations:
1010: Reset device
1013: Power down device
1017: Reset device property value
1001: get device info
1002: Open session
1003: Close session
1004: Get storage IDs
1005: Get storage info
1006: Get number of objects
1007: Get object handles
1008: Get object info
1009: Get object
100b: Delete object
100c: Send object info
100d: Send object
100f: Format storage
1014: Get device property description
1015: Get device property value
1016: Set device property value
101b: Get partial object
9801: Get object properties supported
9802: Get object property description
9803: Get object property value
9810: Get object references
9811: Set object references
9805: Get object property list
9804: Set object property value
9806: Set object property list
9202: Report Acquired Items
9203: Get transferable playlist types
9201: Report Added/Deleted Items
Events supported:
0x4004
0x4005
Device Properties Supported:
0x5001: Battery Level
0x501f: Copyright Info
0xd401: Synchronization Partner
0xd402: Friendly Device Name
0xd404: Unknown property
Playable File (Object) Types and Object Properties Supported:
b984: 3GP
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, READ ONLY
dc07: ObjectFileName STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc44: Name STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
de99: AudioWAVECodec UINT32 data type enumeration: 85, 352, 353, 354,
GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 2, 1, GET/SET
de93: SampleRate UINT32 data type range: MIN 32768, MAX 45158, STEP 1
GET/SET
de9a: AudioBitRate UINT32 data type range: MIN 8192, MAX 196608, STEP
1 READ ONLY
dc9b: AlbumArtist STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc96: Composer STRING data type GET/SET
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1
GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
db01: unknown(db01) UINT8 data type enumeration: 0, 1, GET/SET
db02: unknown(db02) array of UINT8 data type byte array: GET/SET
dc9d: DRMStatus UINT16 data type enumeration: 2, 0, 1, 2, GET/SET
b901: WMA
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, READ ONLY
dc07: ObjectFileName STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc44: Name STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
de99: AudioWAVECodec UINT32 data type enumeration: 85, 352, 353, 354,
GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 2, 1, GET/SET
de93: SampleRate UINT32 data type range: MIN 32768, MAX 45158, STEP 1
GET/SET
de9a: AudioBitRate UINT32 data type range: MIN 8192, MAX 196608, STEP
1 READ ONLY
dc9b: AlbumArtist STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc96: Composer STRING data type GET/SET
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1
GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
db01: unknown(db01) UINT8 data type enumeration: 0, 1, GET/SET
db02: unknown(db02) array of UINT8 data type byte array: GET/SET
dc9d: DRMStatus UINT16 data type enumeration: 2, 0, 1, 2, GET/SET
3009: MP3
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, READ ONLY
dc07: ObjectFileName STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc44: Name STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
de99: AudioWAVECodec UINT32 data type enumeration: 85, 352, 353, 354,
GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 2, 1, GET/SET
de93: SampleRate UINT32 data type range: MIN 32768, MAX 45158, STEP 1
GET/SET
de9a: AudioBitRate UINT32 data type range: MIN 8192, MAX 196608, STEP
1 READ ONLY
dc9b: AlbumArtist STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc96: Composer STRING data type GET/SET
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1
GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
3008: MS Wave
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, READ ONLY
dc07: ObjectFileName STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc44: Name STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
de99: AudioWAVECodec UINT32 data type enumeration: 85, 352, 353, 354,
GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 2, 1, GET/SET
de93: SampleRate UINT32 data type range: MIN 32768, MAX 45158, STEP 1
GET/SET
de9a: AudioBitRate UINT32 data type range: MIN 8192, MAX 196608, STEP
1 READ ONLY
dc9b: AlbumArtist STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc96: Composer STRING data type GET/SET
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1
GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
ba05: Abstract Audio Video Playlist
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, READ ONLY
dc07: ObjectFileName STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc44: Name STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
ba10: WPL Playlist
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, READ ONLY
dc07: ObjectFileName STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc44: Name STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
3000: Undefined Type
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, READ ONLY
dc07: ObjectFileName STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc44: Name STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
b902: OGG
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, READ ONLY
dc07: ObjectFileName STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc44: Name STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
de99: AudioWAVECodec UINT32 data type enumeration: 85, 352, 353, 354,
GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 2, 1, GET/SET
de93: SampleRate UINT32 data type range: MIN 32768, MAX 45158, STEP 1
GET/SET
de9a: AudioBitRate UINT32 data type range: MIN 8192, MAX 196608, STEP
1 READ ONLY
dc9b: AlbumArtist STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc96: Composer STRING data type GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1
GET/SET
300c: ASF
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, READ ONLY
dc07: ObjectFileName STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc44: Name STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
de99: AudioWAVECodec UINT32 data type enumeration: 85, 352, 353, 354,
GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 2, 1, GET/SET
de93: SampleRate UINT32 data type range: MIN 32768, MAX 45158, STEP 1
GET/SET
de9a: AudioBitRate UINT32 data type range: MIN 8192, MAX 196608, STEP
1 READ ONLY
dc9b: AlbumArtist STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc96: Composer STRING data type GET/SET
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1
GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
3001: Association/Directory
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, READ ONLY
dc07: ObjectFileName STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc44: Name STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
Storage Devices:
StorageID: 0x12345678
StorageType: 0x0003
FilesystemType: 0x0002
AccessCapability: 0x0000
MaxCapacity: 7485345792
FreeSpaceInBytes: 7235375104
FreeSpaceInObjects: 0
StorageDescription: Internal Drv
VolumeIdentifier: 1234500LG000000000
Special directories:
Default music folder: 0x00000000
Default playlist folder: 0x00000000
Default picture folder: 0x00000000
Default video folder: 0x00000000
Default organizer folder: 0x00000000
Default zencast folder: 0x00000000
Default album folder: 0x00000000
Default text folder: 0x00000000
MTP-specific device properties:
Friendly name: KM900 Music Sync Player
Synchronization partner: Longhorn Sync Engine
Battery level 10 of 100 (10%)
libmtp supported (playable) filetypes:
Microsoft Windows Media Audio
ISO MPEG-1 Audio Layer 3
RIFF WAVE file
Ogg container format
Microsoft Advanced Systems Format
Unable to acquire device certificate, perhaps this device does not support
this
WMPInfo.xml Does not exist on this device
PTP: Closing session
OK.
