# mtp-detect
libmtp version: 0.3.7

Listing raw device(s)
Found 1 device(s):
Cowon: iAudio D2+ (MTP mode) (0e21:0861) @ bus 0, dev 21
Attempting to connect device(s)
USB low-level info:
Using kernel interface "usbfs"
bcdUSB: 512
bDeviceClass: 0
bDeviceSubClass: 0
bDeviceProtocol: 0
idVendor: 0e21
idProduct: 0861
IN endpoint maxpacket: 512 bytes
OUT endpoint maxpacket: 512 bytes
Raw device info:
Bus location: 0
Device number: 21
Device entry info:
Vendor: Cowon
Vendor id: 0x0e21
Product: iAudio D2+ (MTP mode)
Vendor id: 0x0861
Device flags: 0x00000006
Microsoft device descriptor 0xee:
0000: 1203 4d00 5300 4600 5400 3100 3000 3000 ..M.S.F.T.1.0.0.
0010: 0100 ..
Device info:
Manufacturer: COWON SYSTEMS, Inc.
Model: COWON D2 2.02
Device version: 2.02
Serial number: 0273F000A5EFDD792090410133609071
Vendor extension ID: 0x00000006
Vendor extension description: microsoft.com/WMPPD: 11.0;microsoft.com/WMDRMPD: 10.1;microsoft.com/WMPPD: 10.0;microsoft.com/AAVT: 1.0;microsoft.com/WMDRMND: 1.0;audible.com: 1.0;
Detected object size: 64 bits
Supported operations:
1001: get device info
1002: Open session
1003: Close session
1004: Get storage IDs
1005: Get storage info
1006: Get number of objects
1007: Get object handles
1008: Get object info
1009: Get object
100b: Delete object
100c: Send object info
100d: Send object
100f: Format storage
1010: Reset device
1014: Get device property description
1015: Get device property value
1016: Set device property value
9810: Get object references
9811: Set object references
9802: Get object property description
9801: Get object properties supported
9803: Get object property value
9804: Set object property value
9805: Get object property list
9806: Set object property list
101b: Get partial object
9201: Report Added/Deleted Items
9202: Report Acquired Items
9101: Get secure time challenge
9102: Get secure time response
9103: Set license response
9104: Get sync list
9105: Send meter challenge query
9106: Get meter challenge
9107: Get meter response
9108: Clean data store
9109: Get license state
910a: Send WMDRM-PD Command
910b: Send WMDRM-PD Request
9170: Open Media Session
9171: Close Media Session
9172: Get Next Data Block
9173: Set Current Time Position
9180: Send Registration Request
9181: Get Registration Response
9182: Get Proximity Challenge
9183: Send Proximity Response
9184: Send WMDRM-ND License Request
9185: Get WMDRM-ND License Response
Events supported:
0x4004
0x4005
Device Properties Supported:
0xd405: Device Icon
0xd100: Unknown property
0x5001: Battery Level
0xd401: Synchronization Partner
0xd402: Friendly Device Name
0xd101: Secure Time
0xd102: Device Certificate
0xd103: Revocation Info
Playable File (Object) Types and Object Properties Supported:
3001: Association/Directory
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
dc9a: AlbumName STRING data type GET/SET
3009: MP3
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222, GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3, GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc46: Artist STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
b901: WMA
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 320000, STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222, GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3, GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc46: Artist STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
3008: MS Wave
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222, GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3, GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc46: Artist STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
b904: Audible.com Codec
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222, GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3, GET/SET
da00: unknown(da00) UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8, GET/SET
da02: unknown(da02) UINT32 data type ANY 32BIT VALUE form READ ONLY
da03: unknown(da03) UINT16 data type enumeration: 0, 1, READ ONLY
da01: unknown(da01) STRING data type GET/SET
da04: unknown(da04) array of UINT8 data type ANY 8BIT VALUE form GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc8c: Genre STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
3801: JPEG
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
dc88: Height UINT32 data type range: MIN 1, MAX 270, STEP 1 GET/SET
3804: BMP
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
dc88: Height UINT32 data type range: MIN 1, MAX 270, STEP 1 GET/SET
300a: MS AVI
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
dc88: Height UINT32 data type range: MIN 1, MAX 270, STEP 1 GET/SET
de97: ScanDepth UINT16 data type enumeration: 1, READ ONLY
de9d: FramesPerThousandSeconds UINT32 data type enumeration: 0, 20000, 25000, 29970, 30000, 60000, GET/SET
de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 859189832, 958804552, 1195724877, 827739479, 844516695, 861293911, GET/SET
de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 850000, STEP 1 GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc8c: Genre STRING data type GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222, GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
dea1: EncodingProfile STRING data type GET/SET
b981: WMV
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
dc88: Height UINT32 data type range: MIN 1, MAX 270, STEP 1 GET/SET
de97: ScanDepth UINT16 data type enumeration: 1, READ ONLY
de9d: FramesPerThousandSeconds UINT32 data type enumeration: 0, 20000, 25000, 29970, 30000, 60000, GET/SET
de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 859189832, 958804552, 1195724877, 827739479, 844516695, 861293911, GET/SET
de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 850000, STEP 1 GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc8c: Genre STRING data type GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 128000, STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222, GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
dea1: EncodingProfile STRING data type GET/SET
b903: AAC
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222, GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3, GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc46: Artist STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
300c: ASF
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
dc88: Height UINT32 data type range: MIN 1, MAX 270, STEP 1 GET/SET
de97: ScanDepth UINT16 data type enumeration: 1, READ ONLY
de9d: FramesPerThousandSeconds UINT32 data type enumeration: 0, 20000, 25000, 29970, 30000, 60000, GET/SET
de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 859189832, 958804552, 1195724877, 827739479, 844516695, 861293911, GET/SET
de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 850000, STEP 1 GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc8c: Genre STRING data type GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222, GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
dea1: EncodingProfile STRING data type GET/SET
3001: Association/Directory
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
dc9a: AlbumName STRING data type GET/SET
ba05: Abstract Audio Video Playlist
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
3000: Undefined Type
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
b802: Firmware
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
ba03: Abstract Audio Album
dc44: Name STRING data type GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
dc86: RepresentativeSampleData array of UINT8 data type byte array: GET/SET
dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, READ ONLY
dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
dc9b: AlbumArtist STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
Storage Devices:
StorageID: 0x00010001
StorageType: 0x0003 fixed RAM storage
FilesystemType: 0x0002 generic hierarchical
AccessCapability: 0x0000 read/write
MaxCapacity: 3996581888
FreeSpaceInBytes: 21168128
FreeSpaceInObjects: 10355
StorageDescription: Internal Storage
VolumeIdentifier: 0273F000A5EFDD792090410133609071
StorageID: 0x00020001
StorageType: 0x0004 removable RAM storage
FilesystemType: 0x0002 generic hierarchical
AccessCapability: 0x0000 read/write
MaxCapacity: 16096690176
FreeSpaceInBytes: 345276416
FreeSpaceInObjects: 11112
StorageDescription: External Storage
VolumeIdentifier: 1273F000A5EFDD792090410133609071
Special directories:
Default music folder: 0x20000006
Default playlist folder: 0x00000000
Default picture folder: 0x20000003
Default video folder: 0x20000005
Default organizer folder: 0x00000000
Default zencast folder: 0x00000000
Default album folder: 0x00000000
Default text folder: 0x20000007
MTP-specific device properties:
Friendly name: COWON D2 2.02
Synchronization partner: Longhorn Sync Engine
Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
ISO MPEG-1 Audio Layer 3
Microsoft Windows Media Audio
RIFF WAVE file
Audible.com Audio Codec
JPEG file
BMP bitmap file
Audio Video Interleave
Microsoft Windows Media Video
Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
Microsoft Advanced Systems Format
Firmware file

Secure Time:
<DRMCLOCK type="status"><VALUE>#20090503
10:36:14Z#</VALUE><FLAG>DRM_CLK_SET</FLAG></DRMCLOCK>AG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID
private="1">AnPwAKXv3XkgkEEBM2CQcQAAAAA=</UNIQUEID><PUBLICKEY
private="1">FocgXnNjh3yjRT7aMhsJXS9JlhBNybR+M0F0C2ki1zHjSz1PI8/lFQ==</PUBLICKEY><KEYDATA>KQ6TsBwEpX86TWal0a/uCsjRLno=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>NG6lq1S5sNGgtBRlqT+9v0fCYH/gECTNQNqXRtkkQBktn5IA1VMrUA==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>imRLUBTdYwr/wuCdJ5pYee5ysRo=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.107.27</SECURITYVERSION><CERTIFICATE
private="1">FocgXnNjh3yjRT7aMhsJXS9JlhBNybR+M0F0C2ki1zHjSz1PI8/lFQIEaxtY2ogHvahilwVek+LHriDlf4tNGUWnE4kIf0bVWrd0Pd5HeEZ90h2H</CERTIFICATE></FALLBACK><CERTIFICATE
type="GROUP"><DATA><NAME>COWON D2</NAME><MANUFACTURER>COWON Systems,
Inc.</MANUFACTURER><MAKE>COWON Systems, Inc.</MAKE><DISTRIBUTOR>COWON
Systems, Inc.</DISTRIBUTOR><MODEL>COWON
D2</MODEL><SECURITYLEVEL>2000</SECURITYLEVEL><HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR><HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR><FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR><FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR><FEATURES><CLOCK>2</CLOCK><SECURECLOCK><URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL><PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY></SECURECLOCK><METERING>1</METERING><LICENSE_ACQ>1</LICENSE_ACQ><LICENSE_SYNC>1</LICENSE_SYNC><ENCRYPTION>1</ENCRYPTION><SYMMETRIC_OPT>1</SYMMETRIC_OPT></FEATURES><LIMITS><MAXCHAINDEPTH>2</MAXCHAINDEPTH><MAXLICENSESIZE>10240</MAXLICENSESIZE><MAXHEADERSIZE>5120</MAXHEADERSIZE></LIMITS><PUBLICKEY>nqh5lLdQUwb/0yQ9y3+cUH+Qg2XeitjH+HPqmIt1wGvt8KuMCXeLgg==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>RtHy/phLBjyBu6k4EBx1W4S3K1GZJMlR9XnsLYMShOuiOU3NWzoyWA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>1663</AUTH_ID><PUBLICKEY>5FiLcleC03a+pIcQA/uDrHgsHW1t2t9dQM9IhYTm5iHJdLD9RsGsBw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>dwo25uJJdhF215IfA6swRGEL+yzu+ZUjSyuVJI1rqRCK+y2lZgthWg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>q02PxB6SylsBhUa00Ul6rmqr+yVsLERU3MNfHbdn+XaSzbEEhynAgg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
inep: usb_get_endpoint_status(): Connection timed out
outep: usb_get_endpoint_status(): Connection timed out
usb_clear_halt() on IN endpoint: Connection timed out
usb_clear_halt() on OUT endpoint: Connection timed out
usb_clear_halt() on INTERRUPT endpoint: Connection timed out
OK.
