Listing raw device(s)
Found 1 device(s):
Toshiba: Gigabeat MET401 (0930:001d) @ bus 0, dev 3
Attempting to connect device(s)
PTP: Opening session
USB low-level info:
Using kernel interface "usbfs"
bcdUSB: 512
bDeviceClass: 255
bDeviceSubClass: 0
bDeviceProtocol: 0
idVendor: 0930
idProduct: 001d
IN endpoint maxpacket: 512 bytes
OUT endpoint maxpacket: 512 bytes
Raw device info:
Bus location: 0
Device number: 3
Device entry info:
Vendor: Toshiba
Vendor id: 0x0930
Product: Gigabeat MET401
Vendor id: 0x001d
Device flags: 0x00000000
Microsoft device descriptor 0xee:
0000: 1203 4d00 5300 4600 5400 3100 3000 3000 ..M.S.F.T.1.0.0.
0010: fe00 ..
Microsoft device response to control message 1, CMD 0xfe:
0000: 2800 0000 0001 0400 0100 0000 0000 0000 (...............
0010: 0001 4d54 5000 0000 0000 0000 0000 0000 ..MTP...........
0020: 0000 0000 0000 0000 ........
Potential MTP Device with VendorID:0930 and ProductID:001d responded to
control message 2 with a response that was too short. Problems may arrise
but continuing
Device info:
Manufacturer: TOSHIBA
Model: gigabeat_T Series
Device version: PMC: 2.21 (3:0); Platform: 2.1 (3.4)
Serial number: 32b0db90 - aced0f4e - 80bd1ff8 - 8ee00652
Vendor extension ID: 0x00000006
Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD:
10.1; microsoft.com/WMPPD: 11.1; microsoft.com/WMPMCPREMCONT: 1.0;
Detected object size: 64 bits
Supported operations:
1001: get device info
1002: Open session
1003: Close session
1004: Get storage IDs
1005: Get storage info
1006: Get number of objects
1007: Get object handles
1008: Get object info
1009: Get object
100b: Delete object
100c: Send object info
100d: Send object
100f: Format storage
1010: Reset device
1014: Get device property description
1015: Get device property value
1016: Set device property value
1019: Move object
101b: Get partial object
9810: Get object references
9811: Set object references
9802: Get object property description
9807: Get interdependent property description
9801: Get object properties supported
9803: Get object property value
9804: Set object property value
9805: Get object property list
9806: Set object property list
9808: Send object property list
9101: Get secure time challenge
9102: Get secure time response
9103: Set license response
9104: Get sync list
9105: Send meter challenge query
9106: Get meter challenge
9107: Get meter response
9108: Clean data store
9109: Get license state
910a: Send WMDRM-PD Command
910b: Send WMDRM-PD Request
9201: Report Added/Deleted Items
9202: Report Acquired Items
9204: Unknown (9204)
Events supported:
None.
Device Properties Supported:
0xd101: Secure Time
0xd401: Synchronization Partner
0x5001: Battery Level
0xd102: Device Certificate
0xd402: Friendly Device Name
0xd131: PlaysForSure ID
Playable File (Object) Types and Object Properties Supported:
3009: MP3
dc44: Name STRING data type GET/SET
dc04: ObjectSize UINT64 data type READ ONLY
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc9d: DRMStatus UINT16 data type enumeration: 0, 1, GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc0a: Keywords STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc42: SyncID STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
d901: BuyFlag UINT8 data type enumeration: 0, 1, GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 550000, STEP 1 READ
ONLY
dc9a: AlbumName STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1
GET/SET
dc8c: Genre STRING data type GET/SET
dc95: MetaGenre UINT16 data type enumeration: 1, 17, 18, 19, 20, 21, 33,
34, 35, 36, 37, 38, 39, 40, 48, GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50
GET/SET
de99: AudioWAVECodec UINT32 data type enumeration: 85, READ ONLY
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
b901: WMA
dc44: Name STRING data type GET/SET
dc04: ObjectSize UINT64 data type READ ONLY
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc9d: DRMStatus UINT16 data type enumeration: 0, 1, GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc0a: Keywords STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc42: SyncID STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
d901: BuyFlag UINT8 data type enumeration: 0, 1, GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 1572864, STEP 1 READ
ONLY
dc9a: AlbumName STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1
GET/SET
dc8c: Genre STRING data type GET/SET
dc95: MetaGenre UINT16 data type enumeration: 1, 17, 18, 19, 20, 21, 33,
34, 35, 36, 37, 38, 39, 40, 48, GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50
GET/SET
de99: AudioWAVECodec UINT32 data type enumeration: 353, 354, 355, 10, READ
ONLY
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
3008: MS Wave
dc44: Name STRING data type GET/SET
dc04: ObjectSize UINT64 data type READ ONLY
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc9d: DRMStatus UINT16 data type enumeration: 0, 1, GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc0a: Keywords STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc42: SyncID STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
d901: BuyFlag UINT8 data type enumeration: 0, 1, GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 1572864, STEP 1 READ
ONLY
dc9a: AlbumName STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1
GET/SET
dc8c: Genre STRING data type GET/SET
dc95: MetaGenre UINT16 data type enumeration: 1, 17, 18, 19, 20, 21, 33,
34, 35, 36, 37, 38, 39, 40, 48, GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
de93: SampleRate UINT32 data type range: MIN 4000, MAX 48000, STEP 50
GET/SET
de99: AudioWAVECodec UINT32 data type enumeration: 353, 85, 1, 2, 6, 17,
49, READ ONLY
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
300c: ASF
dc44: Name STRING data type GET/SET
dc04: ObjectSize UINT64 data type READ ONLY
dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX
30000, STEP 1 GET/SET
dc9d: DRMStatus UINT16 data type enumeration: 0, 1, GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc0a: Keywords STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
dc47: DateAuthored STRING data type DATETIME FORM GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc42: SyncID STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc4b: CopyrightInformation array of UINT16 data type ANY 16BIT VALUE form
GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dea1: EncodingProfile STRING data type GET/SET
d901: BuyFlag UINT8 data type enumeration: 0, 1, GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
de9e: KeyFrameDistance UINT32 data type range: MIN 3, MAX 3, STEP 1 GET/SET

dc9e: SubDescription array of UINT16 data type ANY 16BIT VALUE form GET/SET

dc4c: Source STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc95: MetaGenre UINT16 data type enumeration: 1, 17, 18, 19, 20, 21, 33,
34, 35, 36, 37, 38, 39, 40, 48, GET/SET
de91: TotalBitRate UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ
ONLY
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
dc94: ParentalRating STRING data type GET/SET
dc98: Subtitle STRING data type GET/SET
de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 363520, STEP 1 READ
ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 353, READ ONLY
de92: BitRateType UINT16 data type enumeration: 1, 2, GET/SET
de9f: BufferSize UINT32 data type range: MIN 3, MAX 3, STEP 1 GET/SET
dea0: EncodingQuality UINT32 data type range: MIN 50, MAX 50, STEP 1
GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50
GET/SET
de97: ScanDepth UINT16 data type range: MIN 1, MAX 1, STEP 1 READ ONLY
de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911, 827739479,
844516695, 1347833175, 844125783, GET/SET
de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 736000, STEP 1 READ
ONLY
b981: WMV
dc44: Name STRING data type GET/SET
dc04: ObjectSize UINT64 data type READ ONLY
dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX
30000, STEP 1 GET/SET
dc9d: DRMStatus UINT16 data type enumeration: 0, 1, GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc0a: Keywords STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
dc47: DateAuthored STRING data type DATETIME FORM GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc42: SyncID STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc4b: CopyrightInformation array of UINT16 data type ANY 16BIT VALUE form
GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dea1: EncodingProfile STRING data type GET/SET
d901: BuyFlag UINT8 data type enumeration: 0, 1, GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
de9e: KeyFrameDistance UINT32 data type range: MIN 3, MAX 3, STEP 1 GET/SET

dc9e: SubDescription array of UINT16 data type ANY 16BIT VALUE form GET/SET

dc4c: Source STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc95: MetaGenre UINT16 data type enumeration: 1, 17, 18, 19, 20, 21, 33,
34, 35, 36, 37, 38, 39, 40, 48, GET/SET
de91: TotalBitRate UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ
ONLY
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
dc94: ParentalRating STRING data type GET/SET
dc98: Subtitle STRING data type GET/SET
de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ
ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 353, READ ONLY
de92: BitRateType UINT16 data type enumeration: 1, 2, GET/SET
de9f: BufferSize UINT32 data type range: MIN 3, MAX 3, STEP 1 GET/SET
dea0: EncodingQuality UINT32 data type range: MIN 50, MAX 50, STEP 1
GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50
GET/SET
de97: ScanDepth UINT16 data type range: MIN 1, MAX 1, STEP 1 READ ONLY
de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911, 827739479,
844516695, 1347833175, 844125783, GET/SET
de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 736000, STEP 1 READ
ONLY
3801: JPEG
dc44: Name STRING data type GET/SET
dc04: ObjectSize UINT64 data type READ ONLY
dc88: Height UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc9d: DRMStatus UINT16 data type enumeration: 0, 1, GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc0a: Keywords STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc87: Width UINT32 data type range: MIN 0, MAX 640, STEP 1 GET/SET
dc47: DateAuthored STRING data type DATETIME FORM GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc42: SyncID STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
3804: BMP
dc44: Name STRING data type GET/SET
dc04: ObjectSize UINT64 data type READ ONLY
dc88: Height UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc9d: DRMStatus UINT16 data type enumeration: 0, 1, GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc0a: Keywords STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc87: Width UINT32 data type range: MIN 0, MAX 640, STEP 1 GET/SET
dc47: DateAuthored STRING data type DATETIME FORM GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc42: SyncID STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
3001: Association/Directory
dc44: Name STRING data type GET/SET
dc04: ObjectSize UINT64 data type READ ONLY
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc9d: DRMStatus UINT16 data type enumeration: 0, 1, GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc0a: Keywords STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc42: SyncID STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
ba03: Abstract Audio Album
dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 320,
STEP 1 GET/SET
dc44: Name STRING data type GET/SET
dc04: ObjectSize UINT64 data type READ ONLY
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc9d: DRMStatus UINT16 data type enumeration: 0, 1, GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc0a: Keywords STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP
1 GET/SET
dc42: SyncID STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,
GET/SET
d901: BuyFlag UINT8 data type enumeration: 0, 1, GET/SET
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 240,
STEP 1 GET/SET
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
dc9b: AlbumArtist STRING data type GET/SET
dc86: RepresentativeSampleData array of UINT8 data type byte array: GET/SET

dc46: Artist STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
ba05: Abstract Audio Video Playlist
dc44: Name STRING data type GET/SET
dc04: ObjectSize UINT64 data type READ ONLY
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc9d: DRMStatus UINT16 data type enumeration: 0, 1, GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc0a: Keywords STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc42: SyncID STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
3000: Undefined Type
dc44: Name STRING data type GET/SET
dc04: ObjectSize UINT64 data type READ ONLY
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc9d: DRMStatus UINT16 data type enumeration: 0, 1, GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc0a: Keywords STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc42: SyncID STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
b802: Firmware
dc44: Name STRING data type GET/SET
dc04: ObjectSize UINT64 data type READ ONLY
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc9d: DRMStatus UINT16 data type enumeration: 0, 1, GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc0a: Keywords STRING data type GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc42: SyncID STRING data type GET/SET
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ ONLY
Storage Devices:
StorageID: 0x00010001
StorageType: 0x0003
FilesystemType: 0x0002
AccessCapability: 0x0000
MaxCapacity: 3980918784
FreeSpaceInBytes: 2949480448
FreeSpaceInObjects: 4294967295
StorageDescription: Storage
VolumeIdentifier: 32b0db90 - aced0f4e - 80bd1ff8 - 8ee00652
Special directories:
Default music folder: 0x08000001
Default playlist folder: 0x00000000
Default picture folder: 0x08000006
Default video folder: 0x08000008
Default organizer folder: 0x00000000
Default zencast folder: 0x00000000
Default album folder: 0x0800000b
Default text folder: 0x00000000
MTP-specific device properties:
Friendly name: (NULL)
Synchronization partner: {6D522C79-BD5D-4BA2-B791-7CBFE5EDB75D}
Battery level 93 of 100 (93%)
libmtp supported (playable) filetypes:
ISO MPEG-1 Audio Layer 3
Microsoft Windows Media Audio
RIFF WAVE file
Microsoft Advanced Systems Format
Microsoft Windows Media Video
JPEG file
BMP bitmap file
Firmware file

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID
private="1">zCPCZLYFLvuKt0TnOISNxcmV/gM=</UNIQUEID><PUBLICKEY
private="1">aY+9QpVRs1h7fWqDuetEsTqHrX5mQa3Tp8C9V6k8oylA2vqTdMXTAg==</PUBLI
CKEY><KEYDATA>+6lyJzOWuTQvDLprp/0z8qOR7Ok=</KEYDATA></DATA><MSDRM_SIGNATURE
_VALUE>rzyoDNdhKdSFJXYxwBy8dezNTULUVf8wXXOU9O6LV8m1bHrrCBevRA==</MSDRM_SIGN
ATURE_VALUE><SYMSIGNATURE>ujbe6CEe0ruAawznaq1P0JTqGoY=</SYMSIGNATURE></CERT
IFICATE><FALLBACK><SECURITYVERSION>2.4.109.191</SECURITYVERSION><CERTIFICAT
E
private="1">aY+9QpVRs1h7fWqDuetEsTqHrX5mQa3Tp8C9V6k8oylA2vqTdMXTAgIEbb8x/9R
a9jMtNk1PMJdUSDZwY6uWdMqCnTUh7qXPgkhpR2koNPHV4k1O</CERTIFICATE></FALLBACK><
CERTIFICATE type="GROUP"><DATA><NAME>Gigabeat</NAME>
<MANUFACTURER>Toshiba Corporation</MANUFACTURER>
<MODEL>T Series</MODEL>
<HARDWARE_VER_MAJOR>1.0</HARDWARE_VER_MAJOR>
<FIRMWARE_VER_MAJOR>2.2</FIRMWARE_VER_MAJOR>
<SECURITYLEVEL>2000</SECURITYLEVEL>
<FEATURES>
<CLOCK>1</CLOCK>
<METERING>1</METERING>
<LICENSE_ACQ>1</LICENSE_ACQ>
<LICENSE_SYNC>1</LICENSE_SYNC>
<ENCRYPTION>1</ENCRYPTION>
</FEATURES>
<LIMITS>
<MAXCHAINDEPTH>2</MAXCHAINDEPTH>
<MAXLICENSESIZE>10240</MAXLICENSESIZE>
<MAXHEADERSIZE>5120</MAXHEADERSIZE>
</LIMITS><PUBLICKEY>kCbzqA4FQ9ydIlf1wFVQqfzGCkzzy4kIowhqKZnDzrz1CJjK/sKNEA=
=</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>McIRp9c8wex4xqODCC0lxMDViFUwuvBH
x8jnWqX19omsDZCNw0XXYg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>2339
</AUTH_ID><PUBLICKEY>3C+L7y4RbEeI220k9VkNLWdPZ2NRxfPuiO1n2CfEqgG8lJpCOKWfiQ
==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>MqlbyFzMugkUK9KyavQTXdHswD+xojP
6KT2UIARVlpkeR3u1+m1wbg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbO
gktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNA
TURE_VALUE>+wMFbh+eWDfLNaYMV/W2XpxlP3HZLNhULUFZiHT3hZ7IuNCcPjZeIA==</MSDRM_
SIGNATURE_VALUE></CERTIFICATE></DEVCERT>

Device description WMPInfo.xml file:
<DeviceInfo>
<WMP DeviceID="{954DDB85-5F58-403B-B5D3-F563D1FE742C}"
RelationshipID="{6D522C79-BD5D-4BA2-B791-7CBFE5EDB75D}"/>
</DeviceInfo>
