                                                                     
                                                                     
                                                                     
                                             
libmtp version: 0.3.7

Listing raw device(s)
   Found 1 device(s):
   Samsung: SAMSUNG Trance (04e8:6763) @ bus 0, dev 30
Attempting to connect device(s)
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 04e8
   idProduct: 6763
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 0
      Device number: 30
      Device entry info:
         Vendor: Samsung
         Vendor id: 0x04e8
         Product: SAMSUNG Trance
         Vendor id: 0x6763
         Device flags: 0x0000200a
Microsoft device descriptor 0xee:
	0000: 1203 4d00 5300 4600 5400 3100 3000 3000	..M.S.F.T.1.0.0.
	0010: 0100                                   	..
Device info:
   Manufacturer: SAMSUNG Electronics Inc.
   Model: SAMSUNG Trance
   Device version: (null)
   Serial number: 0AE1BE80000000000000000000000000
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com/WMDRMPD: 10.1;
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1010: Reset device
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   9810: Get object references
   9811: Set object references
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   101b: Get partial object
   9201: Report Added/Deleted Items
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
Events supported:
   0x4004
   0x4005
Device Properties Supported:
   0xd405: Device Icon
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd101: Secure Time
   0xd102: Device Certificate
Playable File (Object) Types and Object Properties Supported:
   3001: Association/Directory
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
   3009: MP3
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
   b901: WMA
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 320000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
   b903: AAC
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
   b983: MP2
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
   3801: JPEG
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc87: Width UINT32 data type range: MIN 1, MAX 320, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 1, MAX 240, STEP 1 GET/SET
   300c: ASF
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc87: Width UINT32 data type range: MIN 1, MAX 320, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 1, MAX 240, STEP 1 GET/SET
      de97: Scan Depth UINT16 data type enumeration: 1,  READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 1195724877, 861293911,  GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 1000, MAX 10000, STEP 1 GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 32768, MAX 768000, STEP 1 GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      dea1: Encoding Profile STRING data type GET/SET
   3001: Association/Directory
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
   ba05: Abstract Audio Video Playlist
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
   3000: Undefined Type
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
   b802: Firmware
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
   ba03: Abstract Audio Album
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc9b: Album Artist STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 929710080
      FreeSpaceInBytes: 241811456
      FreeSpaceInObjects: 3867
      StorageDescription: Internal Storage
      VolumeIdentifier: 0AE1BE80000000000000000000000000
Special directories:
   Default music folder: 0x20000002
   Default playlist folder: