libmtp version: 0.3.7

Listing raw device(s)
   Found 1 device(s):
   04e8:4f1f @ bus 0, dev 3
Attempting to connect device(s)
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 04e8
   idProduct: 4f1f
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 0
      Device number: 3
      Device entry info:
         Vendor: (null)
         Vendor id: 0x04e8
         Product: (null)
         Vendor id: 0x4f1f
         Device flags: 0x00000000
Microsoft device descriptor 0xee:
	0000: 1203 4d00 5300 4600 5400 3100 3000 3000	..M.S.F.T.1.0.0.
	0010: 6f00                                   	o.
Microsoft device response to control message 1, CMD 0x6f:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Microsoft device response to control message 2, CMD 0x6f:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Device info:
   Manufacturer: Samsung Electronics Co., Ltd. 
   Model: S8000
   Device version: S8000XPII1
   Serial number: 352028034990874
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMPPD: 11.0; microsoft.com/WMDRMPD: 10.1; 
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   101b: Get partial object
   9810: Get object references
   9811: Set object references
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9201: Report Added/Deleted Items
   1011: Self test device
   1012: Set object protection
   1017: Reset device property value
   1019: Move object
   101a: Copy object
   9808: Send object property list
   9001: Unknown (9001)
   9100: Unknown (9100)
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   9202: Report Acquired Items
Events supported:
   0x4001
   0x4004
   0x4005
   0x4006
Device Properties Supported:
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd404: Unknown property
   0xd407: Unknown property
   0xd101: Secure Time
   0xd102: Device Certificate
Playable File (Object) Types and Object Properties Supported:
   b984: 3GP
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 13000, MAX 192999, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14343, 14347, 14344, 47361, 12299,  READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: RepresentativeSampleDuration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 13000, MAX 192999, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14343, 14347, 14344, 47361, 12299,  READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: RepresentativeSampleDuration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 13000, MAX 192999, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14343, 14347, 14344, 47361, 12299,  READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: RepresentativeSampleDuration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
   b981: WMV
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 720, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 13000, MAX 192999, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 861293911,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 32000, MAX 2097152, STEP 1 GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type enumeration: 0, 15000, 24000, 25000, 29970, 30000,  GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea1: EncodingProfile STRING data type READ ONLY
   3801: JPEG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14343, 14347, 14344, 47361, 12299,  READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: RepresentativeSampleDuration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 0 GET/SET
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
   3807: GIF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14343, 14347, 14344, 47361, 12299,  READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: RepresentativeSampleDuration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 0 GET/SET
   300c: ASF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 720, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 13000, MAX 192999, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 861293911,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 32000, MAX 2097152, STEP 1 GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type enumeration: 0, 15000, 24000, 25000, 29970, 30000,  GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea1: EncodingProfile STRING data type READ ONLY
   ba03: Abstract Audio Album
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14343, 14347, 14344, 47361, 12299,  READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: RepresentativeSampleDuration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 0 GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 1451720704
      FreeSpaceInBytes: 1199013888
      FreeSpaceInObjects: 4294967295
      StorageDescription: Phone
      VolumeIdentifier: 35202803499087402
Special directories:
   Default music folder: 0x0000002f
   Default playlist folder: 0x00000065
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000033
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: S8000
   Synchronization partner: {00000000-0000-0000-0000-000000000000}
   Battery level 65 of 100 (65%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   Microsoft Windows Media Video
   JPEG file
   GIF bitmap file
   Microsoft Advanced Systems Format

Secure Time:
<DRMCLOCK type="status"><VALUE>#20091227 10:12:29Z#</VALUE><FLAG>DRM_CLK_SET</FLAG></DRMCLOCK>A

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">JnmpDJHz8CRCVuXpQvCRqQ==</UNIQUEID><PUBLICKEY private="1">WoQeIfoZg4CMlODWgBv21RH4iV0m/FbA64wmJ4uoE1RPlJ2icGKvGQ==</PUBLICKEY><KEYDATA>K8omLjdykUmJ7DI68+XbHHNXO4k=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>vJL9M2hYvkhVWccjEaBDDYmCN3WukLUGgo3RtXDf9z840idVNTkiEQ==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>AXDx8CNkgGxNXjuJNCQUeOBxr8I=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.114.13</SECURITYVERSION><CERTIFICATE private="1">WoQeIfoZg4CMlODWgBv21RH4iV0m/FbA64wmJ4uoE1RPlJ2icGKvGQIEcg2IEDtoEELx3ur+seu5q5+3Dn1KPSRgfDBVm+OPLQa6UiS10lmK1X2B</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>Cubic31</NAME>
    <MANUFACTURER>SAMSUNG</MANUFACTURER>
    <DISTRIBUTOR>SAMSUNG</DISTRIBUTOR>
    <MODEL>SGH-S8000</MODEL>
    <SECURITYLEVEL>2000</SECURITYLEVEL>
    <HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
    <HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR>
    <FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR>
    <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
    <FEATURES>
        <CLOCK>2</CLOCK>
        <SECURECLOCK>
            <URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
            <PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY>
        </SECURECLOCK>
        <METERING>1</METERING>
        <LICENSE_ACQ>0</LICENSE_ACQ>
        <LICENSE_SYNC>1</LICENSE_SYNC>
        <ENCRYPTION>1</ENCRYPTION>
        <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
    </FEATURES>
    <LIMITS>
        <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
        <MAXLICENSESIZE>10240</MAXLICENSESIZE>
        <MAXHEADERSIZE>5120</MAXHEADERSIZE>
    </LIMITS><PUBLICKEY>sZZi0cv/dmcU2Bb1KP/04kpanCcybQOzzBSRHmZ42rmahFrgIw2FWQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>7u8opXL8mbp850/RopOqtvONCnA1vys1qdTXKMqY8POsypgQ0mQ/TQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>3441</AUTH_ID><PUBLICKEY>Abb3pqHX4u+ZIKo/ueOeTeJszXUVVoCOahFF+lwHIwmaNA3oTLynEw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>vT0csOAP1wl67T9OMas/o30tBWj8TUhx1Q63CdjIqVxV6Qbersh9Mg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>jy3yFxR1yLlx5p4ZSto/ir2a2Ub89uTHiEY72fmZ8ncTc+HXRakPew==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>

WMPInfo.xml file contents:
<DeviceInfo>
    <WMP DeviceID="{CA8A530C-CE2C-4724-AB3D-E5034A3EF13E}" RelationshipID="{00000000-0000-0000-0000-000000000000}"/>
</DeviceInfo>

OK.

 	  	 
