libmtp version: 0.2.6.1

Attempting to connect device(s)
Device 1 (VID=4102 and PID=1141) is UNKNOWN.
Please report this VID/PID and the device model to the libmtp development team
PTP: Opening session
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 255
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 4102
   idProduct: 1141
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000000
Microsoft device descriptor 0xee:
        0000: 1203 4d00 5300 4600 5400 3100 3000 3000   ..M.S.F.T.1.0.0.
        0010: fe00                                      ..
Microsoft device response to control message 1, CMD 0xfe:
        0000: 2800 0000 0001 0400 0100 0000 0000 0000   (...............
        0010: 0001 4d54 5000 0000 0000 0000 0000 0000   ..MTP...........
        0020: 0000 0000 0000 0000                       ........
Microsoft device response to control message 2, CMD 0xfe:
        0000: 2800 0000 0001 0400 0100 0000 0000 0000   (...............
        0010: 0001 4d54 5000 0000 0000 0000 0000 0000   ..MTP...........
        0020: 0000 0000 0000 0000                       ........
Device info:
   Manufacturer: iriver
   Model: iriver E100
   Device version: TP-0.31-N-ENG
   Serial number: 221D9DA65E73B749BEE2C2BA869606DB
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 10.0;
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   101b: Get partial object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1010: Reset device
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   9810: Get object references
   9811: Set object references
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   9201: Report Added/Deleted Items
Events supported:
   None.
Device Properties Supported:
   0xd101: Secure Time
   0xd401: Synchronization Partner
   0x5001: Battery Level
   0xd102: Device Certificate
   0xd402: Friendly Device Name
Playable File (Object) Types and Object Properties Supported:
   3009: MP3
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 384000, STEP 1 READ ONLY
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
   b901: WMA
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 384000, STEP 1 READ ONLY
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
   300c: ASF
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      de97: ScanDepth UINT16 data type enumeration: 1,  READ ONLY
      de91: TotalBitRate UINT32 data type range: MIN 1, MAX 1234000, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 384000, STEP 1 READ ONLY
      dc8c: Genre STRING data type GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      dc94: ParentalRating STRING data type GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911, 0, 859189832, 958804552, 1195724877, 827739479, 844516695,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 850000, STEP 1 READ ONLY
   b981: WMV
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      de97: ScanDepth UINT16 data type enumeration: 1,  READ ONLY
      de91: TotalBitRate UINT32 data type range: MIN 1, MAX 1234000, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 384000, STEP 1 READ ONLY
      dc8c: Genre STRING data type GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      dc94: ParentalRating STRING data type GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911, 0, 859189832, 958804552, 1195724877, 827739479, 844516695,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 850000, STEP 1 READ ONLY
   3801: JPEG
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
   3001: Association/Directory
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
   ba03: Abstract Audio Album
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
   ba05: Abstract Audio Video Playlist
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
   3000: Undefined Type
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
   300a: MS AVI
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
      dc09: DateModified STRING data type READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      de97: ScanDepth UINT16 data type enumeration: 1,  READ ONLY
      de91: TotalBitRate UINT32 data type range: MIN 1, MAX 1234000, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 384000, STEP 1 READ ONLY
      dc8c: Genre STRING data type GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      dc94: ParentalRating STRING data type GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911, 0, 859189832, 958804552, 1195724877, 827739479, 844516695,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 850000, STEP 1 READ ONLY
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 8005951488
      FreeSpaceInBytes: 7986962432
      FreeSpaceInObjects: 4294967295
      StorageDescription: iriver E100 Files
      VolumeIdentifier: 295BB680
Special directories:
   Default music folder: 0x05000160
   Default playlist folder: 0x00000000
   Default picture folder: 0x05000161
   Default video folder: 0x05000167
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x05000166
MTP-specific device properties:
   Friendly name: iriver E100
   Synchronization partner: Longhorn Sync Engine
   Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   Microsoft Advanced Systems Format
   Microsoft Windows Media Video
   JPEG file
   Audio Video Interleave

Secure Time:
<DRMCLOCK type="status"><VALUE>#20080607 19:07:51Z#</VALUE><FLAG>DRM_CLK_NOT_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">vbwnhPegN0G8TdpyfN8iEHzfIhA=</UNIQUEID><PUBLICKEY private="1">gwgEFp4IDGEN1kTBlsKYi4WjBQyUynbJgLfj/nX3PBiSXcyr72Inhg==</PUBLICKEY><KEYDATA>X9igEHuLA+KGSJLeCSoXezHVDks=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>gwgEFp4IDGEN1kTBlsKYi4WjBQxEBpbLlor68NtpJ9fTpQIoI6sFZg==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>TR1/tCkL16gODgMHD9nbaFh8kms=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.110.179</SECURITYVERSION><CERTIFICATE private="1">gwgEFp4IDGEN1kTBlsKYi4WjBQyUynbJgLfj/nX3PBiSXcyr72InhgIEbrODCAQWnggMYQ3WRMGWwpiLhaMFDEJ2vuXzjtooUZDEdNIMca4Ac3sS</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>iriver E100</NAME><MANUFACTURER>iriver</MANUFACTURER><MAKE>iriver</MAKE><DISTRIBUTOR>iriver</DISTRIBUTOR><MODEL>E100</MODEL><SECURITYLEVEL>2000</SECURITYLEVEL><HARDWARE_VER_MAJOR>1.0</HARDWARE_VER_MAJOR><HARDWARE_VER_MINOR>1.0</HARDWARE_VER_MINOR><FIRMWARE_VER_MAJOR>1.0</FIRMWARE_VER_MAJOR><FIRMWARE_VER_MINOR>1.0</FIRMWARE_VER_MINOR><FEATURES><CLOCK>2</CLOCK><SECURECLOCK><URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL><PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY></SECURECLOCK><METERING>1</METERING><LICENSE_ACQ>0</LICENSE_ACQ><LICENSE_SYNC>1</LICENSE_SYNC><ENCRYPTION>0</ENCRYPTION><SYMMETRIC_OPT>0</SYMMETRIC_OPT></FEATURES><LIMITS><MAXCHAINDEPTH>2</MAXCHAINDEPTH><MAXLICENSESIZE>6656</MAXLICENSESIZE><MAXHEADERSIZE>5120</MAXHEADERSIZE></LIMITS><PUBLICKEY>2iVOcUjU7JrpG+uOw9vVbTb8jDP6sV4dDXK6dHIL+Wk5M9Qi/BclQg==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>wXNWf4yNWXzMSKmNUPSWSV1AxjzNFLJbobqx0V1p6U8GJhTJCFXgSg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>2583</AUTH_ID><PUBLICKEY>+K7NGoI9HmjKoRiHuYZc+jzrxxI5/FyecBmrMwUGMVpVSSz0yf0afw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>XQp6TZ6dU7CXjnLV63oEx3QdOUCuKJiUAA8aWwbIUaaagtDFP6ulJg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>xyI6ehQfX1XKnjVTtCJgqgjfyy3GzKkucEMXquxs1/KUrpENRGQjBA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
WMPInfo.xml Does not exist on this device
PTP: Closing session
usb_clear_halt() on INTERRUPT endpoint: Broken pipe
OK.
