Device 0 (VID=04e8 and PID=68af) is UNKNOWN.
Please report this VID/PID and the device model to the libmtp development team
libmtp version: 1.0.3

Listing raw device(s)
   Found 1 device(s):
   04e8:68af @ bus 2, dev 3
Attempting to connect device(s)
USB low-level info:
   Using kernel interface "dummy"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 04e8
   idProduct: 68af
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 2
      Device number: 3
      Device entry info:
         Vendor: (null)
         Vendor id: 0x04e8
         Product: (null)
         Vendor id: 0x68af
         Device flags: 0x00000000
Configuration 0, interface 0, altsetting 0:
   Interface implements PTP class, no further probing.
Device info:
   Manufacturer: Samsung Electronics Co., Ltd. 
   Model: GT-B2710
   Device version: B2710XXJK1
   Serial number: 353531041042851
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMPPD: 11.0; microsoft.com/WMDRMPD: 10.1; 
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   101b: Get partial object
   9810: Get object references
   9811: Set object references
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9201: Report Added/Deleted Items
   1011: Self test device
   1012: Set object protection
   1017: Reset device property value
   1019: Move object
   101a: Copy object
   9808: Send object property list
   9001: Unknown (9001)
   9100: Unknown (9100)
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   9202: Report Acquired Items
Events supported:
   0x4001
   0x4004
   0x4005
   0x4006
Device Properties Supported:
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd404: Unknown property
   0xd407: Perceived Device Type
   0xd101: Secure Time
   0xd102: Device Certificate
Playable File (Object) Types and Object Properties Supported:
   b984: 3GP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 85,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 320999, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2,  GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14343, 14347, 14344, 47361, 12299,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: Representative Sample Duration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   b982: MP4
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 176, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 144, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de97: Scan Depth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 85, 352, 353,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 16999, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 32000, MAX 288000, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type enumeration: 0, 15000,  GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   3009: MP3
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 85,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 320999, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2,  GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14343, 14347, 14344, 47361, 12299,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: Representative Sample Duration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   b901: WMA
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 85, 352, 353,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 192999, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2,  GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14343, 14347, 14344, 47361, 12299,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: Representative Sample Duration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   b981: WMV
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 176, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 144, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de97: Scan Depth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 85, 352, 353,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 16999, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 32000, MAX 288000, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type enumeration: 0, 15000,  GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   3801: JPEG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 3000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 3000, STEP 1 GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14343, 14347, 14344, 47361, 12299,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: Representative Sample Duration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 0 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   3001: Association/Directory
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
   3000: Undefined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
   3807: GIF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 3000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 3000, STEP 1 GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14343, 14347, 14344, 47361, 12299,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: Representative Sample Duration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 0 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   3804: BMP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 3000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 3000, STEP 1 GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14343, 14347, 14344, 47361, 12299,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: Representative Sample Duration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 0 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   380b: PNG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 3000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 3000, STEP 1 GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14343, 14347, 14344, 47361, 12299,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: Representative Sample Duration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 0 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   300c: ASF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 176, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 144, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de97: Scan Depth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 85, 352, 353,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 16999, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 32000, MAX 288000, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type enumeration: 0, 15000,  GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
   ba03: Abstract Audio Album
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 3000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 3000, STEP 1 GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14343, 14347, 14344, 47361, 12299,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: Representative Sample Duration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 0 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
Storage Devices:
   StorageID: 0x00020001
      StorageType: 0x0004 removable RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 1960169472
      FreeSpaceInBytes: 76406784
      FreeSpaceInObjects: 4294967295
      StorageDescription: Card
      VolumeIdentifier: 353531041042851-20001
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 128647168
      FreeSpaceInBytes: 12087296
      FreeSpaceInObjects: 4294967295
      StorageDescription: Phone
      VolumeIdentifier: 353531041042851-10001
Special directories:
   Default music folder: 0xffffffff
   Default playlist folder: 0xffffffff
   Default picture folder: 0xffffffff
   Default video folder: 0xffffffff
   Default organizer folder: 0xffffffff
   Default zencast folder: 0xffffffff
   Default album folder: 0xffffffff
   Default text folder: 0xffffffff
MTP-specific device properties:
   Friendly name: GT-B2710
   Synchronization partner: (NULL)
   Battery level 85 of 100 (85%)
libmtp supported (playable) filetypes:
   MPEG-4 Part 14 Container Format (Audio+Video Emphasis)
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   Microsoft Windows Media Video
   JPEG file
   Abstract Playlist file
   GIF bitmap file
   BMP bitmap file
   Portable Network Graphics
   Microsoft Advanced Systems Format
   Abstract Album file

Secure Time:
<DRMCLOCK type="status"><VALUE>#20112222 13:58:43Z#</VALUE><FLAG>DRM_CLK_NOT_SET</FLAG></DRMCLOCK>A
OK.
