# mtp-detect
libmtp version: 0.2.6.1

Attempting to connect device(s)
Potential MTP Device with VendorID:04da and ProductID:2145 responded to control
message 2 with a response that was too short. Problems may arrise but continuing
Device 1 (VID=04da and PID=2145) is UNKNOWN.
Please report this VID/PID and the device model to the libmtp development team
PTP: Opening session
Detect: Successfully connected 1 devices
USB low-level info:
  Using kernel interface "usbfs"
  bcdUSB: 512
  bDeviceClass: 255
  bDeviceSubClass: 0
  bDeviceProtocol: 0
  idVendor: 04da
  idProduct: 2145
  IN endpoint maxpacket: 64 bytes
  OUT endpoint maxpacket: 64 bytes
  Device flags: 0x00000000
Microsoft device descriptor 0xee:
	0000: 1203 4d00 5300 4600 5400 3100 3000 3000	..M.S.F.T.1.0.0.
	0010: fe00                                   	..
Microsoft device response to control message 1, CMD 0xfe:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Potential MTP Device with VendorID:04da and ProductID:2145 responded to control
message 2 with a response that was too short. Problems may arrise but continuing
Device info:
  Manufacturer: NTT DoCoMo, Inc.
  Model: FOMA P905i
  Device version: 1.00
  Serial number: 359932012198934
  Vendor extension ID: 0x00000006
  Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD:
10.1;
  Detected object size: 64 bits
Supported operations:
  1001: get device info
  1002: Open session
  1003: Close session
  1004: Get storage IDs
  1005: Get storage info
  1007: Get object handles
  1008: Get object info
  100d: Send object
  9808: Send object property list
  9802: Get object property description
  1014: Get device property description
  1015: Get device property value
  9801: Get object properties supported
  9803: Get object property value
  9805: Get object property list
  1009: Get object
  100b: Delete object
  9806: Set object property list
  9811: Set object references
  9810: Get object references
  1016: Set device property value
  9103: Set license response
  9104: Get sync list
  9105: Send meter challenge query
  9106: Get meter challenge
  9107: Get meter response
  9108: Clean data store
  9109: Get license state
  9201: Report Added/Deleted Items
  9804: Set object property value
Events supported:
  None.
Device Properties Supported:
  0xd402: Friendly Device Name
  0xd102: Device Certificate
Playable File (Object) Types and Object Properties Supported:
  b901: WMA
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form GET/SET
     dc44: Name STRING data type GET/SET
     dc07: ObjectFileName STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     de93: SampleRate UINT32 data type enumeration: 32000, 44100, 48000,  READ
ONLY
     de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 393216, STEP
1 READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
  ba03: Abstract Audio Album
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form GET/SET
     dc44: Name STRING data type GET/SET
     dc07: ObjectFileName STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,
14344,  READ ONLY
     dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 51200,
STEP 1 READ ONLY
     dc86: RepresentativeSampleData array of UINT8 data type byte array:
GET/SET
     dc83: RepresentativeSampleHeight UINT32 data type ANY 32BIT VALUE form
GET/SET
     dc84: RepresentativeSampleWidth UINT32 data type ANY 32BIT VALUE form
GET/SET
  3801: JPEG
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form GET/SET
     dc44: Name STRING data type GET/SET
     dc07: ObjectFileName STRING data type GET/SET
  3808: JFIF
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form GET/SET
     dc44: Name STRING data type GET/SET
     dc07: ObjectFileName STRING data type GET/SET
  ba05: Abstract Audio Video Playlist
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form GET/SET
     dc07: ObjectFileName STRING data type GET/SET
  3001: Association/Directory
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form GET/SET
     dc07: ObjectFileName STRING data type GET/SET
  3000: Undefined Type
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form GET/SET
     dc44: Name STRING data type GET/SET
     dc07: ObjectFileName STRING data type GET/SET
Storage Devices:
  StorageID: 0x20000001
     StorageType: 0x0004
     FilesystemType: 0x0000
     AccessCapability: 0x0000
     MaxCapacity: 2007105536
     FreeSpaceInBytes: 1028214784
     FreeSpaceInObjects: 4294967295
     StorageDescription: FOMA P905i
     VolumeIdentifier: FOMA P905i
Special directories:
  Default music folder: 0x80000004
  Default playlist folder: 0x80000006
  Default picture folder: 0x00000000
  Default video folder: 0x80000005
  Default organizer folder: 0x00000000
  Default zencast folder: 0x00000000
  Default album folder: 0x00000000
  Default text folder: 0x00000000
MTP-specific device properties:
  Friendly name: FOMA P905i
  Synchronization partner: (NULL)
libmtp supported (playable) filetypes:
  Microsoft Windows Media Audio
  JPEG file
  JFIF file

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID
private="1">MzU5OTMyMDEyMTk4OTM0AA==</UNIQUEID><PUBLICKEY
private="1">Adw2RbDMqN3623OpbuQ7ITqI30m7NzRg9CzllExqcJp/+8S1mJp2Yg==</PUBLICKEY>
<KEYDATA>n61BlX1zKoM02xgoMyJExkGQJ6E=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>A4K
+BK7dqQV+5CUHjZanbdQ1PUUzA9U3QqUY49T67mPxBwYiTH2+Yw==</MSDRM_SIGNATURE_VALUE><SY
MSIGNATURE>CH1xzklFcUG9psOZGdkwk5iP1J8=</SYMSIGNATURE></CERTIFICATE><FALLBACK><S
ECURITYVERSION>2.4.108.233</SECURITYVERSION><CERTIFICATE
private="1">Adw2RbDMqN3623OpbuQ7ITqI30m7NzRg9CzllExqcJp/+8S1mJp2YgIEbOkRkrDP4J/p
41/lyIJhR/emYvf2MsQP+42XHYI6OwPxQ9/U+ooMQRQc</CERTIFICATE></FALLBACK><CERTIFICATE
type="GROUP"><DATA><NAME>FOMA P905i</NAME>
   <MANUFACTURER>NTT DoCoMo,Inc.</MANUFACTURER>
   <MAKE>FOMA</MAKE>
   <DISTRIBUTOR>NTT DoCoMo,Inc.</DISTRIBUTOR>
   <MODEL>FOMA P905i</MODEL>
   <SECURITYLEVEL>2000</SECURITYLEVEL>
   <HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
   <HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR>
   <FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR>
   <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
   <FEATURES>
       <CLOCK>1</CLOCK>
       <METERING>1</METERING>
       <LICENSE_ACQ>1</LICENSE_ACQ>
       <LICENSE_SYNC>1</LICENSE_SYNC>
       <ENCRYPTION>0</ENCRYPTION>
       <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
   </FEATURES>
   <LIMITS>
       <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
       <MAXLICENSESIZE>10240</MAXLICENSESIZE>
       <MAXHEADERSIZE>5120</MAXHEADERSIZE>
   </LIMITS><PUBLICKEY>HwUCI7gHH1ZybUNQRIoCo7lQbDueSYHFAd1hKelLIeIOpcHYSCkVRA==
</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>dthTs0fWHk8uKep5zgaHpNgBQYZ5jlJenfYM1R
FjHD+A66mQcmJ4ag==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>2125</AUT
H_ID><PUBLICKEY>ThEIUCcbtn0ezIiysPDfAGofE3yX9h56YU2JOuXdI+4m9d2U5a6ITA==</PUBLIC
KEY></DATA><MSDRM_SIGNATURE_VALUE>qWuUY8ejlOo0YtatVCNw2G1fllU7cKxFKzX65RdUjiIaRe
E2LHw5Zw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnb
YaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE
3ccB47pqSRZsN88JmpROZk9uHIJvrTqo2tFebbaN84urCZ7iAWFOGQ==</MSDRM_SIGNATURE_VALUE
</CERTIFICATE></DEVCERT>
WMPInfo.xml Does not exist on this device
PTP: Closing session
OK.