Device 0 (VID=054c and PID=05a8) is a Sony NWZ-S765.
object 8 has parent 0xffffffff (-1) continuing anyway
object 9 has parent 0xffffffff (-1) continuing anyway
object a has parent 0xffffffff (-1) continuing anyway
object b has parent 0xffffffff (-1) continuing anyway
object c has parent 0xffffffff (-1) continuing anyway
object d has parent 0xffffffff (-1) continuing anyway
object e has parent 0xffffffff (-1) continuing anyway
object f has parent 0xffffffff (-1) continuing anyway
object 10 has parent 0xffffffff (-1) continuing anyway
object 11 has parent 0xffffffff (-1) continuing anyway
object 1f4 has parent 0xffffffff (-1) continuing anyway
object 1f5 has parent 0xffffffff (-1) continuing anyway

libmtp version: 1.1.0

Listing raw device(s)
   Found 1 device(s):
   Sony: NWZ-S765 (054c:05a8) @ bus 1, dev 12
Attempting to connect device(s)
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 054c
   idProduct: 05a8
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 1
      Device number: 12
      Device entry info:
         Vendor: Sony
         Vendor id: 0x054c
         Product: NWZ-S765
         Vendor id: 0x05a8
         Device flags: 0x12000006
Device info:
   Manufacturer: Sony Corporation
   Model: WALKMAN NWZ-S765
   Device version: 1.00
   Serial number: 00000000000000000000000005436965
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; sony.net/WMFU: 1.0; 
   Detected object size: 64 bits
   Extensions:
        microsoft.com: 1.0
         microsoft.com/WMDRMPD: 10.1
         sony.net/WMFU: 1.0
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   101b: Get partial object
   9810: Get object references
   9811: Set object references
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9201: Report Added/Deleted Items
   9807: Get interdependent property description
   9808: Send object property list
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   9401: Unknown (9401)
   9402: Unknown (9402)
Events supported:
   None.
Device Properties Supported:
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd101: Secure Time
   0xd102: Device Certificate
   0xd303: Unknown property
Playable File (Object) Types and Object Properties Supported:
   3000: Undefined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
   3001: Association/Directory
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
   3008: MS Wave
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 1,  GET/SET
      de9a: Audio Bit Rate UINT32 data type enumeration: 128000, 176400, 192000, 256000, 352800, 384000, 512000, 705600, 768000, 1024000, 1411200, 1536000,  GET/SET
      de91: Total Bit Rate UINT32 data type enumeration: 128000, 176400, 192000, 256000, 352800, 384000, 512000, 705600, 768000, 1024000, 1411200, 1536000,  GET/SET
   3009: MP3
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 85,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 32000, MAX 320000, STEP 1 GET/SET
      de91: Total Bit Rate UINT32 data type range: MIN 32000, MAX 320000, STEP 1 GET/SET
   300c: ASF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 1, MAX 270, STEP 1 GET/SET
      dc89: Duration UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 353,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 5512000, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 826496599, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 5000000, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 1000, MAX 30000, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type GET/SET
      de97: Scan Depth UINT16 data type enumeration: 1,  GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 15, MAX 15, STEP 1 GET/SET
   3801: JPEG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 65536, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 200, STEP 1 GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 200, STEP 1 GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      dc87: Width UINT32 data type range: MIN 1, MAX 4096, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 1, MAX 4096, STEP 1 GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
   b802: Firmware
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
   b901: WMA
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 352, 353,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 512000, STEP 1 GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      de91: Total Bit Rate UINT32 data type range: MIN 5000, MAX 512000, STEP 1 GET/SET
   b982: MP4
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc42: Sync ID STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 34, MAX 720, STEP 2 GET/SET
      dc88: Height UINT32 data type range: MIN 32, MAX 480, STEP 2 GET/SET
      dc89: Duration UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 5648,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 16000, MAX 576000, STEP 1 GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      de91: Total Bit Rate UINT32 data type range: MIN 0, MAX 10576000, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 844313677, 875967048,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX 10000000, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 1000, MAX 30000, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type GET/SET
   b984: 3GP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 5648,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 16000, MAX 576000, STEP 1 GET/SET
      de91: Total Bit Rate UINT32 data type range: MIN 16000, MAX 576000, STEP 1 GET/SET
   ba03: Abstract Audio Album
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 65536, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 200, STEP 1 GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 200, STEP 1 GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
   b981: WMV
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 32, MAX 720, STEP 2 GET/SET
      dc88: Height UINT32 data type range: MIN 32, MAX 480, STEP 2 GET/SET
      dc89: Duration UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 353,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 6512000, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 826496599, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 6000000, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 1000, MAX 30000, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type GET/SET
      de97: Scan Depth UINT16 data type enumeration: 1,  GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 15, MAX 15, STEP 1 GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 15139110912
      FreeSpaceInBytes: 10569613312
      FreeSpaceInObjects: 4294967295
      StorageDescription: Storage Media
      VolumeIdentifier: 00000000000000000000000005436965
Special directories:
   Default music folder: 0x00000008
   Default playlist folder: 0xffffffff
   Default picture folder: 0x0000000b
   Default video folder: 0x0000000c
   Default organizer folder: 0xffffffff
   Default zencast folder: 0xffffffff
   Default album folder: 0x000001f4
   Default text folder: 0xffffffff
MTP-specific device properties:
   Friendly name: WALKMAN
   Synchronization partner: (NULL)
   Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
   Folder
   RIFF WAVE file
   ISO MPEG-1 Audio Layer 3
   Microsoft Advanced Systems Format
   JPEG file
   Firmware file
   Microsoft Windows Media Audio
   MPEG-4 Part 14 Container Format (Audio+Video Emphasis)
   Abstract Album file
   Abstract Playlist file
   Microsoft Windows Media Video

Secure Time:
<DRMCLOCK type="status"><VALUE>#20114433 20:26:16Z#</VALUE><FLAG>DRM_CLK_NOT_SET</FLAG></DRMCLOCK>AG></DRMCLOCK>

WMPInfo.xml file contents:
<DeviceInfo>
    <WMP DeviceID="{15762964-BBCD-4530-8A2D-03A836DE1FC2}" RelationshipID="{A3EBBD19-116D-4BD8-AE85-E95BF79EFDAB}"/>
</DeviceInfo>

OK.
