libmtp version: 0.3.7

Listing raw device(s)
   Found 1 device(s):
   106c:3215 @ bus 0, dev 20
Attempting to connect device(s)
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 106c
   idProduct: 3215
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 0
      Device number: 20
      Device entry info:
         Vendor: (null)
         Vendor id: 0x106c
         Product: (null)
         Vendor id: 0x3215
         Device flags: 0x00000000
Microsoft device descriptor 0xee:
	0000: 1203 4d00 5300 4600 5400 3100 3000 3000	..M.S.F.T.1.0.0.
	0010: fe00                                   	..
Microsoft device response to control message 1, CMD 0xfe:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Device info:
   Manufacturer: Qualcomm
   Model: Windows Simulator
   Device version: Qualcomm MTP1.0
   Serial number: 000000000000000000a00000087f5e91
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0;microsoft.com/WMDRMPD: 10.1;microsoft.com/WMPPD: 10.0;
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   101b: Get partial object
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9810: Get object references
   9811: Set object references
   9201: Report Added/Deleted Items
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
Events supported:
   0x4001
   0x4004
   0x4005
Device Properties Supported:
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd102: Device Certificate
Playable File (Object) Types and Object Properties Supported:
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc06: AssociationDesc UINT32 data type ANY 32BIT VALUE form GET/SET
   3009: MP3
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 0, MAX 15000000, STEP 1 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 0, MAX 1000000, STEP 1 GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
   300b: MPEG
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 0, MAX 15000000, STEP 1 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 0, MAX 1000000, STEP 1 GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 0, MAX 8000000, STEP 1 GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 859189832, 958804552, 1195724877, 827739479, 844516695, 861293911,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 READ ONLY
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 0, MAX 60000, STEP 1 GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
   b982: MP4
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 0, MAX 15000000, STEP 1 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 0, MAX 1000000, STEP 1 GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 0, MAX 8000000, STEP 1 GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 859189832, 958804552, 1195724877, 827739479, 844516695, 861293911,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 READ ONLY
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 0, MAX 60000, STEP 1 GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
   300c: ASF
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 0, MAX 15000000, STEP 1 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 0, MAX 1000000, STEP 1 GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 0, MAX 8000000, STEP 1 GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 859189832, 958804552, 1195724877, 827739479, 844516695, 861293911,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 READ ONLY
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 0, MAX 60000, STEP 1 GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
   3801: JPEG
      dc87: Width UINT32 data type range: MIN 0, MAX 1920, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 1080, STEP 1 READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
   3808: JFIF
      dc87: Width UINT32 data type range: MIN 0, MAX 1920, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 1080, STEP 1 READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
   b802: Firmware
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
   b900: Undefined Audio
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 0, MAX 15000000, STEP 1 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 0, MAX 1000000, STEP 1 GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
   b901: WMA
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 0, MAX 15000000, STEP 1 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 0, MAX 1000000, STEP 1 GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
   b980: Undefined Video
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 0, MAX 15000000, STEP 1 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 0, MAX 1000000, STEP 1 GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 0, MAX 8000000, STEP 1 GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 859189832, 958804552, 1195724877, 827739479, 844516695, 861293911,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 READ ONLY
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 0, MAX 60000, STEP 1 GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
   b981: WMV
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 0, MAX 15000000, STEP 1 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 0, MAX 1000000, STEP 1 GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 0, MAX 8000000, STEP 1 GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 859189832, 958804552, 1195724877, 827739479, 844516695, 861293911,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 READ ONLY
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 0, MAX 60000, STEP 1 GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
   ba03: Abstract Audio Album
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
   ba04: Abstract Video Album
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
   ba05: Abstract Audio Video Playlist
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
Storage Devices:
   StorageID: 0x00020001
      StorageType: 0x0004 removable RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 989528064
      FreeSpaceInBytes: 518553600
      FreeSpaceInObjects: 4294967295
      StorageDescription: External Memory
      VolumeIdentifier: (null)
Special directories:
   Default music folder: 0x00000004
   Default playlist folder: 0x00000006
   Default picture folder: 0x00000005
   Default video folder: 0x00000008
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000003
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: Pantech CDM8999
   Synchronization partner: {00000000-0000-0000-0000-000000000000}
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   MPEG video stream
   MPEG-4 Part 14 Container Format (Audio+Video Empahsis)
   Microsoft Advanced Systems Format
   JPEG file
   JFIF file
   Firmware file
   Undefined audio file
   Microsoft Windows Media Audio
   Undefined video file
   Microsoft Windows Media Video

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">yoDDqRShyK2mYJZ9c/cSHuR7vjE=</UNIQUEID><PUBLICKEY private="1">pIaRCpBL7CdA3L2k7XMBsQ2pjhc4Axc+tWT6Pf4xVt2WPtbIld58ZA==</PUBLICKEY><KEYDATA>C0kz9Leve6CvWEMxy0WX72tISSk=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>mX+sDGRNKfz+P4u7nMqvRmVhnAry6Ut8bSRC/ohPVtaVA7VEJeucSg==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>hEqfgmU22fz1mRZ+ohqeC+y6nRk=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.116.37</SECURITYVERSION><CERTIFICATE private="1">pIaRCpBL7CdA3L2k7XMBsQ2pjhc4Axc+tWT6Pf4xVt2WPtbIld58ZAIEdCWXfBS24dtTDfqP4+LKEn+6oAvGSFp97V9Q91YVxXPCKGzoFR9M/ktp</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>VZW-1027</NAME>
    <MANUFACTURER>Pantech</MANUFACTURER>
    <MAKE>VZW-1027</MAKE>
    <DISTRIBUTOR>Verizon Wireless</DISTRIBUTOR>
    <MODEL>MOD 3.0</MODEL>
    <SECURITYLEVEL>2000</SECURITYLEVEL>
    <HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
    <HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR>
    <FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR>
    <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
    <FEATURES>
        <CLOCK>1</CLOCK>
        <METERING>1</METERING>
        <LICENSE_ACQ>1</LICENSE_ACQ>
        <LICENSE_SYNC>1</LICENSE_SYNC>
        <ENCRYPTION>1</ENCRYPTION>
        <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
    </FEATURES>
    <LIMITS>
        <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
        <MAXLICENSESIZE>10240</MAXLICENSESIZE>
        <MAXHEADERSIZE>5120</MAXHEADERSIZE>
    </LIMITS><PUBLICKEY>Y6MV8xqF9y35VN9RfsCP9iKSplr1NLp0jaHiHaW6IuLreMIg2mJAJg==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>obcPJxemEe+KW+ITUaGimNdrGAq4s4TpdW+Ugte5M73h5s6i/b/TKw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>3977</AUTH_ID><PUBLICKEY>hWw0FU2gcELjQp1HY+QyN7NJ6iphRYcTTOjF4KwYn/3XSs9IU7n/WA==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>Jm5BL6JXSU3WYCu7zSiPEOXq60zUDPOl5JvF3LD709vDiyVmoT0GFQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>3tCoVsnL5lV+SaJl2I80CrO0FzNWrdTjsfD3E6rMyvKbJrohDOT/VQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>

WMPInfo.xml file contents:
<DeviceInfo>
    <WMP DeviceID="{081E42D7-B691-4F2E-AAB0-25BDCF1EED73}" RelationshipID="{00000000-0000-0000-0000-000000000000}"/>
</DeviceInfo>

OK.
