libmtp version: 0.2.1

Attempting to connect device(s)
Potential MTP Device with VendorID:0781 and ProductID:7450 responded to
control message 2 with a response that was too short. Problems may arrise
but continuing
PTP: Opening session
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0781
   idProduct: 7450
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000002
Microsoft device descriptor 0xee:
        0000: 1203 4d00 5300 4600 5400 3100 3000 3000   ..M.S.F.T.1.0.0.
        0010: fe00 4d54 5000 0000 0000 0000 0000 0000   ..MTP...........
        0020: 0000 0000 0000 0000 6400 3000 3100 3800   ........d.0.1.8.
        0030: 3000 3400 3700 2d00 3600 6300 3000 3000   0.4.7.-.6.c.0.0.
        0040: 3300 6100 6600 3400 2d00 3000 3000 3000   3.a.f.4.-.0.0.0.
        0050: 3000 3000 3000 3000 3000 0000 0000 0000   0.0.0.0.0.......
        0060: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0070: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0080: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0090: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00a0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00b0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00c0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00d0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00e0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00f0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0100: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0110: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0120: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0130: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0140: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0150: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0160: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0170: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0180: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0190: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01a0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01b0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01c0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01d0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01e0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01f0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0200: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0210: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0220: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0230: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0240: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0250: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0260: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0270: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0280: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0290: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02a0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02b0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02c0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02d0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02e0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02f0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0300: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0310: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0320: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0330: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0340: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0350: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0360: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0370: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0380: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0390: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03a0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03b0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03c0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03d0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03e0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03f0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
Microsoft device response to control message 1, CMD 0xfe:
        0000: 2800 0000 0001 0400 0100 0000 0000 0000   (...............
        0010: 0001 4d54 5000 0000 0000 0000 0000 0000   ..MTP...........
        0020: 0000 0000 0000 0000 6400 3000 3100 3800   ........d.0.1.8.
        0030: 3000 3400 3700 2d00 3600 6300 3000 3000   0.4.7.-.6.c.0.0.
        0040: 3300 6100 6600 3400 2d00 3000 3000 3000   3.a.f.4.-.0.0.0.
        0050: 3000 3000 3000 3000 3000 0000 0000 0000   0.0.0.0.0.......
        0060: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0070: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0080: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0090: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00a0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00b0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00c0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00d0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00e0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        00f0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0100: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0110: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0120: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0130: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0140: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0150: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0160: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0170: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0180: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0190: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01a0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01b0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01c0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01d0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01e0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        01f0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0200: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0210: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0220: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0230: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0240: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0250: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0260: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0270: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0280: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0290: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02a0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02b0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02c0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02d0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02e0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        02f0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0300: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0310: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0320: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0330: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0340: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0350: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0360: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0370: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0380: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        0390: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03a0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03b0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03c0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03d0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03e0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
        03f0: 0000 0000 0000 0000 0000 0000 0000 0000   ................
Potential MTP Device with VendorID:0781 and ProductID:7450 responded to
control message 2 with a response that was too short. Problems may arrise
but continuing
Device info:
   Manufacturer: SanDisk
   Model: Sansa c250
   Device version: Sansa 01.01.06P
   Serial number: 4453033f-32305453-5d018047-6c003af4-00000000
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com/WMDRMPD: 10.1
Supported operations:
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   101b: Get partial object
   100c: Send object info
   100d: Send object
   100b: Delete object
   1012: Set object protection
   100f: Format storage
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9810: Get object references
   9811: Set object references
   9201: Report Added/Deleted Items
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
Events supported:
   0x4004
   0x4005
Device Properties Supported:
   0x5001: Battery Level
   0xd101: Secure Time
   0xd102: Device Certificate
   0xd401: Synchronization Partner
   0xd402: Device Friendly Name
Playable File (Object) Types and Object Properties Supported:
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type GET/SET
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type GET/SET
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 1500000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 85, 353, 384, 41222, 304, 1,  READ ONLY
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3, GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 2147483000, STEP 1000 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
   300c: ASF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 1500000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 85, 353, 384, 41222, 304, 1,  READ ONLY
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3, GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 2147483000, STEP 1000 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
   300a: MS AVI
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 1500000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 85, 353, 384, 41222, 304, 1,  READ ONLY
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3, GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 2147483000, STEP 1000 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
   3801: JPEG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 220, STEP 1 READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 176, STEP 1 READ ONLY
   3804: BMP
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 220, STEP 1 READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 176, STEP 1 READ ONLY
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type GET/SET
   ba03: Abstract Audio Album
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,  READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 220, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 176, STEP 1 READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 77440, STEP 10 READ ONLY
      dc8c: Genre STRING data type GET/SET
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 1500000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 85, 353, 384, 41222, 304, 1,  READ ONLY
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3, GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 2147483000, STEP 1000 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 2020982464
      FreeSpaceInBytes: 38256320
      FreeSpaceInObjects: 4294967295
      StorageDescription: Internal Memory
      VolumeIdentifier: VOL0_Sansa_c250_4453033f-32305453-5d018047-6c003af4-00000000
Special directories:
   Default music folder: 0x00000000
   Default playlist folder: 0x00000000
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: Sansa c250
   Synchronization partner: {00000000-0000-0000-0000-000000000000}
   Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Advanced Systems Format
   Audio Video Interleave
   JPEG file
   BMP bitmap file
   Microsoft Windows Media Audio

Secure Time:
<DRMCLOCK type="status"><VALUE>#20070815
03:00:27Z#</VALUE><FLAG>DRM_CLK_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID
private="1">PwNTRFNUMDJHgAFd9DoAbAAAAAA=</UNIQUEID><PUBLICKEY
private="1">vPNbgTRkxhEafnVrob5Lhat/CwsPKt54wmrxiNGfm1zaE1U/NtuVhw==</PUBLICKEY><KEYDATA>TtFnh7U7Pg8/oY3RRMgz7f5WDZ0=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>/UKEp4NFuqncbVnodwNEpg7tB4QzxEX5uBEGPUwTrzyiERNERrqEQw==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>77sImUOi0amd9wYBbRcZ7JElZgw=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.106.11</SECURITYVERSION><CERTIFICATE
private="1">vPNbgTRkxhEafnVrob5Lhat/CwsPKt54wmrxiNGfm1zaE1U/NtuVhwIEagup8abeALgJznwoPSv6U/eE0zueQYwkMKo56CY5WzuWg1ZFk0oIyi0O</CERTIFICATE></FALLBACK><CERTIFICATE
type="GROUP"><DATA><NAME>Sansa C200</NAME>
    <MANUFACTURER>Micro-Star</MANUFACTURER>
    <MAKE>MSI</MAKE>
    <DISTRIBUTOR>Micro-Star Int’l Co Ltd</DISTRIBUTOR>
    <MODEL>SanDisk Sansa Series</MODEL>
    <SECURITYLEVEL>2000</SECURITYLEVEL>
    <HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
    <HARDWARE_VER_MINOR>1</HARDWARE_VER_MINOR>
    <FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR>
    <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
    <FEATURES>
        <CLOCK>2</CLOCK>
          <SECURECLOCK>
                <URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
                <PUBLICKEY>
!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==
</PUBLICKEY>
          </SECURECLOCK>
        <METERING>1</METERING>
        <LICENSE_ACQ>1</LICENSE_ACQ>
        <LICENSE_SYNC>1</LICENSE_SYNC>
        <ENCRYPTION>1</ENCRYPTION>
  <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
    </FEATURES>
    <LIMITS>
        <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
        <MAXLICENSESIZE>10240</MAXLICENSESIZE>
        <MAXHEADERSIZE>5120</MAXHEADERSIZE>
   
</LIMITS><PUBLICKEY>dif5mSOYklFEWQW8Rk6I2+ugeFhuLpr7A+dBU3qH5sBoSXXuhYCgaQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>yszNKX0icRq05GWdgw2JODKILnIFvegA2rf6oWgBRJeCaLqCa7bNLw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>1391</AUTH_ID><PUBLICKEY>4c2hgvX/sgV7OjJu82BQ9by7lxh2r6XZOOG0qx8QLa7h4AiO0JOVhQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>hreAI4Q0sKU6t+K+phUFHtjf0hjgSJguTc9R5XmzRu9hflAuTr4xZQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>8q56WrXAXSViV/Birc27ZR5APyMzCijSV8+pXdpi0B+66ctdri+Tcw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
WMPInfo.xml Does not exist on this device
PTP: Closing session
Clearing stall on IN endpoint
Clearing stall on OUT endpoint
OK.


libmtp version: 0.1.5

Attempting to connect device(s)
Detect: Successfully connected 1 devices
USB low-level info:
  Using kernel interface "usbfs"
  bcdUSB: 512
  bDeviceClass: 0
  bDeviceSubClass: 0
  bDeviceProtocol: 0
  idVendor: 0781
  idProduct: 7450
  IN endpoint maxpacket: 512 bytes
  OUT endpoint maxpacket: 512 bytes
  Device flags: 0x00000002
Device info:
  Manufacturer: SanDisk
  Model: Sansa c240
  Device version: Sansa 01.01.00F
  Serial number: 4453033f-31305453-b7108047-6b00887a-00000000
  Vendor extension ID: 0x00000006
  Vendor extension description: microsoft.com/WMDRMPD: 10.1
Supported operations:
  1014: Get device property description
  1015: Get device property value
  1016: Set device property value
  1017: Reset device property value
  1001: get device info
  1002: Open session
  1003: Close session
  1004: Get storage IDs
  1005: Get storage info
  1006: Get number of objects
  1007: Get object handles
  1008: Get object info
  1009: Get object
  101b: Get partial object
  100c: Send object info
  100d: Send object
  100b: Delete object
  1012: Set object protection
  100f: Format storage
  9801: Get object properties supported
  9802: Get object property description
  9803: Get object property value
  9804: Set object property value
  9805: Get object property list
  9806: Set object property list
  9810: Get object references
  9811: Set object references
  9201: Report Added/Deleted Items
  9101: Get secure time challenge
  9102: Get secure time response
  9103: Set license response
  9104: Get sync list
  9105: Send meter challenge query
  9106: Get meter challenge
  9107: Get meter response
  9108: Clean data store
  9109: Get license state
  910a: Send WMDRM-PD Command
  910b: Send WMDRM-PD Request
Events supported:
  0x4004
  0x4005
Device Properties Supported:
  0x5001: Battery Level
  0xd101: Secure Time
  0xd102: Device Certificate
  0xd401: Synchronization Partner
  0xd402: Device Friendly Name
Playable File (Object) Types and Object Properties Supported:
  3001: Association/Directory
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc09: DateModified STRING data type GET/SET
  3000: Undefined Type
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc09: DateModified STRING data type GET/SET
  3009: MP3
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc09: DateModified STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 50 READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 1500000, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 85, 353, 384, 41222, 304, 1,  READ ONLY
     de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 2147483000, STEP 1000 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
  300c: ASF
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc09: DateModified STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 50 READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 1500000, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 85, 353, 384, 41222, 304, 1,  READ ONLY
     de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 2147483000, STEP 1000 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
  300a: MS AVI
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc09: DateModified STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 50 READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 1500000, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 85, 353, 384, 41222, 304, 1,  READ ONLY
     de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 2147483000, STEP 1000 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
  3801: JPEG
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc09: DateModified STRING data type GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc88: Height UINT32 data type range: MIN 0, MAX 220, STEP 1 READ ONLY
     dc87: Width UINT32 data type range: MIN 0, MAX 176, STEP 1 READ ONLY
  3804: BMP
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc09: DateModified STRING data type GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc88: Height UINT32 data type range: MIN 0, MAX 220, STEP 1 READ ONLY
     dc87: Width UINT32 data type range: MIN 0, MAX 176, STEP 1 READ ONLY
  ba05: Abstract Audio Video Playlist
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc09: DateModified STRING data type GET/SET
  ba03: Abstract Audio Album
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc09: DateModified STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,  READ ONLY
     dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
     dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 220, STEP 1 READ ONLY
     dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 176, STEP 1 READ ONLY
     dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 77440, STEP 10 READ ONLY
     dc8c: Genre STRING data type GET/SET
  b901: WMA
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc09: DateModified STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 50 READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 1500000, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 85, 353, 384, 41222, 304, 1,  READ ONLY
     de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 2147483000, STEP 1000 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
Storage Devices:
  StorageID: 0x00010001
     StorageType: 0x0003
     FilesystemType: 0x0002
     AccessCapability: 0x0000
     MaxCapacity: 997986120
     FreeSpaceInBytes: 9183048
     FreeSpaceInObjects: 4294967295
     StorageDescription: Internal Memory
     VolumeIdentifier: VOL0_Sansa_c240_4453033f-31305453-b7108047-6b00887a-00000000
Special directories:
  Default music folder: 0x00000001
  Default playlist folder: 0x00000003
  Default picture folder: 0x00000000
  Default video folder: 0x00000000
  Default organizer folder: 0x00000000
  Default zencast folder: 0x00000000
  Default album folder: 0x00000000
  Default text folder: 0x00000000
MTP-specific device properties:
  Friendly name: Sansa c240
  Synchronization partner: {00000000-0000-0000-0000-000000000000}
  Battery level 43 of 100 (43%)
libmtp supported (playable) filetypes:
  ISO MPEG-1 Audio Layer 3
  Microsoft Advanced Systems Format
  Audio Video Interleave
  JPEG file
  BMP bitmap file
  Microsoft Windows Media Audio

Secure Time:
<DRMCLOCK type="status"><VALUE>#20070508 22:48:36Z#</VALUE><FLAG>DRM_CLK_NEEDS_REFRESH</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">PwNTRFNUMDFHgBC3eogAawAAAAA=</UNIQUEID><PUBLICKEY private="1">uI9WF1l30WJuj1nCxrs0UaCtW1huJFSMaCNzRt1vrt0R9fP6mLEOBw==</PUBLICKEY><KEYDATA>LsWFcvmzrRqyDsz21nhG87LMqcc=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>qJ5Gp94Y0TYos4cxOIs0XHJSo2w0OQv+iRWqLf357ZJfxVQUeNGAaA==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>NJ7ml0xXGldHdBl518raEMWbtTM=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.106.11</SECURITYVERSION><CERTIFICATE private="1">uI9WF1l30WJuj1nCxrs0UaCtW1huJFSMaCNzRt1vrt0R9fP6mLEOBwIEagt5JFtwO/GzWFl9QJHGCmMcwbCWB83G3TZ7dk6icJXHX9+QqLym0ANS</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>Sansa C200</NAME>
   <MANUFACTURER>Micro-Star</MANUFACTURER>
   <MAKE>MSI</MAKE>
   <DISTRIBUTOR>Micro-Star Int’l Co Ltd</DISTRIBUTOR>
   <MODEL>SanDisk Sansa Series</MODEL>
   <SECURITYLEVEL>2000</SECURITYLEVEL>
   <HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
   <HARDWARE_VER_MINOR>1</HARDWARE_VER_MINOR>
   <FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR>
   <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
   <FEATURES>
       <CLOCK>2</CLOCK>
         <SECURECLOCK>
               <URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
               <PUBLICKEY>
!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==
</PUBLICKEY>
         </SECURECLOCK>
       <METERING>1</METERING>
       <LICENSE_ACQ>1</LICENSE_ACQ>
       <LICENSE_SYNC>1</LICENSE_SYNC>
       <ENCRYPTION>1</ENCRYPTION>
 <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
   </FEATURES>
   <LIMITS>
       <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
       <MAXLICENSESIZE>10240</MAXLICENSESIZE>
       <MAXHEADERSIZE>5120</MAXHEADERSIZE>
   </LIMITS><PUBLICKEY>dif5mSOYklFEWQW8Rk6I2+ugeFhuLpr7A+dBU3qH5sBoSXXuhYCgaQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>yszNKX0icRq05GWdgw2JODKILnIFvegA2rf6oWgBRJeCaLqCa7bNLw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>1391</AUTH_ID><PUBLICKEY>4c2hgvX/sgV7OjJu82BQ9by7lxh2r6XZOOG0qx8QLa7h4AiO0JOVhQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>hreAI4Q0sKU6t+K+phUFHtjf0hjgSJguTc9R5XmzRu9hflAuTr4xZQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>8q56WrXAXSViV/Birc27ZR5APyMzCijSV8+pXdpi0B+66ctdri+Tcw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
WMPInfo.xml Does not exist on this device
OK.
