$ examples/detect
libmtp version: 0.2.2

Attempting to connect device(s)
PTP: Opening session
PTP_ERROR_IO: Trying again after re-initializing USB interface
PTP: Opening session
Detect: Successfully connected 1 devices
USB low-level info:
  Using kernel interface "usbfs"
  bcdUSB: 512
  bDeviceClass: 0
  bDeviceSubClass: 0
  bDeviceProtocol: 0
  idVendor: 04e8
  idProduct: 6734
  IN endpoint maxpacket: 512 bytes
  OUT endpoint maxpacket: 512 bytes
  Device flags: 0x00000002
Microsoft device descriptor 0xee:
       0000: 1203 4d00 5300 4600 5400 3100 3000 3000   ..M.S.F.T.1.0.0.
       0010: 0100                                      ..
Device info:
  Manufacturer: Samsung Electronics Co.
  Model: Samsung Juke
  Device version:
  Serial number: B4744780000000000000000000000000
  Vendor extension ID: 0x00000006
  Vendor extension description: microsoft.com/WMDRMPD: 10.1;
  Detected object size: 64 bits
Supported operations:
  1001: get device info
  1002: Open session
  1003: Close session
  1004: Get storage IDs
  1005: Get storage info
  1006: Get number of objects
  1007: Get object handles
  1008: Get object info
  1009: Get object
  100b: Delete object
  100c: Send object info
  100d: Send object
  100f: Format storage
  1010: Reset device
  1014: Get device property description
  1015: Get device property value
  1016: Set device property value
  9810: Get object references
  9811: Set object references
  9802: Get object property description
  9801: Get object properties supported
  9803: Get object property value
  9804: Set object property value
  9805: Get object property list
  9806: Set object property list
  101b: Get partial object
  9201: Report Added/Deleted Items
  9101: Get secure time challenge
  9102: Get secure time response
  9103: Set license response
  9104: Get sync list
  9105: Send meter challenge query
  9106: Get meter challenge
  9107: Get meter response
  9108: Clean data store
  9109: Get license state
  910a: Send WMDRM-PD Command
  910b: Send WMDRM-PD Request
Events supported:
  0x4004
  0x4005
Device Properties Supported:
  0x5001: Battery Level
  0xd401: Synchronization Partner
  0xd402: Friendly Device Name
  0xd101: Secure Time
  0xd102: Device Certificate
  0xd103: Revocation Info
Playable File (Object) Types and Object Properties Supported:
  3001: Association/Directory
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc9a: AlbumName STRING data type GET/SET
  3009: MP3
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     dc96: Composer STRING data type GET/SET
  b901: WMA
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 320000, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     dc96: Composer STRING data type GET/SET
  b903: AAC
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     dc96: Composer STRING data type GET/SET
  3801: JPEG
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc87: Width UINT32 data type range: MIN 1, MAX 320, STEP 1 GET/SET
     dc88: Height UINT32 data type range: MIN 1, MAX 240, STEP 1 GET/SET
  300c: ASF
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc87: Width UINT32 data type range: MIN 1, MAX 320, STEP 1 GET/SET
     dc88: Height UINT32 data type range: MIN 1, MAX 240, STEP 1 GET/SET
     de97: ScanDepth UINT16 data type enumeration: 1,  READ ONLY
     de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
     de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 1195724877, 861293911,  GET/SET
     de9e: KeyFrameDistance UINT32 data type range: MIN 1000, MAX 10000, STEP 1 GET/SET
     de9c: VideoBitRate UINT32 data type range: MIN 32768, MAX 768000, STEP 1 GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     dea1: EncodingProfile STRING data type GET/SET
  3001: Association/Directory
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc9a: AlbumName STRING data type GET/SET
  ba05: Abstract Audio Video Playlist
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
  3000: Undefined Type
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
  b802: Firmware
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
  ba03: Abstract Audio Album
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
Unknown OPFF type 6
     dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, READ ONLY
     dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
     dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
     dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
     dc9b: AlbumArtist STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
Storage Devices:
  StorageID: 0x00010001
     StorageType: 0x0003
     FilesystemType: 0x0002
     AccessCapability: 0x0000
     MaxCapacity: 2012217344
     FreeSpaceInBytes: 1398882304
     FreeSpaceInObjects: 2908
     StorageDescription: Internal Storage
     VolumeIdentifier: B4744780000000000000000000000000
Special directories:
  Default music folder: 0x20000003
  Default playlist folder: 0x20000004
  Default picture folder: 0x00000000
  Default video folder: 0x00000000
  Default organizer folder: 0x00000000
  Default zencast folder: 0x00000000
  Default album folder: 0x00000000
  Default text folder: 0x00000000
MTP-specific device properties:
  Friendly name: Samsung Juke
  Synchronization partner: Longhorn Sync Engine
  Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
  ISO MPEG-1 Audio Layer 3
  Microsoft Windows Media Audio
  Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
  JPEG file
  Microsoft Advanced Systems Format
  Firmware file

Secure Time:
<DRMCLOCK type="status"><VALUE>#20071101
02:46:56Z#</VALUE><FLAG>DRM_CLK_NEEDS_REFRESH</FLAG></DRMCLOCK>AG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID
private="1">tHRHgAAAAAAAAAAAAAAAAAAAAAA=</UNIQUEID><PUBLICKEY
private="1">TAgc/2jPXxLq/gHJRijomE0mwTnQhOd/PEUo1DLuQzEAty76lYBTYg==</PUBLICKEY><KEYDATA>XuBkAeQgg2A8GdHVO/lUyVbQLww=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>owp1zrBHh7eMEs/uJQ9C/ppEdCExtOK9B0vOjwe0sEcKkxRgELMpbA==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>8OHgXjFSSbjrS/lMIosgZfZU5j4=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.108.219</SECURITYVERSION><CERTIFICATE
private="1">TAgc/2jPXxLq/gHJRijomE0mwTnQhOd/PEUo1DLuQzEAty76lYBTYgIEbNskkonvYMMgJmc0XbA/vcj2O1bjC0QrZdxTNhedz9B5Pu2XhVmVd3Yi</CERTIFICATE></FALLBACK><CERTIFICATE
type="GROUP"><DATA><NAME>SCH-U470</NAME><MANUFACTURER>Samsung
Elec.</MANUFACTURER><MAKE>Samsung Elec.</MAKE><DISTRIBUTOR>Samsung
Elec.</DISTRIBUTOR><MODEL>SCH-U470</MODEL><SECURITYLEVEL>2000</SECURITYLEVEL><HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR><HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR><FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR><FIRMWARE_VER_MINOR>1</FIRMWARE_VER_MINOR><FEATURES><CLOCK>2</CLOCK><SECURECLOCK><URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL><PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY></SECURECLOCK><METERING>1</METERING><LICENSE_ACQ>0</LICENSE_ACQ><LICENSE_SYNC>1</LICENSE_SYNC><ENCRYPTION>0</ENCRYPTION><SYMMETRIC_OPT>1</SYMMETRIC_OPT><SUPPORT_REVOCATION><GUID>{CD75E604-543D-4A9C-9F09-FE6D24E8BF90}</GUID></SUPPORT_REVOCATION></FEATURES><LIMITS><MAXCHAINDEPTH>2</MAXCHAINDEPTH><MAXLICENSESIZE>10240</MAXLICENSESIZE><MAXHEADERSIZE>5120</MAXHEADERSIZE></LIMITS><PUBLICKEY>a/H0OaFHmUy8tvBU+lBAn0g/2SX5aBzazaysIjC+fJyH+KZyI/2KEQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>u0EXC4fOhglw5n4sOlS3Y2jtD0MPP0MpMEZm1PjEjxcyodTfxyOrQQ==</MSDRM_SIGNATURE_VALUE></CERT
 IFICATE><CERTIFICATE
type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>2111</AUTH_ID><PUBLICKEY>uk8RAuRderOsSQOiiL+cwyuTvi3jyu7fauvsiLVbwkSI3B1XWbzsMQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>7Uz/2vA+NynmkNrdMbHu770r0GS8/3/we4G5D5x7gDJ4ckMu/onpRA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>Xer3lXCg0TbG0D4ibUEiNLaE8Ah5l4o8QgYEIzJohL+EnCVhHh42gA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
WMPInfo.xml Does not exist on this device
PTP: Closing session
inep: usb_get_endpoint_status(): Connection timed out
outep: usb_get_endpoint_status(): Connection timed out
usb_clear_halt() on IN endpoint: Connection timed out
usb_clear_halt() on OUT endpoint: Connection timed out
usb_clear_halt() on INTERRUPT endpoint: Connection timed out
OK.
