Device 0 (VID=0fca and PID=8007) is a RIM BlackBerry Storm.
libmtp version: 1.0.2

Listing raw device(s)
   Found 1 device(s):
   RIM: BlackBerry Storm (0fca:8007) @ bus 1, dev 9
Attempting to connect device(s)
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0fca
   idProduct: 8007
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 1
      Device number: 9
      Device entry info:
         Vendor: RIM
         Vendor id: 0x0fca
         Product: BlackBerry Storm
         Vendor id: 0x8007
         Device flags: 0x04000003
Configuration 0, interface 1, altsetting 0:
   Interface description contains the string "MTP"
   Device recognized as MTP, no further probing.
Device info:
   Manufacturer: Research In Motion
   Model: 9650
   Device version: 5.0.0.621
   Serial number: 00000000-32155fab-a000001ce236a0
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMPPD: 11.0; microsoft.com/WMDRMPD: 10.1;
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   101b: Get partial object
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9201: Report Added/Deleted Items
   9202: Report Acquired Items
   9810: Get object references
   9811: Set object references
   9101: Get secure time challenge
   9104: Get sync list
   9106: Get meter challenge
   9108: Clean data store
   9102: Get secure time response
   9103: Set license response
   9105: Send meter challenge query
   9107: Get meter response
   9109: Get license state
Events supported:
   0x4001
   0x4004
   0x4005
   0x4008
Device Properties Supported:
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd102: Device Certificate
   0xd404: Unknown property
Playable File (Object) Types and Object Properties Supported:
   b984: 3GP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 17, 352, 353, 354, 355, 85, 41222, 28781, 255, 31265, 6, 7, 49, 80,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1536000, STEP 1 READ ONLY
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 360, STEP 1 GET/SET
      de97: Scan Depth UINT16 data type range: MIN 0, MAX 1, STEP 2 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911, 859189832, 875967048, 1395937357,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 2000000, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  READ ONLY
      db02: Unknown property array of UINT8 data type byte array:  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   3009: MP3
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 17, 352, 353, 354, 355, 85, 41222, 28781, 255, 31265, 6, 7, 49, 80,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1536000, STEP 1 READ ONLY
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  READ ONLY
      db02: Unknown property array of UINT8 data type byte array:  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   b901: WMA
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 17, 352, 353, 354, 355, 85, 41222, 28781, 255, 31265, 6, 7, 49, 80,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1536000, STEP 1 READ ONLY
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  READ ONLY
      db02: Unknown property array of UINT8 data type byte array:  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   3008: MS Wave
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 17, 352, 353, 354, 355, 85, 41222, 28781, 255, 31265, 6, 7, 49, 80,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1536000, STEP 1 READ ONLY
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  READ ONLY
      db02: Unknown property array of UINT8 data type byte array:  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   b900: Undefined Audio
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 17, 352, 353, 354, 355, 85, 41222, 28781, 255, 31265, 6, 7, 49, 80,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1536000, STEP 1 READ ONLY
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  READ ONLY
      db02: Unknown property array of UINT8 data type byte array:  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   b904: Audible.com Codec
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 17, 352, 353, 354, 355, 85, 41222, 28781, 255, 31265, 6, 7, 49, 80,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1536000, STEP 1 READ ONLY
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  READ ONLY
      db02: Unknown property array of UINT8 data type byte array:  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   b906: FLAC
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 17, 352, 353, 354, 355, 85, 41222, 28781, 255, 31265, 6, 7, 49, 80,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1536000, STEP 1 READ ONLY
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  READ ONLY
      db02: Unknown property array of UINT8 data type byte array:  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   b903: AAC
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 17, 352, 353, 354, 355, 85, 41222, 28781, 255, 31265, 6, 7, 49, 80,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1536000, STEP 1 READ ONLY
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  READ ONLY
      db02: Unknown property array of UINT8 data type byte array:  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   ba03: Abstract Audio Album
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14344, 14347, 14340,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 500, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 500, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  READ ONLY
   ba09: Abstract Audio Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  READ ONLY
   ba10: WPL Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  READ ONLY
   ba11: M3U Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  READ ONLY
   ba82: XMLDocument
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  READ ONLY
   3000: Undefined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  READ ONLY
   3001: Association/Directory
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  READ ONLY
   3801: JPEG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 4992, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 3328, STEP 1 GET/SET
      dcd3: Image Bit Depth UINT32 data type range: MIN 0, MAX 32, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   380b: PNG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 4992, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 3328, STEP 1 GET/SET
      dcd3: Image Bit Depth UINT32 data type range: MIN 0, MAX 32, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   3807: GIF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 4992, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 3328, STEP 1 GET/SET
      dcd3: Image Bit Depth UINT32 data type range: MIN 0, MAX 32, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   3804: BMP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 4992, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 3328, STEP 1 GET/SET
      dcd3: Image Bit Depth UINT32 data type range: MIN 0, MAX 32, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   3800: Defined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 4992, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 3328, STEP 1 GET/SET
      dcd3: Image Bit Depth UINT32 data type range: MIN 0, MAX 32, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   380d: TIFF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 4992, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 3328, STEP 1 GET/SET
      dcd3: Image Bit Depth UINT32 data type range: MIN 0, MAX 32, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   b980: Undefined Video
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 17, 352, 353, 354, 355, 85, 41222, 28781, 255, 31265, 6, 7, 49, 80,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1536000, STEP 1 READ ONLY
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      dc8c: Genre STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 360, STEP 1 GET/SET
      de97: Scan Depth UINT16 data type range: MIN 0, MAX 1, STEP 2 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911, 859189832, 875967048, 1395937357,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 2000000, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dea1: Encoding Profile STRING data type READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 30000, STEP 1 READ ONLY
      de9e: Key Frame Distance UINT32 data type range: MIN 0, MAX 300, STEP 1 READ ONLY
   300a: MS AVI
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 17, 352, 353, 354, 355, 85, 41222, 28781, 255, 31265, 6, 7, 49, 80,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1536000, STEP 1 READ ONLY
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      dc8c: Genre STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 360, STEP 1 GET/SET
      de97: Scan Depth UINT16 data type range: MIN 0, MAX 1, STEP 2 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911, 859189832, 875967048, 1395937357,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 2000000, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dea1: Encoding Profile STRING data type READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 30000, STEP 1 READ ONLY
      de9e: Key Frame Distance UINT32 data type range: MIN 0, MAX 300, STEP 1 READ ONLY
   b981: WMV
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 17, 352, 353, 354, 355, 85, 41222, 28781, 255, 31265, 6, 7, 49, 80,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1536000, STEP 1 READ ONLY
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      dc8c: Genre STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      de97: Scan Depth UINT16 data type range: MIN 0, MAX 1, STEP 2 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911, 859189832, 875967048, 1395937357,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 384000, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dea1: Encoding Profile STRING data type READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 30000, STEP 1 READ ONLY
      de9e: Key Frame Distance UINT32 data type range: MIN 0, MAX 300, STEP 1 READ ONLY
   300b: MPEG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 17, 352, 353, 354, 355, 85, 41222, 28781, 255, 31265, 6, 7, 49, 80,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1536000, STEP 1 READ ONLY
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      dc8c: Genre STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 360, STEP 1 GET/SET
      de97: Scan Depth UINT16 data type range: MIN 0, MAX 1, STEP 2 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911, 859189832, 875967048, 1395937357,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 2000000, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dea1: Encoding Profile STRING data type READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 30000, STEP 1 READ ONLY
      de9e: Key Frame Distance UINT32 data type range: MIN 0, MAX 300, STEP 1 READ ONLY
   300c: ASF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 17, 352, 353, 354, 355, 85, 41222, 28781, 255, 31265, 6, 7, 49, 80,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1536000, STEP 1 READ ONLY
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      dc8c: Genre STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 360, STEP 1 GET/SET
      de97: Scan Depth UINT16 data type range: MIN 0, MAX 1, STEP 2 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911, 859189832, 875967048, 1395937357,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 2000000, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dea1: Encoding Profile STRING data type READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 30000, STEP 1 READ ONLY
      de9e: Key Frame Distance UINT32 data type range: MIN 0, MAX 300, STEP 1 READ ONLY
   ba13: ASX Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 17, 352, 353, 354, 355, 85, 41222, 28781, 255, 31265, 6, 7, 49, 80,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1536000, STEP 1 READ ONLY
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      dc8c: Genre STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 360, STEP 1 GET/SET
      de97: Scan Depth UINT16 data type range: MIN 0, MAX 1, STEP 2 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911, 859189832, 875967048, 1395937357,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 2000000, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dea1: Encoding Profile STRING data type READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 30000, STEP 1 READ ONLY
      de9e: Key Frame Distance UINT32 data type range: MIN 0, MAX 300, STEP 1 READ ONLY
   b982: MP4
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 17, 352, 353, 354, 355, 85, 41222, 28781, 255, 31265, 6, 7, 49, 80,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1536000, STEP 1 READ ONLY
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 360, STEP 1 GET/SET
      de97: Scan Depth UINT16 data type range: MIN 0, MAX 1, STEP 2 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911, 859189832, 875967048, 1395937357,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 2000000, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  READ ONLY
      db02: Unknown property array of UINT8 data type byte array:  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   3002: Script
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  READ ONLY
   3005: HTML
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  READ ONLY
   ba80: Undefined Document
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  READ ONLY
   ba83: Microsoft Word Document
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  READ ONLY
   ba85: Microsoft Excel Spreadsheet (.xls)
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  READ ONLY
   ba86: Microsoft Powerpoint (.ppt)
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  READ ONLY
   3004: Text
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  READ ONLY
Storage Devices:
   StorageID: 0x00020001
      StorageType: 0x0004 removable RAM storage
      FilesystemType: 0x0001 generic flat filesystem
      AccessCapability: 0x0000 read/write
      MaxCapacity: 1966800896
      FreeSpaceInBytes: 1571815424
      FreeSpaceInObjects: 0
      StorageDescription: Media Card
      VolumeIdentifier: 20001-32155fab-a000001ce236a0
Special directories:
   Default music folder: 0x00200007
   Default playlist folder: 0xffffffff
   Default picture folder: 0x00200004
   Default video folder: 0xffffffff
   Default organizer folder: 0xffffffff
   Default zencast folder: 0xffffffff
   Default album folder: 0xffffffff
   Default text folder: 0xffffffff
MTP-specific device properties:
   Friendly name: BlackBerry 9650
   Synchronization partner: 32155fab
   Battery level 3 of 100 (2%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   RIFF WAVE file
   Undefined audio file
   Audible.com Audio Codec
   Free Lossless Audio Codec (FLAC)
   Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
   Abstract Album file
   Abstract Playlist file
   XML file
   JPEG file
   Portable Network Graphics
   GIF bitmap file
   BMP bitmap file
   TIFF bitmap file
   Undefined video file
   Audio Video Interleave
   Microsoft Windows Media Video
   MPEG video stream
   Microsoft Advanced Systems Format
   MPEG-4 Part 14 Container Format (Audio+Video Emphasis)
   HTML file
   DOC file
   XLS file
   PPT file
   Text file
OK.
