libmtp version: 1.0.1

Listing raw device(s)
   Found 1 device(s):
   RIM: BlackBerry Storm (0fca:8007) @ bus 0, dev 6
Attempting to connect device(s)
BlackBerry magic part 1:
	0000: 4000 0000 0001 0400 0200 0000 0000 0000	@...............
	0010: 0001 0000 0000 0000 0000 0000 0000 0000	................
	0020: 0000 0000 0000 0000 0101 4d54 5000 0000	..........MTP...
	0030: 0000 3400 0000 0000 0000 0000 0000 0000	..4.............
BlackBerry magic part 2:
	0000: 0200                                   	..
BlackBerry magic part 3:
	0000: 1100 0001 04                           	.....
BlackBerry magic part 4:
	0000: 1100 0001 0400 0102 0102 0202 0302 0303	................
	0010: 02                                     	.
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0fca
   idProduct: 8007
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 0
      Device number: 6
      Device entry info:
         Vendor: RIM
         Vendor id: 0x0fca
         Product: BlackBerry Storm
         Vendor id: 0x8007
         Device flags: 0x04000002
Configuration 0, interface 1, altsetting 0:
   Interface description contains the string "MTP"
   Device recognized as MTP, no further probing.
Device info:
   Manufacturer: Research In Motion
   Model: 9500
   Device version: 100
   Serial number: 00000000-********-**************
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 11.0; vodafone.com/omadrmv2: 1.0;
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100a: Get thumbnail
   100b: Delete object
   100c: Send object info
   100d: Send object
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   101b: Get partial object
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9201: Report Added/Deleted Items
   9202: Report Acquired Items
   9810: Get object references
   9811: Set object references
   9101: Get secure time challenge
   9104: Get sync list
   9106: Get meter challenge
   9108: Clean data store
   9102: Get secure time response
   9103: Set license response
   9105: Send meter challenge query
   9107: Get meter response
   9109: Get license state
Events supported:
   0x4001
   0x4004
   0x4005
   0x4008
Device Properties Supported:
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd102: Device Certificate
   0xd404: Unknown property
Playable File (Object) Types and Object Properties Supported:
   b984: 3GP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 352, 353, 85,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1500000, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      db02: Unknown property array of UINT8 data type byte array:  GET/SET
      db01: Unknown property UINT8 data type enumeration: 0, 1,  GET/SET
   3009: MP3
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 352, 353, 85,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1500000, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
   b901: WMA
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 352, 353, 85,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1500000, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
   3008: MS Wave
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   ba05: Abstract Audio Video Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   ba09: Abstract Audio Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   ba10: WPL Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   ba11: M3U Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   ba82: XMLDocument
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   3000: Undefined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     Error 2: PTP Layer error 02fe: get_device_unicode_property(): failed to get unicode property.
Error 2: (Look this up in ptp.h for an explanation.)
 dc09: Date Modified STRING data type DATETIME FORM READ ONLY
   3001: Association/Directory
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc06: Association Desc UINT32 data type ANY 32BIT VALUE form GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0001 generic flat filesystem
      AccessCapability: 0x0000 read/write
      MaxCapacity: 910098432
      FreeSpaceInBytes: 910098432
      FreeSpaceInObjects: 0
      StorageDescription: Mémoire terminal
      VolumeIdentifier: 10001-********-**************
   StorageID: 0x00020001
      StorageType: 0x0004 removable RAM storage
      FilesystemType: 0x0001 generic flat filesystem
      AccessCapability: 0x0000 read/write
      MaxCapacity: 7820148736
      FreeSpaceInBytes: 7820148736
      FreeSpaceInObjects: 0
      StorageDescription: Carte Média
      VolumeIdentifier: 20001-********-**************
Special directories:
   Default music folder: 0x00000000
   Default playlist folder: 0x00000000
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: (NULL)
   Synchronization partner: (NULL)
   Battery level 5 of 100 (5%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   RIFF WAVE file
   Abstract Playlist file
   XML file
Unable to acquire device certificate, perhaps this device does not support this
OK.
