Potential MTP Device with VendorID:0781 and ProductID:7460 responded to control message 2 with a response that was too short. Problems may arrise but continuing
PTP: Opening session
libmtp version: 0.1.5

Attempting to connect device(s)
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0781
   idProduct: 7460
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000007
Device info:
   Manufacturer: Sandisk
   Model: Sansa Express
   Device version: 01.00.15A2
   Serial number: 0002FA9380574D150002FA9380510D97
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 10.0; microsoft.com/WMPPD: 11.0; audible.com: 1.0
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   101b: Get partial object
   100b: Delete object
   100c: Send object info
   100d: Send object
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   100f: Format storage
   9810: Get object references
   9811: Set object references
   9201: Report Added/Deleted Items
   9202: Report Acquired Items
   9203: Get type of playlists that are allowed to be transfered
   97f1: Unknown(97f1)
   97f2: Unknown(97f2)
   97f3: Unknown(97f3)
   97f4: Unknown(97f4)
   1010: Reset device
Events supported:
   0x4004: Store added
   0x4005: Store removed
Device Properties Supported:
   0xd101: Secure Time
   0xd102: Device Certificate
   0xd402: Device Friendly Name
   0xd401: Synchronization Partner
   0x5001: Battery Level
   0xd405: Device Icon
   0xd100: Unknown property
Playable File (Object) Types and Object Properties Supported:
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 4300000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 80, 85,  READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
   3008: MS Wave
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 2304000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 17,  READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 352, 353,  READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
   300c: ASF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 352, 353,  READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 220, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 220, STEP 1 GET/SET
      dc09: DateModified STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 0, MAX 24050, STEP 1 GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 861293911,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 5000, MAX 385000, STEP 1 READ ONLY
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  READ ONLY
      dea1: EncodingProfile STRING data type GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
   3801: JPEG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc09: DateModified STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
   3807: GIF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc09: DateModified STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
   3804: BMP
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc09: DateModified STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
   ba03: Abstract Audio Album
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
   b904: Audible.com Codec
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0,  READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      da00: unknown(da00) UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8,  READ ONLY
      da02: unknown(da02) UINT32 data type ANY 32BIT VALUE form GET/SET
      da01: unknown(da01) STRING data type READ ONLY
      da03: unknown(da03) UINT16 data type enumeration: 0, 1,  GET/SET
      da04: unknown(da04) UINT128 data type READ ONLY
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 1023002624
      FreeSpaceInBytes: 132071424
      FreeSpaceInObjects: 4294967295
      StorageDescription: Internal Memory
      VolumeIdentifier: 0002FA9380574D150002FA9380510D97
Special directories:
   Default music folder: 0x00000066
   Default playlist folder: 0x00000000
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: Sansa Express
   Synchronization partner: Sansa Express
   Battery level 129 of 129 (100%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   RIFF WAVE file
   Microsoft Windows Media Audio
   Microsoft Advanced Systems Format
   JPEG file
   GIF bitmap file
   BMP bitmap file
   Audible.com Audio Codec
Unable to acquire device certificate, perhaps this device does not support this
WMPInfo.xml Does not exist on this device
OK.
