libmtp version: 1.0.6

Listing raw device(s)
Device 0 (VID=04e8 and PID=5130) is a Samsung YP-Q3.
  Found 1 device(s):
  Samsung: YP-Q3 (04e8:5130) @ bus 2, dev 13
Attempting to connect device(s)
USB low-level info:
  Using kernel interface "usbfs"
  bcdUSB: 512
  bDeviceClass: 0
  bDeviceSubClass: 0
  bDeviceProtocol: 0
  idVendor: 04e8
  idProduct: 5130
  IN endpoint maxpacket: 512 bytes
  OUT endpoint maxpacket: 512 bytes
  Raw device info:
     Bus location: 2
     Device number: 13
     Device entry info:
        Vendor: Samsung
        Vendor id: 0x04e8
        Product: YP-Q3
        Vendor id: 0x5130
        Device flags: 0x00001206
Microsoft device descriptor 0xee:
       0000: 1203 4d00 5300 4600 5400 3100 3000 3000   ..M.S.F.T.1.0.0.
       0010: 0100                                      ..
Device info:
  Manufacturer: SAMSUNG
  Model: Q3
  Device version:
  Serial number: 942C74A8B0A300000000000000000000
  Vendor extension ID: 0x00000006
  Vendor extension description: microsoft.com/WMPPD: 11.0;microsoft.com/WMDRMPD: 10.1;microsoft.com/WMPPD: 10.0;audible.com: 1.0;
  Detected object size: 64 bits
  Extensions:
       microsoft.com/WMPPD: 11.0
       microsoft.com/WMDRMPD: 10.1
       microsoft.com/WMPPD: 10.0
       audible.com: 1.0
Supported operations:
  1001: get device info
  1002: Open session
  1003: Close session
  1004: Get storage IDs
  1005: Get storage info
  1006: Get number of objects
  1007: Get object handles
  1008: Get object info
  1009: Get object
  100b: Delete object
  9808: Send object property list
  100c: Send object info
  100d: Send object
  100f: Format storage
  1010: Reset device
  1014: Get device property description
  1015: Get device property value
  1016: Set device property value
  9810: Get object references
  9811: Set object references
  9802: Get object property description
  9801: Get object properties supported
  9803: Get object property value
  9804: Set object property value
  9805: Get object property list
  9806: Set object property list
  101b: Get partial object
  9201: Report Added/Deleted Items
  9202: Report Acquired Items
  9101: Get secure time challenge
  9102: Get secure time response
  9103: Set license response
  9104: Get sync list
  9105: Send meter challenge query
  9106: Get meter challenge
  9107: Get meter response
  9108: Clean data store
  9109: Get license state
  910a: Send WMDRM-PD Command
  910b: Send WMDRM-PD Request
Events supported:
  0x4004
  0x4005
Device Properties Supported:
  0xd405: Device Icon
  0x5001: Battery Level
  0xd401: Synchronization Partner
  0xd402: Friendly Device Name
  0xd101: Secure Time
  0xd102: Device Certificate
  0xd103: Revocation Info
Playable File (Object) Types and Object Properties Supported:
  3001: Association/Directory
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc9a: Album Name STRING data type GET/SET
  3009: MP3
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
     de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: Audio Bit Rate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
     de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
     de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc99: Original Release Date STRING data type DATETIME FORM GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9a: Album Name STRING data type GET/SET
     dc9b: Album Artist STRING data type GET/SET
  b901: WMA
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
     de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 320000, STEP 1 READ ONLY
     de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
     de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc99: Original Release Date STRING data type DATETIME FORM GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9a: Album Name STRING data type GET/SET
     dc9b: Album Artist STRING data type GET/SET
  3008: MS Wave
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
     de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
     de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
     de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc99: Original Release Date STRING data type DATETIME FORM GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9a: Album Name STRING data type GET/SET
     dc9b: Album Artist STRING data type GET/SET
  3801: JPEG
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
     dc88: Height UINT32 data type range: MIN 1, MAX 272, STEP 1 GET/SET
  380b: PNG
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
     dc88: Height UINT32 data type range: MIN 1, MAX 272, STEP 1 GET/SET
  3804: BMP
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
     dc88: Height UINT32 data type range: MIN 1, MAX 272, STEP 1 GET/SET
  3807: GIF
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
     dc88: Height UINT32 data type range: MIN 1, MAX 272, STEP 1 GET/SET
  3004: Text
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
  300a: MS AVI
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
     dc88: Height UINT32 data type range: MIN 1, MAX 272, STEP 1 GET/SET
     de97: Scan Depth UINT16 data type enumeration: 1,  READ ONLY
     de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
     de9b: Video Four CC Codec UINT32 data type enumeration: 0, 1195724877, 861293911,  GET/SET
     de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
     de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 850000, STEP 1 GET/SET
     dc99: Original Release Date STRING data type DATETIME FORM GET/SET
     dc8c: Genre STRING data type GET/SET
     de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
     de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
     dea1: Encoding Profile STRING data type GET/SET
  300d: Apple Quicktime
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
  b981: WMV
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
     dc88: Height UINT32 data type range: MIN 1, MAX 272, STEP 1 GET/SET
     de97: Scan Depth UINT16 data type enumeration: 1,  READ ONLY
     de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
     de9b: Video Four CC Codec UINT32 data type enumeration: 0, 1195724877, 861293911,  GET/SET
     de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
     de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 850000, STEP 1 GET/SET
     dc99: Original Release Date STRING data type DATETIME FORM GET/SET
     dc8c: Genre STRING data type GET/SET
     de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 1956000, STEP 1 READ ONLY
     de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
     dea1: Encoding Profile STRING data type GET/SET
  b903: AAC
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
     de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
     de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
     de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc99: Original Release Date STRING data type DATETIME FORM GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9a: Album Name STRING data type GET/SET
     dc9b: Album Artist STRING data type GET/SET
  300c: ASF
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
     dc88: Height UINT32 data type range: MIN 1, MAX 272, STEP 1 GET/SET
     de97: Scan Depth UINT16 data type enumeration: 1,  READ ONLY
     de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
     de9b: Video Four CC Codec UINT32 data type enumeration: 0, 1195724877, 861293911,  GET/SET
     de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
     de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 850000, STEP 1 GET/SET
     dc99: Original Release Date STRING data type DATETIME FORM GET/SET
     dc8c: Genre STRING data type GET/SET
     de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
     de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
     dea1: Encoding Profile STRING data type GET/SET
  3001: Association/Directory
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc9a: Album Name STRING data type GET/SET
  ba05: Abstract Audio Video Playlist
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
  3000: Undefined Type
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
  b802: Firmware
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
  ba03: Abstract Audio Album
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
     dc81: Representative Sample Format UINT16 data type enumeration: 14337,  READ ONLY
     dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
     dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
     dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
     dc9b: Album Artist STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
  b900: Undefined Audio
     dc44: Name STRING data type GET/SET
     dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: Object Size UINT64 data type READ ONLY
     dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
     dc09: Date Modified STRING data type DATETIME FORM GET/SET
     dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
     dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
     d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
     de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
     de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
     de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc99: Original Release Date STRING data type DATETIME FORM GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9a: Album Name STRING data type GET/SET
     dc9b: Album Artist STRING data type GET/SET
Storage Devices:
  StorageID: 0x00010001
     StorageType: 0x0003 fixed RAM storage
     FilesystemType: 0x0002 generic hierarchical
     AccessCapability: 0x0000 read/write
     MaxCapacity: 7826251776
     FreeSpaceInBytes: 2626666496
     FreeSpaceInObjects: 15770
     StorageDescription: Internal Storage
     VolumeIdentifier: 942C74A8B0A300000000000000000000
Special directories:
  Default music folder: 0x20000005
  Default playlist folder: 0xffffffff
  Default picture folder: 0x20000006
  Default video folder: 0x20000009
  Default organizer folder: 0xffffffff
  Default zencast folder: 0xffffffff
  Default album folder: 0xffffffff
  Default text folder: 0x20000008
MTP-specific device properties:
  Friendly name: Q3
  Synchronization partner: Longhorn Sync Engine
  Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
  Folder
  ISO MPEG-1 Audio Layer 3
  Microsoft Windows Media Audio
  RIFF WAVE file
  JPEG file
  Portable Network Graphics
  BMP bitmap file
  GIF bitmap file
  Text file
  Audio Video Interleave
  Apple Quicktime container format
  Microsoft Windows Media Video
  Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
  Microsoft Advanced Systems Format
  Folder
  Abstract Playlist file
  Firmware file
  Abstract Album file
  Undefined audio file
  Ogg container format

Secure Time:
<DRMCLOCK type="status"><VALUE>#19702215 22:22:88Z#</VALUE><FLAG>DRM_CLK_NEEDS_REFRESH</FLAG></DRMCLOCK>AG></DRMCLOCK>
OK.
