libmtp version: 1.0.2

Listing raw device(s)
   Found 1 device(s):
   1e74:6512 @ bus 3, dev 2
Attempting to connect device(s)
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 255
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 1e74
   idProduct: 6512
   IN endpoint maxpacket: 64 bytes
   OUT endpoint maxpacket: 64 bytes
   Raw device info:
      Bus location: 3
      Device number: 2
      Device entry info:
         Vendor: (null)
         Vendor id: 0x1e74
         Product: (null)
         Vendor id: 0x6512
         Device flags: 0x00000000
Microsoft device descriptor 0xee:
	0000: 1203 4d00 5300 4600 5400 3100 3000 3000	..M.S.F.T.1.0.0.
	0010: fe00                                   	..
Microsoft device response to control message 1, CMD 0xfe:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Microsoft device response to control message 2, CMD 0xfe:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Device responds to control message 2 with some data.
Device info:
   Manufacturer: COBY
   Model: COBY MP705
   Device version: MTP-0.99-N-ENG
   Serial number: FD86FC402574A941ACEAA0FBBF953CE4
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 10.0;
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   101b: Get partial object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1010: Reset device
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   9810: Get object references
   9811: Set object references
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   9201: Report Added/Deleted Items
Events supported:
   None.
Device Properties Supported:
   0xd101: Secure Time
   0xd401: Synchronization Partner
   0x5001: Battery Level
   0xd102: Device Certificate
   0xd402: Friendly Device Name
Playable File (Object) Types and Object Properties Supported:
   3009: MP3
      dc44: Name STRING data type GET/SET
      dc04: Object Size UINT64 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 384000, STEP 1 READ ONLY
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
   b901: WMA
      dc44: Name STRING data type GET/SET
      dc04: Object Size UINT64 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 384000, STEP 1 READ ONLY
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
   300c: ASF
      dc44: Name STRING data type GET/SET
      dc04: Object Size UINT64 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      de97: Scan Depth UINT16 data type enumeration: 1,  READ ONLY
      de91: Total Bit Rate UINT32 data type range: MIN 1, MAX 1234000, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 384000, STEP 1 READ ONLY
      dc8c: Genre STRING data type GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      dc94: Parental Rating STRING data type GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 861293911, 0, 859189832, 958804552, 1195724877, 827739479, 844516695,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 850000, STEP 1 READ ONLY
   b981: WMV
      dc44: Name STRING data type GET/SET
      dc04: Object Size UINT64 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      de97: Scan Depth UINT16 data type enumeration: 1,  READ ONLY
      de91: Total Bit Rate UINT32 data type range: MIN 1, MAX 1234000, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 384000, STEP 1 READ ONLY
      dc8c: Genre STRING data type GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      dc94: Parental Rating STRING data type GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 861293911, 0, 859189832, 958804552, 1195724877, 827739479, 844516695,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 850000, STEP 1 READ ONLY
   3801: JPEG
      dc44: Name STRING data type GET/SET
      dc04: Object Size UINT64 data type READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
   3001: Association/Directory
      dc44: Name STRING data type GET/SET
      dc04: Object Size UINT64 data type READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
   ba03: Abstract Audio Album
      dc44: Name STRING data type GET/SET
      dc04: Object Size UINT64 data type READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 24576, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 180, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 180, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   ba05: Abstract Audio Video Playlist
      dc44: Name STRING data type GET/SET
      dc04: Object Size UINT64 data type READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
   3000: Undefined Type
      dc44: Name STRING data type GET/SET
      dc04: Object Size UINT64 data type READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
   300a: MS AVI
      dc44: Name STRING data type GET/SET
      dc04: Object Size UINT64 data type READ ONLY
      dc89: Duration UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc07: Object File Name STRING data type GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      de97: Scan Depth UINT16 data type enumeration: 1,  READ ONLY
      de91: Total Bit Rate UINT32 data type range: MIN 1, MAX 1234000, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 384000, STEP 1 READ ONLY
      dc8c: Genre STRING data type GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      dc94: Parental Rating STRING data type GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 861293911, 0, 859189832, 958804552, 1195724877, 827739479, 844516695,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 850000, STEP 1 READ ONLY
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 3984912384
      FreeSpaceInBytes: 2327183360
      FreeSpaceInObjects: 4294967295
      StorageDescription: internal storage
      VolumeIdentifier: FD86FC402574A941ACEA4AFBBF953CE4
Special directories:
   Default music folder: 0xffffffff
   Default playlist folder: 0xffffffff
   Default picture folder: 0xffffffff
   Default video folder: 0xffffffff
   Default organizer folder: 0xffffffff
   Default zencast folder: 0xffffffff
   Default album folder: 0xffffffff
   Default text folder: 0xffffffff
MTP-specific device properties:
   Friendly name: 
   Synchronization partner: 
   Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   Microsoft Advanced Systems Format
   Microsoft Windows Media Video
   JPEG file
   Abstract Album file
   Abstract Playlist file
   Audio Video Interleave

Secure Time:


 	  	 
