libmtp version: 0.2.4

Attempting to connect device(s)
Detect: Successfully connected 1 devices
USB low-level info:
  Using kernel interface "usbfs"
  bcdUSB: 512
  bDeviceClass: 0
  bDeviceSubClass: 0
  bDeviceProtocol: 0
  idVendor: 0471
  idProduct: 084e
  IN endpoint maxpacket: 512 bytes
  OUT endpoint maxpacket: 512 bytes
  Device flags: 0x00000002
Microsoft device descriptor 0xee:
       0000: 1203 4d00 5300 4600 5400 3100 3000 3000   ..M.S.F.T.1.0.0.
       0010: 0100                                      ..
Device info:
  Manufacturer: Philips
  Model: Philips GoGear SA60XX
  Device version: PH03010D02
  Serial number: 0000000B6AF626CC0704240846460CAC
  Vendor extension ID: 0x00000006
  Vendor extension description: microsoft.com/WMDRMPD: 10.1;audible.com: 1.0;
  Detected object size: 64 bits
Supported operations:
  1001: get device info
  1002: Open session
  1003: Close session
  1004: Get storage IDs
  1005: Get storage info
  1006: Get number of objects
  1007: Get object handles
  1008: Get object info
  1009: Get object
  100b: Delete object
  100c: Send object info
  100d: Send object
  100f: Format storage
  1010: Reset device
  1014: Get device property description
  1015: Get device property value
  1016: Set device property value
  9810: Get object references
  9811: Set object references
  9802: Get object property description
  9801: Get object properties supported
  9803: Get object property value
  9804: Set object property value
  9805: Get object property list
  9806: Set object property list
  101b: Get partial object
  9201: Report Added/Deleted Items
  9101: Get secure time challenge
  9102: Get secure time response
  9103: Set license response
  9104: Get sync list
  9105: Send meter challenge query
  9106: Get meter challenge
  9107: Get meter response
  9108: Clean data store
  9109: Get license state
  910a: Send WMDRM-PD Command
  910b: Send WMDRM-PD Request
Events supported:
  0x4004
  0x4005
Device Properties Supported:
  0x5001: Battery Level
  0xd401: Synchronization Partner
  0xd402: Friendly Device Name
  0xd101: Secure Time
  0xd102: Device Certificate
  0xd103: Revocation Info
Playable File (Object) Types and Object Properties Supported:
  3009: MP3
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
  b901: WMA
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 320000, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
  3008: MS Wave
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
  3801: JPEG
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc87: Width UINT32 data type range: MIN 1, MAX 320, STEP 1 GET/SET
     dc88: Height UINT32 data type range: MIN 1, MAX 240, STEP 1 GET/SET
  300a: MS AVI
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc87: Width UINT32 data type range: MIN 1, MAX 320, STEP 1 GET/SET
     dc88: Height UINT32 data type range: MIN 1, MAX 240, STEP 1 GET/SET
     de97: ScanDepth UINT16 data type enumeration: 1,  READ ONLY
     de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
     de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 1195724877, 861293911,  GET/SET
     de9e: KeyFrameDistance UINT32 data type range: MIN 1000, MAX 10000, STEP 1 GET/SET
     de9c: VideoBitRate UINT32 data type range: MIN 32768, MAX 2048000, STEP 1 GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     dea1: EncodingProfile STRING data type GET/SET
  b981: WMV
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc87: Width UINT32 data type range: MIN 1, MAX 320, STEP 1 GET/SET
     dc88: Height UINT32 data type range: MIN 1, MAX 240, STEP 1 GET/SET
     de97: ScanDepth UINT16 data type enumeration: 1,  READ ONLY
     de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
     de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 1195724877, 861293911,  GET/SET
     de9e: KeyFrameDistance UINT32 data type range: MIN 1000, MAX 10000, STEP 1 GET/SET
     de9c: VideoBitRate UINT32 data type range: MIN 32768, MAX 2048000, STEP 1 GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     dea1: EncodingProfile STRING data type GET/SET
  300c: ASF
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc87: Width UINT32 data type range: MIN 1, MAX 320, STEP 1 GET/SET
     dc88: Height UINT32 data type range: MIN 1, MAX 240, STEP 1 GET/SET
     de97: ScanDepth UINT16 data type enumeration: 1,  READ ONLY
     de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
     de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 1195724877, 861293911,  GET/SET
     de9e: KeyFrameDistance UINT32 data type range: MIN 1000, MAX 10000, STEP 1 GET/SET
     de9c: VideoBitRate UINT32 data type range: MIN 32768, MAX 2048000, STEP 1 GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     dea1: EncodingProfile STRING data type GET/SET
  3001: Association/Directory
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc9a: AlbumName STRING data type GET/SET
  ba05: Abstract Audio Video Playlist
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
  3000: Undefined Type
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
  b802: Firmware
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
  ba03: Abstract Audio Album
     dc44: Name STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
     dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,  READ ONLY
     dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
     dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
     dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
     dc9b: AlbumArtist STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
Storage Devices:
  StorageID: 0x00010001
     StorageType: 0x0003
     FilesystemType: 0x0002
     AccessCapability: 0x0000
     MaxCapacity: 1966080000
     FreeSpaceInBytes: 1506623488
     FreeSpaceInObjects: 5903
     StorageDescription: Internal Storage
     VolumeIdentifier: 0000000B6AF626CC0704240846460CAC
Special directories:
  Default music folder: 0x20000005
  Default playlist folder: 0x00000000
  Default picture folder: 0x20000003
  Default video folder: 0x00000000
  Default organizer folder: 0x00000000
  Default zencast folder: 0x00000000
  Default album folder: 0x00000000
  Default text folder: 0x00000000
MTP-specific device properties:
  Friendly name: Philips GoGear SA60XX
  Synchronization partner: Longhorn Sync Engine
  Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
  ISO MPEG-1 Audio Layer 3
  Microsoft Windows Media Audio
  RIFF WAVE file
  JPEG file
  Audio Video Interleave
  Microsoft Windows Media Video
  Microsoft Advanced Systems Format
  Firmware file

Secure Time:
<DRMCLOCK type="status"><VALUE>#20071222 11:40:21Z#</VALUE><FLAG>DRM_CLK_SET</FLAG></DRMCLOCK>AG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">AAAAC2r2JswHBCQIRkYMrAAAAAA=</UNIQUEID><PUBLICKEY private="1">H10byO2Ds9un2WFTD3U4u0QWmoPcSlgrAARHblcUx6BOfAgztxcdfA==</PUBLICKEY><KEYDATA>XeiwxPRE1GKcTxyl4IBz6bF9jT8=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>Ddkhr31ldjv+qlMdCW3hr+268yH2O1Ht4Oeblc4Wus586h+04LqxZg==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>0zzpJ9GXmEb8YeVe+qGq2VdPU7g=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION> 2.4.107.107</SECURITYVERSION><CERTIFICATE private="1">H10byO2Ds9un2WFTD3U4u0QWmoPcSlgrAARHblcUx6BOfAgztxcdfAIEa2uAmejzb1HS0H+HUDN6EBm6j7dxQpUT+wMPN6S+tg74Dgtnp6KgqjNr</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>SA60xx</NAME>
   <MANUFACTURER>Perception Digital Ltd</MANUFACTURER>
   <MAKE>Philips Audio & Multi Media Applications</MAKE>
   <DISTRIBUTOR>Koninklijke Philips Electronics N.V.</DISTRIBUTOR>
   <MODEL>00</MODEL>
   <SECURITYLEVEL>2000</SECURITYLEVEL>
   <HARDWARE_VER_MAJOR>02</HARDWARE_VER_MAJOR>
   <HARDWARE_VER_MINOR>00</HARDWARE_VER_MINOR>
   <FIRMWARE_VER_MAJOR>08</FIRMWARE_VER_MAJOR>
   <FIRMWARE_VER_MINOR>00</FIRMWARE_VER_MINOR>
   <FEATURES>
       <CLOCK>2</CLOCK>
       <SECURECLOCK>
           <URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
           <PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY>
       </SECURECLOCK>
       <METERING>1</METERING>
       <LICENSE_ACQ>0</LICENSE_ACQ>
       <LICENSE_SYNC>1</LICENSE_SYNC>
       <ENCRYPTION>1</ENCRYPTION>
       <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
   </FEATURES>
   <LIMITS>
       <MAXCHAINDEPTH>5</MAXCHAINDEPTH>
       <MAXLICENSESIZE>10240</MAXLICENSESIZE>
       <MAXHEADERSIZE>5120</MAXHEADERSIZE>
   </LIMITS><PUBLICKEY>O/xY2BVO97/4QEvlk+ETiHxn13rWyg5HsWO/Uy3DHCQg7rowMRF0gw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>vgUBFIcCPVuNuYhGWODMqCH8XiNw83pAwS9S8KWZckb7T99BX4i+OQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>1743</AUTH_ID><PUBLICKEY>Q5qnbSHxftMJXBVdgoi0Ds8CrUgXgToCUcmJIz4LSDcycDSj2n5FfQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>cdq3bQ3V+qGBJXT52FXvDw4jVzret3LRWnpa6q7bMHiSeyZWfRuQMg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>s9lZMSUkYRzjmE8Ju5CtPS6lclfC1BG7Np/QWoLoOXDlt4gYBywCdw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
WMPInfo.xml Does not exist on this device
OK. 
