libmtp version: 1.1.3

Listing raw device(s)
   Found 1 device(s):
   Samsung: GT-P7310/P7510/N7000/I9100/Galaxy Tab 7.7/10.1/S2/Nexus/Note/Y (04e8:6860) @ bus 2, dev 9
Attempting to connect device(s)
USB low-level info:
   Interface has a kernel driver attached.
   bcdUSB: 512
   bDeviceClass: 239
   bDeviceSubClass: 2
   bDeviceProtocol: 1
   idVendor: 04e8
   idProduct: 6860
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 2
      Device number: 9
      Device entry info:
         Vendor: Samsung
         Vendor id: 0x04e8
         Product: GT-P7310/P7510/N7000/I9100/Galaxy Tab 7.7/10.1/S2/Nexus/Note/Y
         Vendor id: 0x6860
         Device flags: 0x48000003
Configuration 0, interface 0, altsetting 0:
   Interface description contains the string "MTP"
   Device recognized as MTP, no further probing.
Device info:
   Manufacturer: SAMSUNG Electronics Co. Ltd. 
   Model: GT-I9070
   Device version: V1.0
   Serial number: 351524051229403
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMPPD: 11.0; microsoft.com/WMPPD: 10.0; microsoft.com/WMDRMPD:10.1; microsoft.com/playready:1.10; 
   Detected object size: 64 bits
   Extensions:
        microsoft.com: 1.0
        microsoft.com/WMPPD: 11.0
        microsoft.com/WMPPD: 10.0
        microsoft.com/WMDRMPD: 10.1
        microsoft.com/playready: 1.10
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   101b: Get partial object
   9810: Get object references
   9811: Set object references
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9201: Report Added/Deleted Items
   9202: Report Acquired Items
   1011: Self test device
   1012: Set object protection
   1017: Reset device property value
   9807: Get interdependent property description
   9808: Send object property list
   9100: Unknown (9100)
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   910c: Unknown (910c)
   910d: Unknown (910d)
   910e: Unknown (910e)
   910f: Unknown (910f)
   9110: Unknown (9110)
   9111: Unknown (9111)
   9112: Unknown (9112)
   9113: Unknown (9113)
   9114: Unknown (9114)
   9115: Unknown (9115)
   9116: Unknown (9116)
Events supported:
   0x4004
   0x4005
Device Properties Supported:
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd404: Unknown property
   0xd407: Perceived Device Type
   0xd101: Secure Time
   0xd102: Device Certificate
   0xd103: Revocation Info
   0xd104: Unknown property
   0xd105: Unknown property
Playable File (Object) Types and Object Properties Supported:
   b984: 3GP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 384000, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14343, 14347, 47361, 12299,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: Representative Sample Duration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   3009: MP3
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 384000, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14343, 14347, 47361, 12299,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: Representative Sample Duration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   b901: WMA
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 384000, STEP 1 READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14343, 14347, 47361, 12299,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: Representative Sample Duration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   b981: WMV
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 1280, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 720, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de97: Scan Depth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 85, 352, 353,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 192999, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 32000, MAX 10485760, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type enumeration: 0, 15000, 24000, 25000, 29970, 30000,  GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type READ ONLY
   3801: JPEG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 2000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 2000, STEP 1 GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14343, 14347, 47361, 12299,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: Representative Sample Duration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 0 GET/SET
   3001: Association/Directory
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
   3000: Undefined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
   3807: GIF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 2000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 2000, STEP 1 GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14343, 14347, 47361, 12299,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: Representative Sample Duration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 0 GET/SET
   300a: MS AVI
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 1280, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 720, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de97: Scan Depth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 85, 352, 353,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 192999, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 32000, MAX 10485760, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type enumeration: 0, 15000, 24000, 25000, 29970, 30000,  GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type READ ONLY
   300b: MPEG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 1280, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 720, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de97: Scan Depth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 85, 352, 353,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 192999, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 32000, MAX 10485760, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type enumeration: 0, 15000, 24000, 25000, 29970, 30000,  GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type READ ONLY
   300c: ASF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 1280, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 720, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de97: Scan Depth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 85, 352, 353,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 192999, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 32000, MAX 10485760, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type enumeration: 0, 15000, 24000, 25000, 29970, 30000,  GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type READ ONLY
   b982: MP4
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 1280, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 720, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de97: Scan Depth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 85, 352, 353,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 13000, MAX 192999, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 32000, MAX 10485760, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type enumeration: 0, 15000, 24000, 25000, 29970, 30000,  GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea1: Encoding Profile STRING data type READ ONLY
   ba10: WPL Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
   ba11: M3U Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
   ba03: Abstract Audio Album
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 2000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 2000, STEP 1 GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14343, 14347, 47361, 12299,  READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: Representative Sample Duration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 0 GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 4202364928
      FreeSpaceInBytes: 4098195456
      FreeSpaceInObjects: 4294967295
      StorageDescription: Phone
      VolumeIdentifier: SECZ9519043CHOHB
   StorageID: 0x00020002
      StorageType: 0x0004 removable RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 3961749504
      FreeSpaceInBytes: 3961651200
      FreeSpaceInObjects: 4294967295
      StorageDescription: Card
      VolumeIdentifier: SECZ9519043CHOHB01
Special directories:
   Default music folder: 0xffffffff
   Default playlist folder: 0xffffffff
   Default picture folder: 0xffffffff
   Default video folder: 0xffffffff
   Default organizer folder: 0xffffffff
   Default zencast folder: 0xffffffff
   Default album folder: 0xffffffff
   Default text folder: 0xffffffff
MTP-specific device properties:
   Friendly name: GT-I9070
   Synchronization partner: Longhorn Sync Engine
   Battery level 99 of 100 (99%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   Microsoft Windows Media Video
   JPEG file
   Folder
   Abstract Playlist file
   GIF bitmap file
   Audio Video Interleave
   MPEG video stream
   Microsoft Advanced Systems Format
   MPEG-4 Part 14 Container Format (Audio+Video Emphasis)
   Abstract Album file

Secure Time:
<DRMCLOCK type="status"><VALUE>#20120606 08:04:23Z#</VALUE><FLAG>DRM_CLK_NOT_SET</FLAG></DRMCLOCK>
OK.
