libmtp version: 0.2.4

Attempting to connect device(s)
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 255
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0930
   idProduct: 0019
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000000
Microsoft device descriptor 0xee:
	0000: 1203 4d00 5300 4600 5400 3100 3000 3000	..M.S.F.T.1.0.0.
	0010: fe00                                   	..
Microsoft device response to control message 1, CMD 0xfe:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Device info:
   Manufacturer: TOSHIBA
   Model: gigabeat T Series
   Device version: PMC: 2.21 (2:0); Platform: 1.0 (2.4)
   Serial number: 2882db60 - acee2c4e - 80bd1ff8 - 8ee00652
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 11.1; microsoft.com/WMPMCPREMCONT: 1.0
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1010: Reset device
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1019: Move object
   101b: Get partial object
   9810: Get object references
   9811: Set object references
   9802: Get object property description
   9807: Get interdependent property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   9201: Report Added/Deleted Items
   9202: Report Acquired Items
   9204: Unknown (9204)
Events supported:
   None.
Device Properties Supported:
   0xd101: Secure Time
   0xd401: Synchronization Partner
   0x5001: Battery Level
   0xd102: Device Certificate
   0xd402: Friendly Device Name
   0xd131: PlaysForSure ID
Playable File (Object) Types and Object Properties Supported:
   3009: MP3
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc08: DateCreated STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc09: DateModified STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc42: SyncID STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 550000, STEP 1 READ ONLY
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc95: MetaGenre UINT16 data type enumeration: 1, 17, 18, 19, 20, 21, 33, 34, 35, 36, 37, 38, 39, 40, 48,  GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 85,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
   b901: WMA
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc08: DateCreated STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc09: DateModified STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc42: SyncID STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 1572864, STEP 1 READ ONLY
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc95: MetaGenre UINT16 data type enumeration: 1, 17, 18, 19, 20, 21, 33, 34, 35, 36, 37, 38, 39, 40, 48,  GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 353, 355, 10,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
   3008: MS Wave
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc08: DateCreated STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc09: DateModified STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc42: SyncID STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 1572864, STEP 1 READ ONLY
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc95: MetaGenre UINT16 data type enumeration: 1, 17, 18, 19, 20, 21, 33, 34, 35, 36, 37, 38, 39, 40, 48,  GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de93: SampleRate UINT32 data type range: MIN 4000, MAX 48000, STEP 50 GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 353, 85, 1, 2, 6, 17, 49,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
   300c: ASF
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc09: DateModified STRING data type GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc47: DateAuthored STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc42: SyncID STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc4b: CopyrightInformation array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dea1: EncodingProfile STRING data type GET/SET
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      de9e: KeyFrameDistance UINT32 data type range: MIN 3, MAX 3, STEP 1 GET/SET
      dc9e: SubDescription array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc4c: Source STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc95: MetaGenre UINT16 data type enumeration: 1, 17, 18, 19, 20, 21, 33, 34, 35, 36, 37, 38, 39, 40, 48,  GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      dc94: ParentalRating STRING data type GET/SET
      dc98: Subtitle STRING data type GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 363520, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 353,  READ ONLY
      de92: BitRateType UINT16 data type enumeration: 1, 2,  GET/SET
      de9f: BufferSize UINT32 data type range: MIN 3, MAX 3, STEP 1 GET/SET
      dea0: EncodingQuality UINT32 data type range: MIN 50, MAX 50, STEP 1 GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 GET/SET
      de97: ScanDepth UINT16 data type range: MIN 1, MAX 1, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911, 827739479, 844516695, 1347833175, 844125783,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 850000, STEP 1 READ ONLY
   b981: WMV
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc09: DateModified STRING data type GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc47: DateAuthored STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc42: SyncID STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc4b: CopyrightInformation array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dea1: EncodingProfile STRING data type GET/SET
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      de9e: KeyFrameDistance UINT32 data type range: MIN 3, MAX 3, STEP 1 GET/SET
      dc9e: SubDescription array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc4c: Source STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc95: MetaGenre UINT16 data type enumeration: 1, 17, 18, 19, 20, 21, 33, 34, 35, 36, 37, 38, 39, 40, 48,  GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      dc94: ParentalRating STRING data type GET/SET
      dc98: Subtitle STRING data type GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 353,  READ ONLY
      de92: BitRateType UINT16 data type enumeration: 1, 2,  GET/SET
      de9f: BufferSize UINT32 data type range: MIN 3, MAX 3, STEP 1 GET/SET
      dea0: EncodingQuality UINT32 data type range: MIN 50, MAX 50, STEP 1 GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 GET/SET
      de97: ScanDepth UINT16 data type range: MIN 1, MAX 1, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911, 827739479, 844516695, 1347833175, 844125783,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 850000, STEP 1 READ ONLY
   3801: JPEG
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 640, STEP 1 GET/SET
      dc47: DateAuthored STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc42: SyncID STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
   3804: BMP
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 640, STEP 1 GET/SET
      dc47: DateAuthored STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc42: SyncID STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
   3001: Association/Directory
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc42: SyncID STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
   ba03: Abstract Audio Album
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc42: SyncID STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,  GET/SET
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc9b: AlbumArtist STRING data type GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
   ba05: Abstract Audio Video Playlist
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc42: SyncID STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
   3000: Undefined Type
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc42: SyncID STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
   b802: Firmware
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc42: SyncID STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 4006084608
      FreeSpaceInBytes: 2009071616
      FreeSpaceInObjects: 4294967295
      StorageDescription: Storage
      VolumeIdentifier: 2882db60 - acee2c4e - 80bd1ff8 - 8ee00652
Special directories:
   Default music folder: 0x08000004
   Default playlist folder: 0x00000000
   Default picture folder: 0x08000001
   Default video folder: 0x08000003
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x08000007
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: (NULL)
   Synchronization partner: {26D8149D-9189-4DE9-94AE-95594F674433}
   Battery level 93 of 100 (93%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   RIFF WAVE file
   Microsoft Advanced Systems Format
   Microsoft Windows Media Video
   JPEG file
   BMP bitmap file
   Firmware file

Secure Time:
<DRMCLOCK type="status"><VALUE>#20071209 13:16:57Z#</VALUE><FLAG>DRM_CLK_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">J/HelP1bwxt+od0lIBQ89K6osQM=</UNIQUEID><PUBLICKEY private="1">63A22JMMlPDkDz52xvYhZ8IlgiuGLAO1BwtWwr3UCgd4bNS7TAJ6Yg==</PUBLICKEY><KEYDATA>6WMSq6+xb26kp2b1Y6UiCxznxfw=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>1AjAYxDONoqxs3nhD48tu6GZZzwXKGlMbxuYltvfZhnsH0KH4Cbfhg==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>vet93M4zoQIS9dpUzV7B8tCQohs=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.107.223</SECURITYVERSION><CERTIFICATE private="1">63A22JMMlPDkDz52xvYhZ8IlgiuGLAO1BwtWwr3UCgd4bNS7TAJ6YgIEa99bh75g6t2c47iqa1ZszTIMmAEHJWXQwtmoOP0AehMAahmDacjdTNVC</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>gigabeat T401</NAME>
    <MANUFACTURER>Toshiba Corporation</MANUFACTURER>
    <MODEL>MEVT401</MODEL>
    <FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR>
    <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
    <HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
    <HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR>
    <SECURITYLEVEL>2000</SECURITYLEVEL>
    <FEATURES>
        <CLOCK>2</CLOCK>
	<SECURECLOCK>
            <URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
            <PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY>
        </SECURECLOCK>
        <METERING>1</METERING>
        <LICENSE_ACQ>1</LICENSE_ACQ>
        <LICENSE_SYNC>1</LICENSE_SYNC>
        <ENCRYPTION>0</ENCRYPTION>
	<SYMMETRIC_OPT>1</SYMMETRIC_OPT> 
    </FEATURES>
    <LIMITS>
        <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
        <MAXLICENSESIZE>10240</MAXLICENSESIZE>
        <MAXHEADERSIZE>5120</MAXHEADERSIZE>
    </LIMITS><PUBLICKEY>x/vBRN5rpKG1OW0jXNKgqDIpTkp/I1cZ6KA/8rd8c3mSTHIAiFqGZQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>GdiWGnhYbYcHrGsVaqUG7iInUQDHy4P2VPb2pdlpseRYRlL4y5Cvbg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>1859</AUTH_ID><PUBLICKEY>Mtp/WMYcetnBdGLVytzm+XJQEDQ6/+UG9C8pLCA74iN2l8HDoXU0DA==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>ocJTXNKCQIFdk5LDV8FNYkmL3jmyzys32TZTmvvfMdKr8CD8zOyAbA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>ELr3ZFG2DcsvpebAGBcr21qjnoNh9i4OJ1tSMkvAI9MSN0pMRdrgMw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>

Device description WMPInfo.xml file:
<DeviceInfo>
    <WMP DeviceID="{4EFD62FB-F112-43C9-BF67-F54A41578BBB}" RelationshipID="{26D8149D-9189-4DE9-94AE-95594F674433}"/>
</DeviceInfo>

OK.
