~/usr/bin/mtp-detect
libmtp version: 0.3.7-cvs

Listing raw device(s)
Found 1 device(s):
Archos: 5 (MTP mode) - 1 (0e79:1331) @ bus 0, dev 29
Attempting to connect device(s)
USB low-level info:
Using kernel interface "usbfs"
bcdUSB: 512
bDeviceClass: 0
bDeviceSubClass: 0
bDeviceProtocol: 0
idVendor: 0e79
idProduct: 1331
IN endpoint maxpacket: 512 bytes
OUT endpoint maxpacket: 512 bytes
Raw device info:
Bus location: 0
Device number: 29
Device entry info:
Vendor: Archos
Vendor id: 0x0e79
Product: 5 (MTP mode) - 1
Vendor id: 0x1331
Device flags: 0x00000002
Microsoft device descriptor 0xee:
0000: 1203 4d00 5300 4600 5400 3100 3000 3000 ..M.S.F.T.1.0.0.
0010: fe00 ..
Microsoft device response to control message 1, CMD 0xfe:
0000: 2800 0000 0001 0400 0100 0000 0000 0000 (...............
0010: 0001 4d54 5000 0000 0000 0000 0000 0000 ..MTP...........
0020: 0000 0000 0000 0000 ........
Microsoft device response to control message 2, CMD 0xfe:
0000: 2800 0000 0001 0400 0100 0000 0000 0000 (...............
0010: 0001 4d54 5000 0000 0000 0000 0000 0000 ..MTP...........
0020: 0000 0000 0000 0000 ........
Device info:
Manufacturer: ARCHOS
Model: Archos 5
Device version: 1.6.03
Serial number: U7NK88G3T989P8
Vendor extension ID: 0x00000006
Vendor extension description: microsoft.com: 1.0;
microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 10.0;
Detected object size: 64 bits
Supported operations:
9101: Get secure time challenge
9102: Get secure time response
9103: Set license response
9104: Get sync list
9105: Send meter challenge query
9106: Get meter challenge
9107: Get meter response
9108: Clean data store
9109: Get license state
1001: get device info
1014: Get device property description
1015: Get device property value
1016: Set device property value
1017: Reset device property value
1002: Open session
1003: Close session
1004: Get storage IDs
1005: Get storage info
100f: Format storage
1010: Reset device
1006: Get number of objects
1007: Get object handles
1008: Get object info
1009: Get object
100c: Send object info
100d: Send object
100b: Delete object
1019: Move object
101a: Copy object
9801: Get object properties supported
9802: Get object property description
9803: Get object property value
9804: Set object property value
9805: Get object property list
9806: Set object property list
9807: Get interdependent property description
9808: Send object property list
9810: Get object references
9811: Set object references
101b: Get partial object
9201: Report Added/Deleted Items
Events supported:
0x4001
0x4004
0x4005
0x400a
Device Properties Supported:
0xd101: Secure Time
0xd102: Device Certificate
0x5001: Battery Level
0xd401: Synchronization Partner
0xd402: Friendly Device Name
Playable File (Object) Types and Object Properties Supported:
3000: Undefined Type
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
3009: MP3
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ
ONLY
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 1
READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 1000, MAX 327680,
STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 85, READ ONLY
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
b901: WMA
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ
ONLY
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 1
READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 320000,
STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 353, READ ONLY
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
3008: MS Wave
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ
ONLY
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 1
READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 64000, MAX 3072000,
STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 1, 17, READ
ONLY
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
b903: AAC
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ
ONLY
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 1
READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000,
STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 255, READ ONLY
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
300a: MS AVI
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc87: Width UINT32 data type range: MIN 1, MAX 720, STEP 1 READ
ONLY
dc88: Height UINT32 data type range: MIN 1, MAX 576, STEP 1 READ
ONLY
dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ
ONLY
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 1
READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 3072000,
STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 1, 17, 85, 353,
READ ONLY
de9c: VideoBitRate UINT32 data type range: MIN 10240, MAX 5120000,
STEP 1 READ ONLY
de9b: VideoFourCCCodec UINT32 data type enumeration: 1482049860,
808802372, 1395937357, 1145656920, GET/SET
dea1: EncodingProfile STRING data type GET/SET
de91: TotalBitRate UINT32 data type range: MIN 10240, MAX 8192000,
STEP 1 READ ONLY
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6,
7, GET/SET
de9d: FramesPerThousandSeconds UINT32 data type range: MIN 1, MAX
30000, STEP 1 GET/SET
de9e: KeyFrameDistance UINT32 data type range: MIN 1, MAX -1, STEP 1
GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
b981: WMV
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc87: Width UINT32 data type range: MIN 1, MAX 720, STEP 1 READ
ONLY
dc88: Height UINT32 data type range: MIN 1, MAX 576, STEP 1 READ
ONLY
dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ
ONLY
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 1
READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 3072000,
STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 1, 17, 85, 353,
READ ONLY
de9c: VideoBitRate UINT32 data type range: MIN 10240, MAX 10240000,
STEP 1 READ ONLY
de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911,
GET/SET
dea1: EncodingProfile STRING data type GET/SET
de91: TotalBitRate UINT32 data type range: MIN 10240, MAX 13312000,
STEP 1 READ ONLY
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6,
7, GET/SET
de9d: FramesPerThousandSeconds UINT32 data type range: MIN 1, MAX
30000, STEP 1 GET/SET
de9e: KeyFrameDistance UINT32 data type range: MIN 1, MAX -1, STEP 1
GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
300c: ASF
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc87: Width UINT32 data type range: MIN 1, MAX 720, STEP 1 READ
ONLY
dc88: Height UINT32 data type range: MIN 1, MAX 576, STEP 1 READ
ONLY
dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ
ONLY
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 1
READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 3072000,
STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 1, 17, 85, 353,
READ ONLY
de9c: VideoBitRate UINT32 data type range: MIN 10240, MAX 10240000,
STEP 1 READ ONLY
de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911,
1482049860, 808802372, 1395937357, 1145656920, GET/SET
dea1: EncodingProfile STRING data type GET/SET
de91: TotalBitRate UINT32 data type range: MIN 10240, MAX 13312000,
STEP 1 READ ONLY
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6,
7, GET/SET
de9d: FramesPerThousandSeconds UINT32 data type range: MIN 1, MAX
30000, STEP 1 GET/SET
de9e: KeyFrameDistance UINT32 data type range: MIN 1, MAX -1, STEP 1
GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
300b: MPEG
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc87: Width UINT32 data type range: MIN 1, MAX 720, STEP 1 READ
ONLY
dc88: Height UINT32 data type range: MIN 1, MAX 576, STEP 1 READ
ONLY
dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ
ONLY
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 1
READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 3072000,
STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 80, READ ONLY
de9c: VideoBitRate UINT32 data type range: MIN 10240, MAX 10240000,
STEP 1 READ ONLY
de9b: VideoFourCCCodec UINT32 data type enumeration: 826757197,
843534413, GET/SET
dea1: EncodingProfile STRING data type GET/SET
de91: TotalBitRate UINT32 data type range: MIN 10240, MAX 13312000,
STEP 1 READ ONLY
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6,
7, GET/SET
de9d: FramesPerThousandSeconds UINT32 data type range: MIN 1, MAX
30000, STEP 1 GET/SET
de9e: KeyFrameDistance UINT32 data type range: MIN 1, MAX -1, STEP 1
GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
b982: MP4
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc87: Width UINT32 data type range: MIN 1, MAX 720, STEP 1 READ
ONLY
dc88: Height UINT32 data type range: MIN 1, MAX 576, STEP 1 READ
ONLY
dc89: Duration UINT32 data type range: MIN 1, MAX -1, STEP 1 READ
ONLY
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 1
READ ONLY
de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 3072000,
STEP 1 READ ONLY
de99: AudioWAVECodec UINT32 data type enumeration: 255, READ ONLY
de9c: VideoBitRate UINT32 data type range: MIN 10240, MAX 5120000,
STEP 1 READ ONLY
de9b: VideoFourCCCodec UINT32 data type enumeration: 875967048,
1129726276, 826496577, 875967064, GET/SET
dea1: EncodingProfile STRING data type GET/SET
de91: TotalBitRate UINT32 data type range: MIN 10240, MAX 8192000,
STEP 1 READ ONLY
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6,
7, GET/SET
de9d: FramesPerThousandSeconds UINT32 data type range: MIN 1, MAX
30000, STEP 1 GET/SET
de9e: KeyFrameDistance UINT32 data type range: MIN 1, MAX -1, STEP 1
GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
3801: JPEG
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc87: Width UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ
ONLY
dc88: Height UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ
ONLY
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
3808: JFIF
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc87: Width UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ
ONLY
dc88: Height UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ
ONLY
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
3804: BMP
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc87: Width UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ
ONLY
dc88: Height UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ
ONLY
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
380b: PNG
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc87: Width UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ
ONLY
dc88: Height UINT32 data type range: MIN 1, MAX 8192, STEP 1 READ
ONLY
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
ba03: Abstract Audio Album
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
dc9a: AlbumName STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
dc81: RepresentativeSampleFormat UINT16 data type enumeration:
14337, GET/SET
dc84: RepresentativeSampleWidth UINT32 data type range: MIN 1, MAX
1024, STEP 1 READ ONLY
dc83: RepresentativeSampleHeight UINT32 data type range: MIN 1, MAX
1024, STEP 1 READ ONLY
dc86: RepresentativeSampleData array of UINT8 data type byte array:
GET/SET
dc82: RepresentativeSampleSize UINT32 data type range: MIN 1, MAX
-1, STEP 1 GET/SET
d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
ba05: Abstract Audio Video Playlist
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
3001: Association/Directory
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770,
32771, READ ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc08: DateCreated STRING data type DATETIME FORM READ ONLY
dc09: DateModified STRING data type DATETIME FORM READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc42: SyncID STRING data type GET/SET
dc44: Name STRING data type GET/SET
dc07: ObjectFileName STRING data type GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
Storage Devices:
StorageID: 0x00010001
StorageType: 0x0003 fixed RAM storage
FilesystemType: 0x0002 generic hierarchical
AccessCapability: 0x0000 read/write
MaxCapacity: 59709652992
FreeSpaceInBytes: 59337244672
FreeSpaceInObjects: 4294967295
StorageDescription: Internal Hard Drive
VolumeIdentifier: (null)
Special directories:
Default music folder: 0x0000001d
Default playlist folder: 0x00000066
Default picture folder: 0x0000002b
Default video folder: 0x00000068
Default organizer folder: 0x00000000
Default zencast folder: 0x00000000
Default album folder: 0x00000000
Default text folder: 0x00000000
MTP-specific device properties:
Friendly name: Archos 5
Synchronization partner: (NULL)
Battery level 3 of 3 (100%)
libmtp supported (playable) filetypes:
ISO MPEG-1 Audio Layer 3
Microsoft Windows Media Audio
RIFF WAVE file
Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
Audio Video Interleave
Microsoft Windows Media Video
Microsoft Advanced Systems Format
MPEG video stream
MPEG-4 Part 14 Container Format (Audio+Video Emphasis)
JPEG file
JFIF file
BMP bitmap file
Portable Network Graphics
Abstract Album file
Abstract Playlist file

Secure Time:
<DRMCLOCK type="status"><VALUE>#20080428
05:40:39Z#</VALUE><FLAG>DRM_CLK_NOT_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID
private="1">AAAAAAAAAAAAAAAAA</UNIQUEID><PUBLICKEY
private="1">AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA</PUBLICKEY><KEYDATA>AAAAAAAAAAAAAAAAAAAAAA</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>AAAAAAAAAAAAAAAAAAAAAA</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.110.51</SECURITYVERSION><CERTIFICATE
private="1">AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA</CERTIFICATE></FALLBACK><CERTIFICATE
type="GROUP"><DATA><NAME>606H</NAME>
<MANUFACTURER>Archos</MANUFACTURER>
<MAKE>606H</MAKE>
<DISTRIBUTOR>Archos</DISTRIBUTOR>
<MODEL>606H</MODEL>
<SECURITYLEVEL>2000</SECURITYLEVEL>
<HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
<HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR>
<FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR>
<FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
<FEATURES>
<CLOCK>2</CLOCK>
<SECURECLOCK>
<URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
<PUBLICKEY>AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA</PUBLICKEY>
</SECURECLOCK>
<METERING>1</METERING>
<LICENSE_ACQ>1</LICENSE_ACQ>
<LICENSE_SYNC>1</LICENSE_SYNC>
<ENCRYPTION>1</ENCRYPTION>
<SYMMETRIC_OPT>1</SYMMETRIC_OPT>
<SUPPORT_REVOCATION>
<GUID>{AAAAAAAAAAAAAAAAAAAA}</GUID>
</SUPPORT_REVOCATION>
</FEATURES>
<LIMITS>
<MAXCHAINDEPTH>2</MAXCHAINDEPTH>
<MAXLICENSESIZE>10240</MAXLICENSESIZE>
<MAXHEADERSIZE>5120</MAXHEADERSIZE>

</LIMITS><PUBLICKEY>AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>AAAAAAAAAAAAAAAAAAAAAAAAAAAAAA</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>2455</AUTH_ID><PUBLICKEY>AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>AAAAAAAAAAAAAAAAAAAAAAAAAAAAA</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>AAAAAAAAAAAAAAAAAAAAAAAAAAAAA</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
OK.
