libmtp version: 1.0.0

Listing raw device(s)
   Found 1 device(s):
   041e:6000 @ bus 0, dev 12
Attempting to connect device(s)
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 255
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 041e
   idProduct: 6000
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 0
      Device number: 12
      Device entry info:
         Vendor: (null)
         Vendor id: 0x041e
         Product: (null)
         Vendor id: 0x6000
         Device flags: 0x00000000
Microsoft device descriptor 0xee:
	0000: 1203 4d00 5300 4600 5400 3100 3000 3000	..M.S.F.T.1.0.0.
	0010: 0100                                   	..
Microsoft device response to control message 1, CMD 0x01:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Microsoft device response to control message 2, CMD 0x01:
	0000: 0c00 0000 0001 0500 0000 0000          	............
Device info:
   Manufacturer: ZiiLABS
   Model: Zii EGG
   Device version: 0.90.07
   Serial number: 100000008C6C0A180000740800005000
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0;microsoft.com/WMPPD: 10.0;
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1007: Get object handles
   100c: Send object info
   100d: Send object
   100f: Format storage
   1014: Get device property description
   1015: Get device property value
   1006: Get number of objects
   1008: Get object info
   1009: Get object
   100b: Delete object
   1010: Reset device
   1012: Set object protection
   1016: Set device property value
   1017: Reset device property value
   1019: Move object
   101b: Get partial object
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9807: Get interdependent property description
   9810: Get object references
   9811: Set object references
Events supported:
   0x4006
Device Properties Supported:
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd001: Unknown property
Playable File (Object) Types and Object Properties Supported:
   3009: MP3
      de99: Audio WAVE Codec UINT32 data type enumeration: 85,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: Audio Bit Depth UINT32 data type enumeration: 8, 16,  READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32771,  READ ONLY
   b901: WMA
      de99: Audio WAVE Codec UINT32 data type enumeration: 352, 353,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 505000, STEP 1 READ ONLY
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: Audio Bit Depth UINT32 data type enumeration: 8, 16,  READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32771,  READ ONLY
   b906: FLAC
      de99: Audio WAVE Codec UINT32 data type enumeration: 61868,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 64000, MAX 1536000, STEP 1 READ ONLY
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: Audio Bit Depth UINT32 data type enumeration: 8, 16,  READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32771,  READ ONLY
   3008: MS Wave
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: Audio Bit Depth UINT32 data type enumeration: 8, 16,  READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32771,  READ ONLY
   ba03: Abstract Audio Album
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 180, STEP 1 READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 24576, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 180, STEP 1 READ ONLY
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32771,  READ ONLY
   ba05: Abstract Audio Video Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32771,  READ ONLY
   ba01: Abstract Multimedia Album
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32771,  READ ONLY
   3801: JPEG
      dc88: Height UINT32 data type range: MIN 0, MAX 3744, STEP 1 GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 96, STEP 1 READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 8192, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 96, STEP 1 READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 10240, STEP 1 GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32771,  READ ONLY
   300a: MS AVI
      de99: Audio WAVE Codec UINT32 data type enumeration: 85, 17, 1,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 8000, MAX 1536000, STEP 1 READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 20, MAX 30000, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 720, STEP 1 GET/SET
      de91: Total Bit Rate UINT32 data type range: MIN 0, MAX 9000000, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 844515635, 828601953, 878070084, 1482049860, 808802372, 875967048, 1196444237, 1395937357, 859189843, 861293911, 875967064, 1145656920,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX 8000000, STEP 1 READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 1280, STEP 1 GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 96, STEP 1 READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 8192, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 96, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: Audio Bit Depth UINT32 data type enumeration: 8, 16,  READ ONLY
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32771,  READ ONLY
   300c: ASF
      de99: Audio WAVE Codec UINT32 data type enumeration: 85, 352, 353, 17, 1,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 1536000, STEP 1 READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 20, MAX 30000, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 720, STEP 1 GET/SET
      de91: Total Bit Rate UINT32 data type range: MIN 0, MAX 9000000, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 844515635, 828601953, 878070084, 1482049860, 808802372, 875967048, 1395937357, 859189843, 861293911, 875967064, 1145656920,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX 8000000, STEP 1 READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 1280, STEP 1 GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 96, STEP 1 READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 8192, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 96, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: Audio Bit Depth UINT32 data type enumeration: 8, 16,  READ ONLY
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32771,  READ ONLY
   b981: WMV
      de99: Audio WAVE Codec UINT32 data type enumeration: 352, 353,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 505000, STEP 1 READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 20, MAX 30000, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 720, STEP 1 GET/SET
      de91: Total Bit Rate UINT32 data type range: MIN 0, MAX 9000000, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 861293911,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX 3500000, STEP 1 READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 1280, STEP 1 GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 96, STEP 1 READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 8192, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 96, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: Audio Bit Depth UINT32 data type enumeration: 8, 16,  READ ONLY
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32771,  READ ONLY
   b982: MP4
      de99: Audio WAVE Codec UINT32 data type enumeration: 41222, 85, 17, 1,  READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 8000, MAX 1536000, STEP 1 READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 20, MAX 30000, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 720, STEP 1 GET/SET
      de91: Total Bit Rate UINT32 data type range: MIN 0, MAX 9000000, STEP 1 READ ONLY
      de9b: Video Four CC Codec UINT32 data type enumeration: 844515635, 828601953, 878070084, 1482049860, 808802372, 875967048, 1196444237, 1395937357, 859189843, 875967064, 1145656920,  READ ONLY
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX 8000000, STEP 1 READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 1280, STEP 1 GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 96, STEP 1 READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX 8192, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 96, STEP 1 READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: Audio Bit Depth UINT32 data type enumeration: 8, 16,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc9a: Album Name STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: Audio Bit Depth UINT32 data type enumeration: 8, 16,  READ ONLY
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32771,  READ ONLY
   b802: Firmware
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32771,  READ ONLY
   3000: Undefined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32771,  READ ONLY
   3001: Association/Directory
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32771,  READ ONLY
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 32193048576
      FreeSpaceInBytes: 31560761344
      FreeSpaceInObjects: 4294967295
      StorageDescription: Storage Media
      VolumeIdentifier: (null)
Special directories:
   Default music folder: 0x0000000d
   Default playlist folder: 0x00000000
   Default picture folder: 0x0000000e
   Default video folder: 0x0000000f
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: Zii EGG
   Synchronization partner: Zii EGG
   Battery level 127 of 255 (49%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   Free Lossless Audio Codec (FLAC)
   RIFF WAVE file
   Abstract Album file
   Abstract Playlist file
   JPEG file
   Audio Video Interleave
   Microsoft Advanced Systems Format
   Microsoft Windows Media Video
   MPEG-4 Part 14 Container Format (Audio+Video Emphasis)
   Firmware file
Unable to acquire device certificate, perhaps this device does not support this
OK.

 	  	 
