libmtp version: 0.2.1

Attempting to connect device(s)
PTP: Opening session
Detect: Successfully connected 1 devices
USB low-level info:
  Using kernel interface "usbfs"
  bcdUSB: 512
  bDeviceClass: 0
  bDeviceSubClass: 0
  bDeviceProtocol: 0
  idVendor: 0781
  idProduct: 7432
  IN endpoint maxpacket: 512 bytes
  OUT endpoint maxpacket: 512 bytes
  Device flags: 0x00000006
Microsoft device descriptor 0xee:
       0000: 1203 4d00 5300 4600 5400 3100 3000 3000   ..M.S.F.T.1.0.0.
       0010: fe00                                      ..
Microsoft device response to control message 1, CMD 0xfe:
       0000: 2800 0000 0001 0400 0100 0000 0000 0000   (...............
       0010: 0001 4d54 5000 0000 0000 0000 0000 0000   ..MTP...........
       0020: 0000 0000 0000 0000                       ........
Microsoft device response to control message 2, CMD 0xfe:
       0000: 2800 0000 0001 0400 0100 0000 0000 0000   (...............
       0010: 0001 4d54 5000 0000 0000 0000 0000 0000   ..MTP...........
       0020: 0000 0000 0000 0000                       ........
Device info:
  Manufacturer: SanDisk
  Model: Sansa Clip 1GB
  Device version: v01.01.11A
  Serial number: 5005C70A4142B4890000000000000000
  Vendor extension ID: 0x00000006
  Vendor extension description: microsoft.com/WMDRMPD: 10.1; audible.com: 1.0;
Supported operations:
  1001: get device info
  1002: Open session
  1003: Close session
  1004: Get storage IDs
  1005: Get storage info
  1006: Get number of objects
  1007: Get object handles
  1008: Get object info
  1009: Get object
  100b: Delete object
  100c: Send object info
  100d: Send object
  100f: Format storage
  1014: Get device property description
  1015: Get device property value
  1016: Set device property value
  1017: Reset device property value
  101b: Get partial object
  9101: Get secure time challenge
  9102: Get secure time response
  9103: Set license response
  9104: Get sync list
  9105: Send meter challenge query
  9106: Get meter challenge
  9107: Get meter response
  9108: Clean data store
  9109: Get license state
  910a: Send WMDRM-PD Command
  910b: Send WMDRM-PD Request
  9201: Report Added/Deleted Items
  9801: Get object properties supported
  9802: Get object property description
  9803: Get object property value
  9804: Set object property value
  9805: Get object property list
  9810: Get object references
  9811: Set object references
Events supported:
  0x4006
Device Properties Supported:
  0x5001: Battery Level
  0x5002: Functional Mode
  0xd100: Unknown property
  0xd101: Secure Time
  0xd102: Device Certificate
  0xd401: Synchronization Partner
  0xd402: Device Friendly Name
Playable File (Object) Types and Object Properties Supported:
  3000: Undefined Type
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc47: DateAuthored STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
  3001: Association/Directory
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc47: DateAuthored STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
  3008: MS Wave
     d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc42: SyncID STRING data type GET/SET
     dc44: Name STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc47: DateAuthored STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 1, MAX 100, STEP 1 GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     de92: BitRateType UINT16 data type enumeration: 2,  GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 9, 50, 80, 85, 352, 353, 354,  READ ONLY
     de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
  3009: MP3
     d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc42: SyncID STRING data type GET/SET
     dc44: Name STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc47: DateAuthored STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 1, MAX 100, STEP 1 GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     de92: BitRateType UINT16 data type enumeration: 2,  GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 9, 50, 80, 85, 352, 353, 354,  READ ONLY
     de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
  300c: ASF
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc47: DateAuthored STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
  b901: WMA
     d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc42: SyncID STRING data type GET/SET
     dc44: Name STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc47: DateAuthored STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 1, MAX 100, STEP 1 GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     de92: BitRateType UINT16 data type enumeration: 2,  GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 9, 50, 80, 85, 352, 353, 354,  READ ONLY
     de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
  b904: Audible.com Codec
     da00: unknown(da00) UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8,  GET/SET
     da01: unknown(da01) STRING data type GET/SET
     da02: unknown(da02) UINT32 data type ANY 32BIT VALUE form READ ONLY
     da03: unknown(da03) UINT16 data type enumeration: 0, 1,  READ ONLY
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc46: Artist STRING data type GET/SET
     dc47: DateAuthored STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 1, MAX 100, STEP 1 GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     de92: BitRateType UINT16 data type enumeration: 2,  GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 9, 50, 80, 85, 352, 353, 354,  READ ONLY
     de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
  ba03: Abstract Audio Album
     d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc42: SyncID STRING data type GET/SET
     dc44: Name STRING data type GET/SET
     dc47: DateAuthored STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc8a: Rating UINT16 data type range: MIN 1, MAX 100, STEP 1 GET/SET
     dc8c: Genre STRING data type GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
  ba05: Abstract Audio Video Playlist
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc47: DateAuthored STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
  ba11: M3U Playlist
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc47: DateAuthored STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
Storage Devices:
  StorageID: 0x00010001
     StorageType: 0x0003
     FilesystemType: 0x0002
     AccessCapability: 0x0000
     MaxCapacity: 1012383744
     FreeSpaceInBytes: 596164608
     FreeSpaceInObjects: 4294967156
     StorageDescription: Internal Memory
     VolumeIdentifier: 5005C70A4142B489
Special directories:
  Default music folder: 0x00000004
  Default playlist folder: 0x00000009
  Default picture folder: 0x00000000
  Default video folder: 0x00000000
  Default organizer folder: 0x00000000
  Default zencast folder: 0x00000000
  Default album folder: 0x00000013
  Default text folder: 0x00000000
MTP-specific device properties:
  Friendly name: Sansa Clip 1GB
  Synchronization partner: Unknown Partner
  Battery level 60 of 100 (60%)
libmtp supported (playable) filetypes:
  RIFF WAVE file
  ISO MPEG-1 Audio Layer 3
  Microsoft Advanced Systems Format
  Microsoft Windows Media Audio
  Audible.com Audio Codec
Unable to acquire device certificate, perhaps this device does not support this
Error 2: PTP Layer error a101: get_device_unicode_property(): failed
to get unicode property.
Error 2: (Look this up in ptp.h for an explanation.)
