# mtp-detect
Unable to open ~/.mtpz-data for reading, MTPZ disabled.
libmtp version: 1.1.8

Listing raw device(s)
Device 0 (VID=05c6 and PID=0a07) is UNKNOWN.
Please report this VID/PID and the device model to the libmtp development team
   Found 1 device(s):
   05c6:0a07 @ bus 1, dev 24
Attempting to connect device(s)
USB low-level info:
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 05c6
   idProduct: 0a07
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 1
      Device number: 24
      Device entry info:
         Vendor: (null)
         Vendor id: 0x05c6
         Product: (null)
         Vendor id: 0x0a07
         Device flags: 0x00000000
Configuration 0, interface 0, altsetting 0:
   Interface description contains the string "MTP"
   Device recognized as MTP, no further probing.
Device info:
   Manufacturer: Intex
   Model: Intex Aqua Fish
   Device version: 2.0.4.14 HW: 0.0.1.8
   Serial number: 911514800207142
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com:1.0; microsoft.com/WMPPD:11.0;
   Detected object size: 64 bits
   Extensions:
        microsoft.com: 1.0
        microsoft.com/WMPPD: 11.0
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1019: Move object
   101a: Copy object
   101b: Get partial object
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9810: Get object references
   9811: Set object references
Events supported:
   0x4002
   0x4003
   0x4007
   0xc801
   0x4004
   0x4005
   0x400a
   0x4009
   0x400c
   0x4008
   0x4006
Device Properties Supported:
   0x5001: Battery Level
   0xd402: Friendly Device Name
   0xd401: Synchronization Partner
   0x501f: Copyright Info
   0xd407: Perceived Device Type
   0xd405: Device Icon
   0xd403: Volume Level
Playable File (Object) Types and Object Properties Supported:
   3801: JPEG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14344, 14347,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
   3807: GIF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14344, 14347,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
   380b: PNG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14344, 14347,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
   380d: TIFF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14344, 14347,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
   3804: BMP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14344, 14347,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
   3008: MS Wave
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
   3009: MP3
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
   b901: WMA
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
   b902: OGG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
   b903: AAC
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
   300a: MS AVI
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 1920, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 1080, STEP 1 GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 1145656899, 1162629709, 827544397, 827739479, 861293911, 875967048,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 100000, STEP 1 GET/SET
   300b: MPEG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 1920, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 1080, STEP 1 GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 1145656899, 1162629709, 827544397, 827739479, 861293911, 875967048,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 100000, STEP 1 GET/SET
   b984: 3GP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 1920, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 1080, STEP 1 GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 1145656899, 1162629709, 827544397, 827739479, 861293911, 875967048,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 100000, STEP 1 GET/SET
   b982: MP4
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 1920, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 1080, STEP 1 GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 1145656899, 1162629709, 827544397, 827739479, 861293911, 875967048,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 100000, STEP 1 GET/SET
   b981: WMV
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 1920, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 1080, STEP 1 GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 1145656899, 1162629709, 827544397, 827739479, 861293911, 875967048,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 100000, STEP 1 GET/SET
   3000: Undefined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   3001: Association/Directory
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   3004: Text
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   3005: HTML
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   ba03: Abstract Audio Album
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   ba05: Abstract Audio Video Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   bb82: vCard2
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   bb83: vCard3
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   be02: vCalendar1
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
Storage Devices:
   StorageID: 0x00010002
      StorageType: 0x0004 removable RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 31092375552
      FreeSpaceInBytes: 30891114496
      FreeSpaceInObjects: 4294967295
      StorageDescription: SD Card
      VolumeIdentifier: media
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 11086577664
      FreeSpaceInBytes: 9628618752
      FreeSpaceInObjects: 4294967295
      StorageDescription: Mass storage
      VolumeIdentifier: media
Special directories:
   Default music folder: 0xffffffff
   Default playlist folder: 0x000002bb
   Default picture folder: 0x000002b9
   Default video folder: 0xffffffff
   Default organizer folder: 0xffffffff
   Default zencast folder: 0xffffffff
   Default album folder: 0xffffffff
   Default text folder: 0xffffffff
MTP-specific device properties:
   Friendly name: Intex Aqua Fish
   Synchronization partner: Sailfish
   Battery level 46 of 100 (46%)
libmtp supported (playable) filetypes:
   JPEG file
   GIF bitmap file
   Portable Network Graphics
   TIFF bitmap file
   BMP bitmap file
   RIFF WAVE file
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   Ogg container format
   Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
   Audio Video Interleave
   MPEG video stream
   MPEG-4 Part 14 Container Format (Audio+Video Emphasis)
   Microsoft Windows Media Video
   Folder
   Text file
   HTML file
   Abstract Album file
   Abstract Playlist file
   VCard version 2
   VCard version 3
   VCalendar version 1
OK.
