mtp-detect now gives:
libmtp version: 0.3.7

Listing raw device(s)
Found 1 device(s):
Sony: Walkman NWZ-W202 (054c:0388) @ bus 0, dev 4
Attempting to connect device(s)
USB low-level info:
Using kernel interface "usbfs"
bcdUSB: 512
bDeviceClass: 0
bDeviceSubClass: 0
bDeviceProtocol: 0
idVendor: 054c
idProduct: 0388
IN endpoint maxpacket: 512 bytes
OUT endpoint maxpacket: 512 bytes
Raw device info:
Bus location: 0
Device number: 4
Device entry info:
Vendor: Sony
Vendor id: 0x054c
Product: Walkman NWZ-W202
Vendor id: 0x0388
Device flags: 0x00000002
Microsoft device descriptor 0xee:
0000: 1203 4d00 5300 4600 5400 3100 3000 3000 ..M.S.F.T.1.0.0.
0010: 0100 ..
Microsoft device response to control message 1, CMD 0x01:
0000: 2800 0000 0001 0400 0100 0000 0000 0000 (...............
0010: 0001 4d54 5000 0000 0000 0000 0000 0000 ..MTP...........
0020: 0000 0000 0000 0000 ........
Device info:
Manufacturer: Sony Corporation
Model: WALKMAN NWZ-W202
Device version: Ver1.00
Serial number: 10FA97F5020088
Vendor extension ID: 0x00000006
Vendor extension description: microsoft.com: 1.0;
microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 10.0;
microsoft.com/WMPPD: 11.0
Detected object size: 64 bits
Supported operations:
1001: get device info
1002: Open session
1003: Close session
1004: Get storage IDs
1005: Get storage info
1006: Get number of objects
1007: Get object handles
1008: Get object info
1009: Get object
101b: Get partial object
100b: Delete object
100c: Send object info
100d: Send object
1014: Get device property description
1015: Get device property value
1016: Set device property value
9802: Get object property description
9801: Get object properties supported
9803: Get object property value
9804: Set object property value
9805: Get object property list
9806: Set object property list
9808: Send object property list
9101: Get secure time challenge
9102: Get secure time response
9103: Set license response
9104: Get sync list
9105: Send meter challenge query
9106: Get meter challenge
9107: Get meter response
9108: Clean data store
9109: Get license state
910a: Send WMDRM-PD Command
910b: Send WMDRM-PD Request
100f: Format storage
9810: Get object references
9811: Set object references
9201: Report Added/Deleted Items
9202: Report Acquired Items
9203: Get transferable playlist types
97f1: Unknown (97f1)
97f2: Unknown (97f2)
97f3: Unknown (97f3)
97f4: Unknown (97f4)
97f5: Unknown (97f5)
1010: Reset device
1012: Set object protection
Events supported:
0x4004
0x4005
Device Properties Supported:
0xd101: Secure Time
0xd102: Device Certificate
0xd402: Friendly Device Name
0xd401: Synchronization Partner
0x5001: Battery Level
0xd405: Device Icon
Playable File (Object) Types and Object Properties Supported:
3009: MP3
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ
ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM
GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc42: SyncID STRING data type GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc9a: AlbumName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
de93: SampleRate UINT32 data type enumeration: 8000, 11025, 16000,
22050, 32000, 44100, 48000, READ ONLY
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 4300000, STEP
1 READ ONLY
dc44: Name STRING data type GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1
GET/SET
de99: AudioWAVECodec UINT32 data type enumeration: 0, 80, 85,
GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc8c: Genre STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
3008: MS Wave
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ
ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM
GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc42: SyncID STRING data type GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc9a: AlbumName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
de93: SampleRate UINT32 data type enumeration: 8000, 11025, 16000,
22050, 32000, 44100, 48000, READ ONLY
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 2304000,
STEP 1 READ ONLY
dc44: Name STRING data type GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1
GET/SET
de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 17,
GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc8c: Genre STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
b901: WMA
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ
ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM
GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc42: SyncID STRING data type GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc9a: AlbumName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
de93: SampleRate UINT32 data type enumeration: 8000, 11025, 16000,
22050, 32000, 44100, 48000, READ ONLY
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 430000,
STEP 1 READ ONLY
dc44: Name STRING data type GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1
GET/SET
de99: AudioWAVECodec UINT32 data type enumeration: 0, 352, 353,
GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc8c: Genre STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
b903: AAC
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ
ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM
GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc42: SyncID STRING data type GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc9a: AlbumName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
de93: SampleRate UINT32 data type enumeration: 8000, 11025, 16000,
22050, 32000, 44100, 48000, READ ONLY
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 430000,
STEP 1 READ ONLY
dc44: Name STRING data type GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1
GET/SET
de99: AudioWAVECodec UINT32 data type enumeration: 0, 41222,
GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc8c: Genre STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
300c: ASF
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ
ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM
GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc42: SyncID STRING data type GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc9a: AlbumName STRING data type GET/SET
dc46: Artist STRING data type GET/SET
dc9b: AlbumArtist STRING data type GET/SET
de93: SampleRate UINT32 data type enumeration: 8000, 11025, 16000,
22050, 32000, 44100, 48000, READ ONLY
de94: NumberOfChannels UINT16 data type enumeration: 1, 2, GET/SET
de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 430000,
STEP 1 READ ONLY
dc44: Name STRING data type GET/SET
dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1
GET/SET
de99: AudioWAVECodec UINT32 data type enumeration: 0, 352, 353,
GET/SET
dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
dc8c: Genre STRING data type GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
de9e: KeyFrameDistance UINT32 data type range: MIN 0, MAX 15000,
STEP 1 GET/SET
de9d: FramesPerThousandSeconds UINT32 data type range: MIN 0, MAX
30050, STEP 1 GET/SET
de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 861293911,
GET/SET
de9c: VideoBitRate UINT32 data type range: MIN 5000, MAX 768010,
STEP 1 READ ONLY
de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6,
7, GET/SET
dea1: EncodingProfile STRING data type GET/SET
dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX
10000, STEP 1 GET/SET
dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX
10000, STEP 1 GET/SET
dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX
-1, STEP 1 READ ONLY
dc81: RepresentativeSampleFormat UINT16 data type enumeration:
14337, 14340, 14343, GET/SET
dc86: RepresentativeSampleData array of UINT8 data type byte array:
GET/SET
3001: Association/Directory
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ
ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc05: AssociationType UINT16 data type enumeration: 0, 1, GET/SET
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM
GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc42: SyncID STRING data type GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc44: Name STRING data type GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
ba05: Abstract Audio Video Playlist
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ
ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM
GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc42: SyncID STRING data type GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc44: Name STRING data type GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
3801: JPEG
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ
ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM
GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc42: SyncID STRING data type GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc44: Name STRING data type GET/SET
dc88: Height UINT32 data type range: MIN 0, MAX 10000, STEP 1
GET/SET
dc87: Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1
GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX
10000, STEP 1 GET/SET
dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX
10000, STEP 1 GET/SET
dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX
-1, STEP 1 READ ONLY
dc81: RepresentativeSampleFormat UINT16 data type enumeration:
14337, 14340, 14343, GET/SET
dc86: RepresentativeSampleData array of UINT8 data type byte array:
GET/SET
3807: GIF
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ
ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM
GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc42: SyncID STRING data type GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc44: Name STRING data type GET/SET
dc88: Height UINT32 data type range: MIN 0, MAX 10000, STEP 1
GET/SET
dc87: Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1
GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX
10000, STEP 1 GET/SET
dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX
10000, STEP 1 GET/SET
dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX
-1, STEP 1 READ ONLY
dc81: RepresentativeSampleFormat UINT16 data type enumeration:
14337, 14340, 14343, GET/SET
dc86: RepresentativeSampleData array of UINT8 data type byte array:
GET/SET
3804: BMP
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ
ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM
GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc42: SyncID STRING data type GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc44: Name STRING data type GET/SET
dc88: Height UINT32 data type range: MIN 0, MAX 10000, STEP 1
GET/SET
dc87: Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
dc09: DateModified STRING data type DATETIME FORM GET/SET
dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1
GET/SET
dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX
10000, STEP 1 GET/SET
dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX
10000, STEP 1 GET/SET
dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX
-1, STEP 1 READ ONLY
dc81: RepresentativeSampleFormat UINT16 data type enumeration:
14337, 14340, 14343, GET/SET
dc86: RepresentativeSampleData array of UINT8 data type byte array:
GET/SET
ba03: Abstract Audio Album
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ
ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM
GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc42: SyncID STRING data type GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc9b: AlbumArtist STRING data type GET/SET
dc44: Name STRING data type GET/SET
dc8c: Genre STRING data type GET/SET
d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX
10000, STEP 1 GET/SET
dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX
10000, STEP 1 GET/SET
dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX
-1, STEP 1 READ ONLY
dc81: RepresentativeSampleFormat UINT16 data type enumeration:
14337, 14340, 14343, GET/SET
dc86: RepresentativeSampleData array of UINT8 data type byte array:
GET/SET
3000: Undefined Type
dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, READ
ONLY
dc04: ObjectSize UINT64 data type READ ONLY
dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM
GET/SET
dc08: DateCreated STRING data type DATETIME FORM GET/SET
dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
dc42: SyncID STRING data type GET/SET
dc0d: Hidden UINT16 data type enumeration: 0, 1, GET/SET
dc4f: NonConsumable UINT8 data type enumeration: 0, 1, GET/SET
dc44: Name STRING data type GET/SET
Storage Devices:
StorageID: 0x00010001
StorageType: 0x0003 fixed RAM storage
FilesystemType: 0x0002 generic hierarchical
AccessCapability: 0x0000 read/write
MaxCapacity: 1928855552
FreeSpaceInBytes: 1652260864
FreeSpaceInObjects: 4294967295
StorageDescription: Storage Media
VolumeIdentifier: 33FA0001324A8D2E0002D9B161C24D2E
Special directories:
Default music folder: 0x00000070
Default playlist folder: 0x00000000
Default picture folder: 0x00000000
Default video folder: 0x00000000
Default organizer folder: 0x00000000
Default zencast folder: 0x00000000
Default album folder: 0x00000000
Default text folder: 0x00000000
MTP-specific device properties:
Friendly name: WALKMAN NWZ-W202
Synchronization partner: WALKMAN NWZ-W202
Battery level 99 of 100 (99%)
libmtp supported (playable) filetypes:
ISO MPEG-1 Audio Layer 3
RIFF WAVE file
Microsoft Windows Media Audio
Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
Microsoft Advanced Systems Format
JPEG file
GIF bitmap file
BMP bitmap file

Secure Time:
<DRMCLOCK type="status"><VALUE>#19700222
12:10:57Z#</VALUE><FLAG>DRM_CLK_NOT_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID
private="1">MzNGQTAwMDEzMjRBOEQyRQoKCgo=</UNIQUEID><PUBLICKEY
private="1">gUDNl6K4A8rKKoOlGxMsTpCTyCM4mDO8bJI2e/PGqHFM8jgyH4TUew==</PUBLICKEY><KEYDATA>RkRHwfFBtwocQxb1vXhq+Wu1U+Q=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>brVpnBTRtkYj21B23R4GOAmhLhnUukZmUKE3+XT+tJyP7XF1ASyYHw==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>oIQcKO3zlqHbw6ZCFDyAqT7LUUg=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.112.171</SECURITYVERSION><CERTIFICATE
private="1">gUDNl6K4A8rKKoOlGxMsTpCTyCM4mDO8bJI2e/PGqHFM8jgyH4TUewIEcKsLkirTsbAN6P51wkXvpgoddvnnVQI6HWxUT9tKwcTpYaD8rul7+GRL</CERTIFICATE></FALLBACK><CERTIFICATE
type="GROUP"><DATA><NAME>Walkman</NAME>
<MANUFACTURER>Sony</MANUFACTURER>
<MAKE>Flextronics</MAKE>
<DISTRIBUTOR>Sony</DISTRIBUTOR>
<MODEL>ICX-1122</MODEL>
<SECURITYLEVEL>2000</SECURITYLEVEL>
<HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
<HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR>
<FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR>
<FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
<FEATURES>
<CLOCK>2</CLOCK>
<SECURECLOCK>
<URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
<PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY>
</SECURECLOCK>
<METERING>1</METERING>
<LICENSE_ACQ>1</LICENSE_ACQ>
<LICENSE_SYNC>1</LICENSE_SYNC>
<ENCRYPTION>1</ENCRYPTION>
<SYMMETRIC_OPT>1</SYMMETRIC_OPT>
</FEATURES>
<LIMITS>
<MAXCHAINDEPTH>2</MAXCHAINDEPTH>
<MAXLICENSESIZE>10240</MAXLICENSESIZE>
<MAXHEADERSIZE>5120</MAXHEADERSIZE>

</LIMITS><PUBLICKEY>5NNetVrlRMwT7x823193ecnr7iGMyC6zQc2tGIQ1ZvYpVrCLAQCPhw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>wSOxVy32A7Zsbgq9h3DrnzQGGQH1exmIQ7n2oq1VLAGMzo9qC8n1Ww==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>3087</AUTH_ID><PUBLICKEY>ELWuIRmtGOqXTRhe/yHSsVtVZoVb1LSZh2sTzypUydaZAUiWRIFnSg==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>Ul2JXnitAFwH1tyNnDjOBgAQyXNDeBnYemNm5HIcC/Bj2jtaoU3yCQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>yzpXMjZimc+n6ZWk1hoKDSfsBiEYSWHdRXnugRsrWI+J1c2Pa58PIQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
OK.

