libmtp version: 0.2.6.1

Attempting to connect device(s)
PTP: Opening session
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 255
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 041e
   idProduct: 4123
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000001
Microsoft device descriptor 0xee:
        0000: 1203 4d00 5300 4600 5400 3100 3000 3000   ..M.S.F.T.1.0.0.
        0010: fe00                                      ..
Microsoft device response to control message 1, CMD 0xfe:
        0000: 2800 0000 0001 0400 0100 0000 0000 0000   (...............
        0010: 0001 4d54 5000 0000 0000 0000 0000 0000   ..MTP...........
        0020: 0000 0000 0000 0000                       ........
Potential MTP Device with VendorID:041e and ProductID:4123 responded to control message 2 with a response that was too short. Problems may arrise but continuing
Device info:
   Manufacturer: Creative Technology Ltd
   Model: Zen Portable Media Center
   Device version: PMC: 1.0 (292:130322); Platform: 1.3 (5.12)
   Serial number: 468a40dd - 00020801 - 3800bc9c - d646df6f
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 10.0;
   Detected object size: 32 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1010: Reset device
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   1019: Move object
   9810: Get object references
   9811: Set object references
   9802: Get object property description
   9807: Get interdependent property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   9201: Report Added/Deleted Items
Events supported:
   None.
Device Properties Supported:
   0xd101: Secure Time
   0xd401: Synchronization Partner
   0x5001: Battery Level
   0xd102: Device Certificate
   0xd402: Friendly Device Name
Playable File (Object) Types and Object Properties Supported:
   3009: MP3
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc09: DateModified STRING data type GET/SET
      dc8a: Rating UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 1500000, STEP 1 READ ONLY
      dc9a: AlbumName STRING data type READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc95: MetaGenre UINT16 data type ANY 16BIT VALUE form GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
   b901: WMA
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc09: DateModified STRING data type GET/SET
      dc8a: Rating UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 1500000, STEP 1 READ ONLY
      dc9a: AlbumName STRING data type READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc95: MetaGenre UINT16 data type ANY 16BIT VALUE form GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
   300c: ASF
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc09: DateModified STRING data type GET/SET
      dc8a: Rating UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc47: DateAuthored STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc4b: CopyrightInformation array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      de97: ScanDepth UINT16 data type enumeration: 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type ANY 16BIT VALUE form GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc95: MetaGenre UINT16 data type ANY 16BIT VALUE form GET/SET
      de9e: KeyFrameDistance UINT32 data type enumeration: 3,  READ ONLY
      dc9e: SubDescription array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc98: Subtitle STRING data type GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      dc94: ParentalRating STRING data type GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 353,  READ ONLY
      de92: BitRateType UINT16 data type enumeration: 3,  READ ONLY
      de9f: BufferSize UINT32 data type enumeration: 3,  READ ONLY
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 READ ONLY
      dea0: EncodingQuality UINT32 data type enumeration: 50,  READ ONLY
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 827739479, 844516695, 861293911, 1347833175,  READ ONLY
      de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 736000, STEP 1 READ ONLY
   b981: WMV
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc09: DateModified STRING data type GET/SET
      dc8a: Rating UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc47: DateAuthored STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc4b: CopyrightInformation array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      de97: ScanDepth UINT16 data type enumeration: 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type ANY 16BIT VALUE form GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc95: MetaGenre UINT16 data type ANY 16BIT VALUE form GET/SET
      de9e: KeyFrameDistance UINT32 data type enumeration: 3,  READ ONLY
      dc9e: SubDescription array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc98: Subtitle STRING data type GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      dc94: ParentalRating STRING data type GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 353,  READ ONLY
      de92: BitRateType UINT16 data type enumeration: 2, 3,  READ ONLY
      de9f: BufferSize UINT32 data type enumeration: 3,  READ ONLY
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 READ ONLY
      dea0: EncodingQuality UINT32 data type enumeration: 50,  READ ONLY
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 827739479, 844516695, 861293911, 1347833175, 844125783,  READ ONLY
      de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 736000, STEP 1 READ ONLY
   3801: JPEG
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc8a: Rating UINT16 data type ANY 16BIT VALUE form GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc47: DateAuthored STRING data type GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: EffectiveRating UINT16 data type ANY 16BIT VALUE form GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      dc08: DateCreated STRING data type GET/SET
   3001: Association/Directory
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
   ba03: Abstract Audio Album
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 320, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 240, STEP 1 READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
   ba05: Abstract Audio Video Playlist
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
   3000: Undefined Type
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
   b802: Firmware
      dc44: Name STRING data type GET/SET
      dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc07: ObjectFileName STRING data type GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 19841679360
      FreeSpaceInBytes: 13992853504
      FreeSpaceInObjects: 4294967295
      StorageDescription: PMC HardDisk
      VolumeIdentifier: (null)
Special directories:
   Default music folder: 0x09000002
   Default playlist folder: 0x090000a0
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x09000007
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: (NULL)
   Synchronization partner: (NULL)
   Battery level 85 of 100 (85%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   Microsoft Advanced Systems Format
   Microsoft Windows Media Video
   JPEG file
   Firmware file

Secure Time:
<DRMCLOCK type="status"><VALUE>#20090126 15:59:10Z#</VALUE><FLAG>DRM_CLK_NEEDS_REFRESH</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">I0bmPv4Y0HfNXzIjBa/PYycH2tc=</UNIQUEID><PUBLICKEY private="1">e1IT6W/5VRSSlOmzEFTwYW7iYneoOYNYk4N0Z6JMrGdDjhN91cxhZw==</PUBLICKEY><KEYDATA>jr96ej1eM3ySU/pOKsH8OH5e3N0=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>Q4kKNCjEyifQR16hYcNut9aJ+0rzp96M2ydr9fqF4ODB3eQoNvueaw==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>DhLnT6rHenq72J3HkEWAkutThoY=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.101.1</SECURITYVERSION><CERTIFICATE private="1">e1IT6W/5VRSSlOmzEFTwYW7iYneoOYNYk4N0Z6JMrGdDjhN91cxhZwIEZQHdeZ8CBTwW9demSrALSCQ1KuDtajy8pAgGj61prcdBR5z8HWYx9v2H</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>Zen Portable Media Center</NAME>
<MANUFACTURER>Creative Technology Ltd.</MANUFACTURER>
<MODEL>PMC-HD0001</MODEL><SECURITYLEVEL>2000</SECURITYLEVEL><HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR><HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR><FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR><FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR><FEATURES><CLOCK>2</CLOCK>
<SECURECLOCK><URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL><PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY></SECURECLOCK><METERING>1</METERING><LICENSE_ACQ>0</LICENSE_ACQ><LICENSE_SYNC>1</LICENSE_SYNC><ENCRYPTION>0</ENCRYPTION><SYMMETRIC_OPT>1</SYMMETRIC_OPT></FEATURES><LIMITS><MAXCHAINDEPTH>2</MAXCHAINDEPTH><MAXLICENSESIZE>10240</MAXLICENSESIZE><MAXHEADERSIZE>5120</MAXHEADERSIZE></LIMITS><PUBLICKEY>aH!t1TTDvlggK2kDp55oQfKqqgJdWz4w6IZSE8gr1ObCT2Kle8UnPA==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>DXdQxutKyTkyAFBZo04b4dUYQi8PFTOy5uqA/nL3247mdZqx8s7DWA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>101</AUTH_ID><PUBLICKEY>WMR8Uct80dL6v5fANe5xvEclVyjYm*Z5lclCcP*FDrBJgG2OEFB*dg==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>SK2D0AS5mG0qo33sDgddidfb54QhiLSo88HcMFK*8tEag!!fezugew==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>Io0kNadzJAsSZdlhn!LYZIFdLBtfdg0O83BOP9yUr7HwBfMFLIlGWQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
