libmtp version: 0.2.4

Attempting to connect device(s)
PTP: Opening session
Detect: Successfully connected 1 devices
USB low-level info:
  Using kernel interface "usbfs"
  bcdUSB: 512
  bDeviceClass: 0
  bDeviceSubClass: 0
  bDeviceProtocol: 0
  idVendor: 054c
  idProduct: 0325
  IN endpoint maxpacket: 512 bytes
  OUT endpoint maxpacket: 512 bytes
  Device flags: 0x00000002
Microsoft device descriptor 0xee:
       0000: 1203 4d00 5300 4600 5400 3100 3000 3000   ..M.S.F.T.1.0.0.
       0010: 3000                                      0.
Microsoft device response to control message 1, CMD 0x30:
       0000: 2800 0000 0001 0400 0100 0000 0000 0000   (...............
       0010: 0001 4d54 5000 0000 0000 0000 0000 0000   ..MTP...........
       0020: 0000 0000 0000 0000                       ........
Microsoft device response to control message 2, CMD 0x30:
       0000: 2800 0000 0001 0400 0100 0000 0000 0000   (...............
       0010: 0001 4d54 5000 0000 0000 0000 0000 0000   ..MTP...........
       0020: 0000 0000 0000 0000                       ........
Device info:
  Manufacturer: Sony Corporation
  Model: WALKMAN NWZ-A816
  Device version: 1.00
  Serial number: 00000000000000000000000005106125
  Vendor extension ID: 0x00000006
  Vendor extension description: microsoft.com: 1.0;
microsoft.com/WMDRMPD: 10.1; sony.net/WMFU: 1.0;
  Detected object size: 64 bits
Supported operations:
  1001: get device info
  1002: Open session
  1003: Close session
  1004: Get storage IDs
  1005: Get storage info
  1006: Get number of objects
  1007: Get object handles
  1008: Get object info
  1009: Get object
  100b: Delete object
  100c: Send object info
  100d: Send object
  1014: Get device property description
  1015: Get device property value
  1016: Set device property value
  101b: Get partial object
  9810: Get object references
  9811: Set object references
  9802: Get object property description
  9801: Get object properties supported
  9803: Get object property value
  9804: Set object property value
  9805: Get object property list
  9806: Set object property list
  9201: Report Added/Deleted Items
  9808: Send object property list
  9101: Get secure time challenge
  9102: Get secure time response
  9103: Set license response
  9104: Get sync list
  9105: Send meter challenge query
  9106: Get meter challenge
  9107: Get meter response
  9108: Clean data store
  9109: Get license state
  910a: Send WMDRM-PD Command
  910b: Send WMDRM-PD Request
  9401: Unknown (9401)
  9402: Unknown (9402)
Events supported:
  None.
Device Properties Supported:
  0x5001: Battery Level
  0xd401: Synchronization Partner
  0xd402: Friendly Device Name
  0xd101: Secure Time
  0xd102: Device Certificate
Playable File (Object) Types and Object Properties Supported:
  3000: Undefined Type
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
  3001: Association/Directory
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
  3008: MS Wave
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc46: Artist STRING data type GET/SET
     dc89: Duration UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de99: AudioWAVECodec UINT32 data type enumeration: 1,  GET/SET
     de9a: AudioBitRate UINT32 data type enumeration: 128000, 176400, 192000, 256000, 352800, 384000, 512000, 705600, 768000, 1024000, 1411200, 1536000,  READ ONLY
  3009: MP3
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc46: Artist STRING data type GET/SET
     dc89: Duration UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     de93: SampleRate UINT32 data type enumeration: 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de99: AudioWAVECodec UINT32 data type enumeration: 85,  GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 32000, MAX 320000, STEP 1 READ ONLY
  300c: ASF
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
  3801: JPEG
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc87: Width UINT32 data type range: MIN 1, MAX 4000, STEP 1 READ ONLY
     dc88: Height UINT32 data type range: MIN 1, MAX 4000, STEP 1 READ ONLY
  b802: Firmware
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
  b901: WMA
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc46: Artist STRING data type GET/SET
     dc89: Duration UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     de93: SampleRate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
     de99: AudioWAVECodec UINT32 data type enumeration: 352, 353,  GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 512000, STEP 1 READ ONLY
     d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
  b982: MP4
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
  b984: 3GP
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
  ba03: Abstract Audio Album
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,  READ ONLY
     dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 65536, STEP 1 READ ONLY
     dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 200, STEP 1 READ ONLY
     dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 200, STEP 1 READ ONLY
     dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
     dc8c: Genre STRING data type GET/SET
     dc9b: AlbumArtist STRING data type GET/SET
     d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
  ba05: Abstract Audio Video Playlist
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
     dc04: ObjectSize UINT64 data type READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
Storage Devices:
  StorageID: 0x00010001
     StorageType: 0x0003
     FilesystemType: 0x0002
     AccessCapability: 0x0000
     MaxCapacity: 3840933888
     FreeSpaceInBytes: 3796303872
     FreeSpaceInObjects: 4294967295
     StorageDescription: Storage Media
     VolumeIdentifier: 00000000000000000000000005106125
Special directories:
  Default music folder: 0x00000004
  Default playlist folder: 0x00000000
  Default picture folder: 0x00000007
  Default video folder: 0x00000008
  Default organizer folder: 0x00000000
  Default zencast folder: 0x00000000
  Default album folder: 0x00000000
  Default text folder: 0x00000000
MTP-specific device properties:
  Friendly name: WALKMAN
  Synchronization partner: (NULL)
  Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
  RIFF WAVE file
  ISO MPEG-1 Audio Layer 3
  Microsoft Advanced Systems Format
  JPEG file
  Firmware file
  Microsoft Windows Media Audio
  MPEG-4 Part 14 Container Format (Audio+Video Empahsis)

Secure Time:
<DRMCLOCK type="status"><VALUE>#20070228
03:58:37Z#</VALUE><FLAG>DRM_CLK_NOT_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID
private="1">AAABBAkHCQUFAwUBAAYBAgU=</UNIQUEID><PUBLICKEY
private="1">UzQ0VQykaeoQPrOgTYfXYXV1hmODVfwgyv713vldhWE4iX9GMeWneA==</PUBLICKEY><KEYDATA>BRDYsH9AiuTaa9BulaySDjA5bM4=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>5KJTDg8P5BMPjeLQ2cC9w3MufyWLSUAhubTlYDCWV4nsOHmomahHMA==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>BwkgCELkJlZjJ1nLoiPPp9yFeqM=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.107.187</SECURITYVERSION><CERTIFICATE
private="1">UzQ0VQykaeoQPrOgTYfXYXV1hmODVfwgyv713vldhWE4iX9GMeWneAIEa7vFjBmH0DBgueM+PS22CbvV/BxgQOFHdnNy8KMWhSXz6ydhQwVkSGg+</CERTIFICATE></FALLBACK><CERTIFICATE
type="GROUP"><DATA><NAME>Walkman</NAME><MANUFACTURER>Sony</MANUFACTURER><MAKE>Sony</MAKE><DISTRIBUTOR>Sony</DISTRIBUTOR><MODEL>Walkman</MODEL><SECURITYLEVEL>2000</SECURITYLEVEL><FEATURES><CLOCK>2</CLOCK><SECURECLOCK><URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL><PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY></SECURECLOCK><METERING>1</METERING><LICENSE_ACQ>1</LICENSE_ACQ><LICENSE_SYNC>1</LICENSE_SYNC><ENCRYPTION>1</ENCRYPTION><SYMMETRIC_OPT>1</SYMMETRIC_OPT></FEATURES><LIMITS><MAXCHAINDEPTH>2</MAXCHAINDEPTH><MAXLICENSESIZE>10240</MAXLICENSESIZE><MAXHEADERSIZE>5120</MAXHEADERSIZE></LIMITS><PUBLICKEY>RDfmmYew6SH8Gd6QaIIqXJCVqgLPn1sPxTc71zYTDvAqbUzRuoZ4TA==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>raN1NS4SI+p9Zg32AalcPDAsIHvsntZiofod4RZRW5iXeWZ+qthFUw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>1823</AUTH_ID><PUBLICKEY>Ha/toGqNBmuSLvLgRNoGmHsuxS4n2PZY/WcbPkI1aY2Pq+cZ8RVSeA==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>lkcNZ5AC4rykVJcjFp1oRO7F4WxtVFmeMKrzPkb1zxhH9f8qhZQjHg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>vB+7tAF0Ee5jbWMEsKWuUqidmBpmW/nzr1TaaYdLTfwD/dN0IbE4gw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
WMPInfo.xml Does not exist on this device
PTP: Closing session
OK.
