mtp-detect
libmtp version: 0.3.6

Listing raw device(s)
Found 1 device(s):
Thomson: Lyra MC5104B (M51 Series) (069b:077c) @ bus 0, dev 6
Attempting to connect device(s)
USB low-level info:
Using kernel interface "usbfs"
bcdUSB: 512
bDeviceClass: 0
bDeviceSubClass: 0
bDeviceProtocol: 0
idVendor: 069b
idProduct: 077c
IN endpoint maxpacket: 512 bytes
OUT endpoint maxpacket: 512 bytes
Raw device info:
Bus location: 0
Device number: 6
Device entry info:
Vendor: Thomson
Vendor id: 0x069b
Product: Lyra MC5104B (M51 Series)
Vendor id: 0x077c
Device flags: 0x00000000
Microsoft device descriptor 0xee:
0000: 1203 4d00 5300 4600 5400 3100 3000 3000 ..M.S.F.T.1.0.0.
0010: 0100 ..
Device info:
Manufacturer: Thomson
Model: M51 Series
Device version: SDK4.210
Serial number: 0002FA937F63C19B0002FA937F610D8C
Vendor extension ID: 0x00000006
Vendor extension description: microsoft.com: 1.0;
microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 10.0; audible.com: 1.0
Detected object size: 64 bits
Supported operations:
1001: get device info
1002: Open session
1003: Close session
1004: Get storage IDs
1005: Get storage info
1006: Get number of objects
1007: Get object handles
1008: Get object info
1009: Get object
101b: Get partial object
100b: Delete object
100c: Send object info
100d: Send object
1014: Get device property description
1015: Get device property value
1016: Set device property value
9802: Get object property description
9801: Get object properties supported
9803: Get object property value
9804: Set object property value
9805: Get object property list
9806: Set object property list
9808: Send object property list
9101: Get secure time challenge
9102: Get secure time response
9103: Set license response
9104: Get sync list
9105: Send meter challenge query
9106: Get meter challenge
9107: Get meter response
9108: Clean data store
9109: Get license state
910a: Send WMDRM-PD Command
910b: Send WMDRM-PD Request
100f: Format storage
9810: Get object references
9811: Set object references
9201: Report Added/Deleted Items
97f1: Unknown (97f1)
97f2: Unknown (97f2)
97f3: Unknown (97f3)
1010: Reset device
Events supported:
0x4004
0x4005
Device Properties Supported:
0xd101: Secure Time
0xd102: Device Certificate
0xd402: Friendly Device Name
0xd401: Synchronization Partner
0x5001: Battery Level
0xd100: Unknown property
Playable File (Object) Types and Object Properties Supported:
3009: MP3
3008: MS Wave
b901: WMA
b902: OGG
3007: AIFF
b903: AAC
300c: ASF
3001: Association/Directory
ba05: Abstract Audio Video Playlist
3801: JPEG
ba11: M3U Playlist
ba03: Abstract Audio Album
3000: Undefined Type
b904: Audible.com Codec
Storage Devices:
StorageID: 0x00010001
StorageType: 0x0003 fixed RAM storage
FilesystemType: 0x0002 generic hierarchical
AccessCapability: 0x0000 read/write
MaxCapacity: 4073979904
FreeSpaceInBytes: 2900426752
FreeSpaceInObjects: 4294967295
StorageDescription: Internal Storage
VolumeIdentifier: 0002FA937F63C19B0002FA937F610D8C
Special directories:
Default music folder: 0x00000000
Default playlist folder: 0x00000000
Default picture folder: 0x00000000
Default video folder: 0x00000000
Default organizer folder: 0x00000000
Default zencast folder: 0x00000000
Default album folder: 0x00000000
Default text folder: 0x00000000
MTP-specific device properties:
Friendly name: (NULL)
Synchronization partner: (NULL)
libmtp supported (playable) filetypes:
ISO MPEG-1 Audio Layer 3
RIFF WAVE file
Microsoft Windows Media Audio
Ogg container format
Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
Microsoft Advanced Systems Format
JPEG file
Audible.com Audio Codec
Unable to acquire device certificate, perhaps this device does not support
this
Error 2: PTP Layer error 02ff: get_device_unicode_property(): failed to
get unicode property.
Error 2: (Look this up in ptp.h for an explanation.)
ERROR: Could not close session!
inep: usb_get_endpoint_status(): No such device
outep: usb_get_endpoint_status(): No such device
usb_clear_halt() on IN endpoint: No such device
usb_clear_halt() on OUT endpoint: No such device
usb_clear_halt() on INTERRUPT endpoint: No such device
OK.
************************
