libmtp version: 0.2.5

Attempting to connect device(s)
PTP: Opening session
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0930
   idProduct: 0018
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000059
Device info:
   Manufacturer: TOSHIBA
   Model: TOSHIBA gigabeat U
   Device version: 1.00US
   Serial number: 1A5B23374455AA55
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 10.0;
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   101b: Get partial object
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9810: Get object references
   9811: Set object references
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   9201: Report Added/Deleted Items
Events supported:
   None.
Device Properties Supported:
   0xd101: Secure Time
   0xd102: Device Certificate
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
Playable File (Object) Types and Object Properties Supported:
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc06: AssociationDesc UINT32 data type ANY 32BIT VALUE form GET/SET
      dc07: ObjectFileName STRING data type READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
   3009: MP3
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 22050, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 85,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 32000, MAX 320000, STEP 1 READ ONLY
   3008: MS Wave
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 22050, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 1, 2,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 705600, MAX 1536000, STEP 1 READ ONLY
   3801: JPEG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
   b802: Firmware
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
   b901: WMA
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 22050, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 352, 353,  READ ONLY
      de9a: AudioBitRate UINT32 data type enumeration: 32000, 48000, 64000, 96000, 128000, 160000, 192000, 256000,  READ ONLY
   300c: ASF
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 22050, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 352, 353,  READ ONLY
      de9a: AudioBitRate UINT32 data type enumeration: 32000, 48000, 64000, 96000, 128000, 160000, 192000, 256000,  READ ONLY
   ba03: Abstract Audio Album
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,  READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 240, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 320, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type byte array: GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 1987833856
      FreeSpaceInBytes: 166289408
      FreeSpaceInObjects: 4294967295
      StorageDescription: Storage
      VolumeIdentifier: (null)
Special directories:
   Default music folder: 0x30010005
   Default playlist folder: 0x30010002
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: TOSHIBA gigabeat U
   Synchronization partner: 84C4F957-962A-4BA7-860E-2BBBBD173ACD
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   RIFF WAVE file
   JPEG file
   Firmware file
   Microsoft Windows Media Audio
   Microsoft Advanced Systems Format

Secure Time:
<DRMCLOCK type="status"><VALUE>#20080128
00:49:58Z#</VALUE><FLAG>DRM_CLK_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID
private="1">MUE1QjIzMzc0NDU1QUE1NQAAAAA=</UNIQUEID><PUBLICKEY
private="1">vlDwTQs9V09uBXIS1s2CC+zPPzQNdjdZHHqmAg5S0PKN/ijWLU49KA==</PUBLICKEY><KEYDATA>4lUBBtk+QkQM8aVdomZHDpjqSNQ=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>keivPI9BmZkdL0F8tPt+sk48qBmVFuiQoAk0QY0yVHKfEE3CUdWqGA==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>hopjarK0z1UYXjtbdLR833jQOv0=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.106.241</SECURITYVERSION><CERTIFICATE
private="1">vlDwTQs9V09uBXIS1s2CC+zPPzQNdjdZHHqmAg5S0PKN/ijWLU49KAIEavHda6648B4acUdFjdlCtxOI/npxdS7UaBvWc5/qvMprJ0bBvEo6qeIv</CERTIFICATE></FALLBACK><CERTIFICATE
type="GROUP"><DATA><NAME>TOSHIBA gigabeat</NAME>
    <MANUFACTURER>TOSHIBA</MANUFACTURER>
    <MAKE>TOSHIBA</MAKE>
    <DISTRIBUTOR>TOSHIBA</DISTRIBUTOR>
    <MODEL>MEUXXX</MODEL>
    <SECURITYLEVEL>2000</SECURITYLEVEL>
    <HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
    <HARDWARE_VER_MINOR>1</HARDWARE_VER_MINOR>
    <FIRMWARE_VER_MAJOR>2</FIRMWARE_VER_MAJOR>
    <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
    <FEATURES>
        <CLOCK>2</CLOCK>
        <SECURECLOCK>
            <URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
           
<PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY>
        </SECURECLOCK>
        <METERING>1</METERING>
        <LICENSE_ACQ>0</LICENSE_ACQ>
        <LICENSE_SYNC>1</LICENSE_SYNC>
        <ENCRYPTION>1</ENCRYPTION>
        <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
    </FEATURES>
    <LIMITS>
        <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
        <MAXLICENSESIZE>10240</MAXLICENSESIZE>
        <MAXHEADERSIZE>5120</MAXHEADERSIZE>
   
</LIMITS><PUBLICKEY>jEnTBNEUdeNO9vCxAeCzL6CdI3pkE4IR1wl6p70Ixx/5m+qG+96pPg==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>WlcEK0NKu2YXWhBWnWJCQAROs4PshdCTEevBxyaG1qwj5WheXVWfDg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>1621</AUTH_ID><PUBLICKEY>3EzYMThGosXetNLAQgw9jxk2tl1h2e869W48bnEW+T13t5udtnZdeg==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>0ZMunnXroTdVa0ioUHlqlgCBWYDk8w9g+iV9MKrSDlBKbTqe+WaVPg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>1zim2b/my9FrK2roZlRmiyqYvh+1pbtIM01HGLR+KWovel+XSgbAMg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
Segmentation fault (core dumped)
