libmtp version: 0.3.4

Listing raw device(s)
   Found 1 device(s):
   0781:7434 @ bus 0, dev 27
Attempting to connect device(s)
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0781
   idProduct: 7434
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 0
      Device number: 27
      Device entry info:
         Vendor: (null)
         Vendor id: 0x0781
         Product: (null)
         Vendor id: 0x7434
         Device flags: 0x00000000
Microsoft device descriptor 0xee:
	0000: 1203 4d00 5300 4600 5400 3100 3000 3000	..M.S.F.T.1.0.0.
	0010: fe00                                   	..
Microsoft device response to control message 1, CMD 0xfe:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Microsoft device response to control message 2, CMD 0xfe:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Device info:
   Manufacturer: SanDisk
   Model: Sansa Clip 2GB
   Device version: v02.01.16A
   Serial number: 0C0FDF0A7009B6A80000000000000000
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com/WMDRMPD: 10.1; audible.com: 1.0; microsoft.com/WMDRMND: 1.0; microsoft.com/AAVT: 1.0; microsoft.com: WMPPD10.0; 
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1012: Set object protection
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   101b: Get partial object
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   9170: Open Media Session
   9171: Close Media Session
   9172: Get Next Data Block
   9173: Set Current Time Position
   9180: Send Registration Request
   9181: Get Registration Response
   9182: Get Proximity Challenge
   9183: Send Proximity Response
   9184: Send WMDRM-ND License Request
   9185: Get WMDRM-ND License Response
   9201: Report Added/Deleted Items
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9810: Get object references
   9811: Set object references
Events supported:
   None.
Device Properties Supported:
   0x5001: Battery Level
   0x5002: Functional Mode
   0xd100: Unknown property
   0xd101: Secure Time
   0xd102: Device Certificate
   0xd103: Revocation Info
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
Playable File (Object) Types and Object Properties Supported:
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
   3008: MS Wave
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 1, 17,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
   3009: MP3
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 85,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
   300c: ASF
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 353,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
   b301: Unknown(b301)
      da00: unknown(da00) UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8,  GET/SET
      da01: unknown(da01) STRING data type GET/SET
      da02: unknown(da02) UINT32 data type ANY 32BIT VALUE form READ ONLY
      da03: unknown(da03) UINT16 data type enumeration: 0, 1,  READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
   b901: WMA
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 352, 353, 354,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
   b902: OGG
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
   b904: Audible.com Codec
      da00: unknown(da00) UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8,  GET/SET
      da01: unknown(da01) STRING data type GET/SET
      da02: unknown(da02) UINT32 data type ANY 32BIT VALUE form READ ONLY
      da03: unknown(da03) UINT16 data type enumeration: 0, 1,  READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
   b906: FLAC
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
   ba03: Abstract Audio Album
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
   ba05: Abstract Audio Video Playlist
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
   ba11: M3U Playlist
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 2016641024
      FreeSpaceInBytes: 532971520
      FreeSpaceInObjects: 4294967295
      StorageDescription: Internal Memory
      VolumeIdentifier: 0C0FDF0A7009B6A8
Special directories:
   Default music folder: 0x00000001
   Default playlist folder: 0x00000002
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000017
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: Sansa Clip 2GB
   Synchronization partner: {00000000-0000-0000-0000-000000000000}
   Battery level 97 of 100 (97%)
libmtp supported (playable) filetypes:
   RIFF WAVE file
   ISO MPEG-1 Audio Layer 3
   Microsoft Advanced Systems Format
   Microsoft Windows Media Audio
   Ogg container format
   Audible.com Audio Codec
   Free Lossless Audio Codec (FLAC)

Secure Time:
<DRMCLOCK type="status"><VALUE>#20090105 21:49:36Z#</VALUE><FLAG>DRM_CLK_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">MABDADAARgBEAEYAMABBADcAMAAwADkAQgA2AEEAOAAwADAAMAAwADAAMAAwADAAMAAwADAAMAAwADAAMAAwAA==</UNIQUEID><PUBLICKEY private="1">fhUC+/QijZ/4rUaDrjis1u0VTG5/bJl/46yNsxAyIQQ9rcg0sGkiUA==</PUBLICKEY><KEYDATA>YmaVekpKkEb9bDxe1toOZw2O6Uo=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>iwNk1uAtpMkytF5Cc1Esx5f7xk82LibzXPwO7ZRJT0Ot9eFX3INVEA==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>yLTRrx6Ilr/MuhHIxv82IuKBxG4=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.111.35</SECURITYVERSION><CERTIFICATE private="1">fhUC+/QijZ/4rUaDrjis1u0VTG5/bJl/46yNsxAyIQQ9rcg0sGkiUAIEbyP83FohB+KBhkYAwiS/SOCjTHfkW/zfd2w2pnPvOC99wum+X8R1LVQR</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>Clip+</NAME>
	<MANUFACTURER>SanDisk Corporation</MANUFACTURER>
	<MAKE>Sansa</MAKE>
	<MODEL>Sansa Clip+</MODEL>
	<SECURITYLEVEL>2000</SECURITYLEVEL>
	<HARDWARE_VER_MAJOR>2</HARDWARE_VER_MAJOR>
	<HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR>
	<FIRMWARE_VER_MAJOR>0</FIRMWARE_VER_MAJOR>
	<FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>

	<SECURITYLEVEL>2000</SECURITYLEVEL>

	<FEATURES>
		<CLOCK>2</CLOCK>
		<SECURECLOCK>
			<URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
			<PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY>
		</SECURECLOCK>

		<METERING>1</METERING>
		<LICENSE_ACQ>1</LICENSE_ACQ>
		<LICENSE_SYNC>1</LICENSE_SYNC>
		<ENCRYPTION>1</ENCRYPTION>
		<SYMMETRIC_OPT>1</SYMMETRIC_OPT>

		<SUPPORT_REVOCATION>
			<GUID>{CD75E604-543D-4A9C-9F09-FE6D24E8BF90}</GUID>
		</SUPPORT_REVOCATION>

	</FEATURES>

	<LIMITS>
		<MAXCHAINDEPTH>2</MAXCHAINDEPTH>
		<MAXLICENSESIZE>10240</MAXLICENSESIZE>
		<MAXHEADERSIZE>5120</MAXHEADERSIZE>
	</LIMITS><PUBLICKEY>VbOg1CGbCRQuQmDdJu7VEbVObj8xxTz3DBkj0I4qX2430HWlCWuleQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>k7W8US0uNGzlL2TKDWcMHhQEMkAKPp0QSU+cu0DuuPxJ3p6HUYaDZA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>2695</AUTH_ID><PUBLICKEY>3JwjYFj2GuZrhCAshbYFNjgb9g2pl2j0nR8PR2rqyk4iIARZrN4GOQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>U/0OkXwkzkCBmOyuE9BAnxs3yHuGodfnpw/QyqUfVc2GbN2EP41OCQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>iCWGAEStZdbKH1OYrXLqSnMBZQOBx6P4mVnYKKu94Zq2ohh00BQlGA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>

Device description WMPInfo.xml file:
<DeviceInfo>
    <WMP DeviceID="{DE25BD8B-0F7E-4DA2-A3DD-52BDE52DF67F}" RelationshipID="{00000000-0000-0000-0000-000000000000}"/>
</DeviceInfo>

OK.

 	  	 
