
libmtp version: 0.2.6.1

Attempting to connect device(s)
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 255
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 1302
   idProduct: 1017
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000000
Microsoft device descriptor 0xee:
        0000: 1203 4d00 5300 4600 5400 3100 3000 3000   ..M.S.F.T.1.0.0.
        0010: 3100                                      1.
Microsoft device response to control message 1, CMD 0x31:
        0000: 2800 0000 0001 0400 0100 0000 0000 0000   (...............
        0010: 0001 4d54 5000 0000 0000 0000 0000 0000   ..MTP...........
        0020: 0000 0000 0000 0000                       ........
Microsoft device response to control message 2, CMD 0x31:
        0000: 2800 0000 0001 0400 0100 0000 0000 0000   (...............
        0010: 0001 4d54 5000 0000 0000 0000 0000 0000   ..MTP...........
        0020: 0000 0000 0000 0000                       ........
Device info:
   Manufacturer: Haier
   Model: ibiza Rhapsody
   Device version: LB.2.5.8.27806
   Serial number: 021C020340053B000000000000000000
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMPPD: 10.0; microsoft.com/WMDRMPD: 10.1; audible.com: 1.0
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   101b: Get partial object
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   9201: Report Added/Deleted Items
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9810: Get object references
   9811: Set object references
Events supported:
   0x4002
   0x4003
   0x4004
   0x4005
   0x4006
   0x4007
   0x4008
   0x400a
   0x400b
   0x400c
Device Properties Supported:
   0xd101: Secure Time
   0xd102: Device Certificate
   0xd402: Friendly Device Name
   0xd405: Device Icon
   0xd100: Unknown property
Playable File (Object) Types and Object Properties Supported:
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
   3008: MS Wave
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 65535, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: AudioBitDepth UINT32 data type enumeration: 8, 16,  READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 352, 353,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 384000, STEP 1 READ ONLY
   3009: MP3
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 65535, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: AudioBitDepth UINT32 data type enumeration: 8, 16,  READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 85,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 384000, STEP 1 READ ONLY
   300a: MS AVI
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc87: Width UINT32 data type range: MIN 16, MAX 320, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 16, MAX 240, STEP 1 READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 65535, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: AudioBitDepth UINT32 data type enumeration: 8, 16,  READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 352, 353,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 384000, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 1446269005, 875967048,  READ ONLY
      dea1: EncodingProfile STRING data type GET/SET
   300c: ASF
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc87: Width UINT32 data type range: MIN 16, MAX 320, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 16, MAX 240, STEP 1 READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 65535, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: AudioBitDepth UINT32 data type enumeration: 8, 16,  READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 352, 353,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 384000, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 1446269005, 875967048,  READ ONLY
      dea1: EncodingProfile STRING data type GET/SET
   3801: JPEG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
   380b: PNG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
   b301: Unknown(b301)
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      da00: unknown(da00) UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9,  GET/SET
      da01: unknown(da01) STRING data type GET/SET
      da02: unknown(da02) UINT32 data type ANY 32BIT VALUE form GET/SET
      da03: unknown(da03) UINT32 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 65535, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: AudioBitDepth UINT32 data type enumeration: 8, 16,  READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 352, 353,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 384000, STEP 1 READ ONLY
   b802: Firmware
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
   b901: WMA
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 65535, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: AudioBitDepth UINT32 data type enumeration: 8, 16,  READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 352, 353,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 384000, STEP 1 READ ONLY
   b903: AAC
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 65535, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: AudioBitDepth UINT32 data type enumeration: 8, 16,  READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 352, 353,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 384000, STEP 1 READ ONLY
   b904: Audible.com Codec
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      da00: unknown(da00) UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9,  GET/SET
      da01: unknown(da01) STRING data type GET/SET
      da02: unknown(da02) UINT32 data type ANY 32BIT VALUE form GET/SET
      da03: unknown(da03) UINT32 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 65535, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: AudioBitDepth UINT32 data type enumeration: 8, 16,  READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 352, 353,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 384000, STEP 1 READ ONLY
   b981: WMV
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc87: Width UINT32 data type range: MIN 16, MAX 320, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 16, MAX 240, STEP 1 READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 65535, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: AudioBitDepth UINT32 data type enumeration: 8, 16,  READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 352, 353,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 384000, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 827739479, 844516695, 861293911,  READ ONLY
      dea1: EncodingProfile STRING data type GET/SET
   b982: MP4
      d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc42: SyncID STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc87: Width UINT32 data type range: MIN 16, MAX 320, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 16, MAX 240, STEP 1 READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc8a: Rating UINT16 data type range: MIN 0, MAX 65535, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      de95: AudioBitDepth UINT32 data type enumeration: 8, 16,  READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 352, 353,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 384000, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 1446269005, 875967048,  READ ONLY
      dea1: EncodingProfile STRING data type GET/SET
   ba03: Abstract Audio Album
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,  READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 65536, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1024, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1024, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
   ba14: PLS Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 3734740992
      FreeSpaceInBytes: 3400687616
      FreeSpaceInObjects: 4294967295
      StorageDescription: Device Storage
      VolumeIdentifier: (null)
Special directories:
   Default music folder: 0x0000001a
   Default playlist folder: 0x0000001d
   Default picture folder: 0x0000001c
   Default video folder: 0x0000001b
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: 
   Synchronization partner: (NULL)
libmtp supported (playable) filetypes:
   RIFF WAVE file
   ISO MPEG-1 Audio Layer 3
   Audio Video Interleave
   Microsoft Advanced Systems Format
   JPEG file
   Portable Network Graphics
   Firmware file
   Microsoft Windows Media Audio
   Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
   Audible.com Audio Codec
   Microsoft Windows Media Video
   MPEG-4 Part 14 Container Format (Audio+Video Empahsis)
