libmtp version: 1.1.1

Listing raw device(s)
   Found 1 device(s):
   Cowon: iAudio 10 (MTP mode) (0e21:0952) @ bus 1, dev 18
Attempting to connect device(s)
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0e21
   idProduct: 0952
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 1
      Device number: 18
      Device entry info:
         Vendor: Cowon
         Vendor id: 0x0e21
         Product: iAudio 10 (MTP mode)
         Vendor id: 0x0952
         Device flags: 0x01000206
Device info:
   Manufacturer: COWON SYSTEMS, Inc.
   Model: iAUDIO 10
   Device version: 1.06
   Serial number: 06250000000000001130091042120266
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com/WMPPD: 11.0;microsoft.com/WMDRMPD: 10.1;microsoft.com/WMPPD: 10.0;audible.com: 1.0;microsoft.com/AAVT: 1.0;microsoft.com/WMDRMND: 1.0;
   Detected object size: 64 bits
   Extensions:
        microsoft.com/WMPPD: 11.0
        microsoft.com/WMDRMPD: 10.1
        microsoft.com/WMPPD: 10.0
        audible.com: 1.0
        microsoft.com/AAVT: 1.0
        microsoft.com/WMDRMND: 1.0
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   9808: Send object property list
   100c: Send object info
   100d: Send object
   100f: Format storage
   1010: Reset device
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   9810: Get object references
   9811: Set object references
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   101b: Get partial object
   9201: Report Added/Deleted Items
   9202: Report Acquired Items
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   9170: Open Media Session
   9171: Close Media Session
   9172: Get Next Data Block
   9173: Set Current Time Position
   9180: Send Registration Request
   9181: Get Registration Response
   9182: Get Proximity Challenge
   9183: Send Proximity Response
   9184: Send WMDRM-ND License Request
   9185: Get WMDRM-ND License Response
Events supported:
   0x4004
   0x4005
Device Properties Supported:
   0xd405: Device Icon
   0xd100: Unknown property
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd101: Secure Time
   0xd102: Device Certificate
   0xd103: Revocation Info
Playable File (Object) Types and Object Properties Supported:
   3001: Association/Directory
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
   3009: MP3
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
   b901: WMA
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 320000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
   3008: MS Wave
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
   b904: Audible.com Codec
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      da00: Unknown property UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9,  GET/SET
      da02: Unknown property UINT32 data type ANY 32BIT VALUE form READ ONLY
      da03: Unknown property UINT16 data type enumeration: 0, 1,  READ ONLY
      da01: Unknown property STRING data type GET/SET
      da04: Unknown property array of UINT8 data type ANY 8BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
   b301: Unknown(b301)
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      da00: Unknown property UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9,  GET/SET
      da02: Unknown property UINT32 data type ANY 32BIT VALUE form READ ONLY
      da03: Unknown property UINT16 data type enumeration: 0, 1,  READ ONLY
      da01: Unknown property STRING data type GET/SET
      da04: Unknown property array of UINT8 data type ANY 8BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
   3801: JPEG
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 1, MAX 270, STEP 1 GET/SET
   3004: Text
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
   300a: MS AVI
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 1, MAX 270, STEP 1 GET/SET
      de97: Scan Depth UINT16 data type enumeration: 1,  READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type enumeration:  GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 1195724877, 861293911,  GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 850000, STEP 1 GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      dea1: Encoding Profile STRING data type GET/SET
   b981: WMV
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 1, MAX 270, STEP 1 GET/SET
      de97: Scan Depth UINT16 data type enumeration: 1,  READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type enumeration:  GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 1195724877, 861293911,  GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 850000, STEP 1 GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 128000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      dea1: Encoding Profile STRING data type GET/SET
   b903: AAC
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 268435456, STEP 1 GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
   300c: ASF
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc87: Width UINT32 data type range: MIN 1, MAX 480, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 1, MAX 270, STEP 1 GET/SET
      de97: Scan Depth UINT16 data type enumeration: 1,  READ ONLY
      de9d: Frames Per Thousand Seconds UINT32 data type enumeration:  GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 1195724877, 861293911,  GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 1, MAX 850000, STEP 1 GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: Sample Rate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      dea1: Encoding Profile STRING data type GET/SET
   3001: Association/Directory
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
   ba05: Abstract Audio Video Playlist
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
   3000: Undefined Type
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
   b802: Firmware
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
   ba03: Abstract Audio Album
      dc44: Name STRING data type GET/SET
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: Buy flag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
      dc81: Representative Sample Format UINT16 data type enumeration: 14337,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc9b: Album Artist STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 32908689408
      FreeSpaceInBytes: 30113251328
      FreeSpaceInObjects: 23663
      StorageDescription: Internal Storage
      VolumeIdentifier: 06250000000000001130091042120266
Special directories:
   Default music folder: 0x2000000d
   Default playlist folder: 0xffffffff
   Default picture folder: 0x20000009
   Default video folder: 0x2000000f
   Default organizer folder: 0xffffffff
   Default zencast folder: 0xffffffff
   Default album folder: 0xffffffff
   Default text folder: 0xffffffff
MTP-specific device properties:
   Friendly name: iAUDIO 10
   Synchronization partner: Longhorn Sync Engine
   Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
   Folder
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   RIFF WAVE file
   Audible.com Audio Codec
   JPEG file
   Text file
   Audio Video Interleave
   Microsoft Windows Media Video
   Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
   Microsoft Advanced Systems Format
   Folder
   Abstract Playlist file
   Firmware file
   Abstract Album file
   Ogg container format
   Free Lossless Audio Codec (FLAC)

Secure Time:
<DRMCLOCK type="status"><VALUE>#20091116 77:40:12Z#</VALUE><FLAG>DRM_CLK_NEEDS_REFRESH</FLAG></DRMCLOCK>AG></DRMCLOCK>
OK.
