libmtp version: 0.2.0

Attempting to connect device(s)
Detect: Successfully connected 1 devices
USB low-level info:
  Using kernel interface "usbfs"
  bcdUSB: 512
  bDeviceClass: 255
  bDeviceSubClass: 0
  bDeviceProtocol: 0
  idVendor: 0421
  idProduct: 04e1
  IN endpoint maxpacket: 64 bytes
  OUT endpoint maxpacket: 64 bytes
  Device flags: 0x00000000
Device info:
  Manufacturer: Nokia
  Model: Nokia N75
  Device version: v. 1.00
  Serial number: ###############
  Vendor extension ID: 0x00000006
  Vendor extension description: microsoft.com:1.0;microsoft.com/WMPPD: 11.0;microsoft.com/WMDRMPD: 10.1
Supported operations:
  1001: get device info
  1002: Open session
  1003: Close session
  1004: Get storage IDs
  1005: Get storage info
  1006: Get number of objects
  1007: Get object handles
  1008: Get object info
  1009: Get object
  100b: Delete object
  100c: Send object info
  100d: Send object
  1010: Reset device
  1014: Get device property description
  1015: Get device property value
  1016: Set device property value
  9801: Get object properties supported
  9802: Get object property description
  9803: Get object property value
  9804: Set object property value
  9810: Get object references
  9811: Set object references
  9201: Report Added/Deleted Items
  9202: Report Acquired Items
  9203: Get type of playlists that are allowed to be transfered
  9101: Get secure time challenge
  9102: Get secure time response
  9103: Set license response
  9104: Get sync list
  9105: Send meter challenge query
  9106: Get meter challenge
  9107: Get meter response
  9108: Clean data store
  9109: Get license state
  910a: Send WMDRM-PD Command
  910b: Send WMDRM-PD Request
Events supported:
  0x400a
  0x4004
  0x4005
Device Properties Supported:
  0xd401: Synchronization Partner
  0xd402: Device Friendly Name
  0xd404: Unknown property
  0xd102: Device Certificate
  0xd101: Secure Time
Playable File (Object) Types and Object Properties Supported:
  3000: Undefined Type
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc4e: DateAdded STRING data type READ ONLY
     dc08: DateCreated STRING data type READ ONLY
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
  3001: Association/Directory
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc4e: DateAdded STRING data type READ ONLY
     dc08: DateCreated STRING data type READ ONLY
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
  b903: AAC
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc4e: DateAdded STRING data type READ ONLY
     dc08: DateCreated STRING data type READ ONLY
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
     dc46: Artist STRING data type GET/SET
     dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc96: Composer STRING data type GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
     dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
     de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 41222,  READ ONLY
  b982: MP4
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc4e: DateAdded STRING data type READ ONLY
     dc08: DateCreated STRING data type READ ONLY
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
     dc46: Artist STRING data type GET/SET
     dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc96: Composer STRING data type GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
     dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 16000, MAX 576000, STEP 1 READ ONLY
     de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 41222,  READ ONLY
  3009: MP3
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc4e: DateAdded STRING data type READ ONLY
     dc08: DateCreated STRING data type READ ONLY
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
     dc46: Artist STRING data type GET/SET
     dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc96: Composer STRING data type GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
     dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
     de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 85,  READ ONLY
  b004: Unknown(b004)
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc4e: DateAdded STRING data type READ ONLY
     dc08: DateCreated STRING data type READ ONLY
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
     dc46: Artist STRING data type GET/SET
     dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc96: Composer STRING data type GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
     dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 16000, MAX 576000, STEP 1 READ ONLY
     de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 1, 85, 41222,  READ ONLY
  b982: MP4
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc4e: DateAdded STRING data type READ ONLY
     dc08: DateCreated STRING data type READ ONLY
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
     dc46: Artist STRING data type GET/SET
     dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc96: Composer STRING data type GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
     dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 16000, MAX 576000, STEP 1 READ ONLY
     de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 41222,  READ ONLY
  b901: WMA
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc4e: DateAdded STRING data type READ ONLY
     dc08: DateCreated STRING data type READ ONLY
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
     dc46: Artist STRING data type GET/SET
     dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc96: Composer STRING data type GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
     dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 384000, STEP 1 READ ONLY
     de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 352, 353,  READ ONLY
  300c: ASF
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc4e: DateAdded STRING data type READ ONLY
     dc08: DateCreated STRING data type READ ONLY
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
     dc46: Artist STRING data type GET/SET
     dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc96: Composer STRING data type GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
     dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 384000, STEP 1 READ ONLY
     de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 352, 353,  READ ONLY
  ba11: M3U Playlist
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc4e: DateAdded STRING data type READ ONLY
     dc08: DateCreated STRING data type READ ONLY
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
  ba05: Abstract Audio Video Playlist
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc4e: DateAdded STRING data type READ ONLY
     dc08: DateCreated STRING data type READ ONLY
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
  3008: MS Wave
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc04: ObjectSize UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc07: ObjectFileName STRING data type GET/SET
     dc4e: DateAdded STRING data type READ ONLY
     dc08: DateCreated STRING data type READ ONLY
     dc09: DateModified STRING data type READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc44: Name STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
     dc46: Artist STRING data type GET/SET
     dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc8c: Genre STRING data type GET/SET
     dc96: Composer STRING data type GET/SET
     dc99: OriginalReleaseDate STRING data type GET/SET
     dc9a: AlbumName STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
     dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 16000, MAX 1536000, STEP 1 READ ONLY
     de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 1,  READ ONLY
Storage Devices:
  StorageID: 0x00040001
     StorageType: 0x0004
     FilesystemType: 0x0002
     AccessCapability: 0x0000
     MaxCapacity: 252837888
     FreeSpaceInBytes: 207028224
     FreeSpaceInObjects: 98
     StorageDescription: Memory card
     VolumeIdentifier: 2979423943
Special directories:
  Default music folder: 0x0075a438
  Default playlist folder: 0x0075aff8
  Default picture folder: 0x00000000
  Default video folder: 0x00000000
  Default organizer folder: 0x00000000
  Default zencast folder: 0x00000000
  Default album folder: 0x00000000
  Default text folder: 0x00000000
MTP-specific device properties:
  Friendly name: Nokia N75
  Synchronization partner: Nokia N75
libmtp supported (playable) filetypes:
  Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
  MPEG-4 Part 14 Container Format (Audio+Video Empahsis)
  ISO MPEG-1 Audio Layer 3
  MPEG-4 Part 14 Container Format (Audio+Video Empahsis)
  Microsoft Windows Media Audio
  Microsoft Advanced Systems Format
  RIFF WAVE file

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">MAAwADQANAAwADAAOQA4ADEANwAwADIAMwAzADMA</UNIQUEID><PUBLICKEY private="1">yfU5i9JAJj8US/NBG9610tzxBEu9WtjY001laPckGolXV6IxVLOpfg==</PUBLICKEY><KEYDATA>AEPx+IjlAAnc9wj/jJMFXOpg5jM=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>fWlj8yrfDFRih3OQc10B2dxsNmxTqPr5KJFFcVcsmw2sSTlx1meCRQ==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>oHBlLp43JLsai1sOfHN+KNd2e+Y=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.105.85</SECURITYVERSION><CERTIFICATE private="1">yfU5i9JAJj8US/NBG9610tzxBEu9WtjY001laPckGolXV6IxVLOpfgIEaVWtMScbzr2guqSZfn4vjUWI9KhARpZcOmlZxtwny3HGe1MpX73rJERU</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>N75</NAME>
   <MANUFACTURER>Nokia</MANUFACTURER>
   <MAKE>Nokia</MAKE>
   <DISTRIBUTOR>Nokia</DISTRIBUTOR>
   <MODEL>RM-128</MODEL>
   <SECURITYLEVEL>2000</SECURITYLEVEL>
   <HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
   <HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR>
   <FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR>
   <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
   <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
   <FEATURES>
       <CLOCK>1</CLOCK>
       <METERING>1</METERING>
       <LICENSE_ACQ>0</LICENSE_ACQ>
       <LICENSE_SYNC>1</LICENSE_SYNC>
       <ENCRYPTION>1</ENCRYPTION>
       <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
   </FEATURES>
   <LIMITS>
       <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
       <MAXLICENSESIZE>10240</MAXLICENSESIZE>
       <MAXHEADERSIZE>5120</MAXHEADERSIZE>
   </LIMITS><PUBLICKEY>HSgky5T25DpZKVVAJO4tzlaysU1EupWfAd8pQpJbZAC6gH7j+UoZRw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>+GIvCXGxfo+fpXKNhpMpTUbqRFW0ddztNJ8Vd1/rfTdaJSqBCnLkDQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>1209</AUTH_ID><PUBLICKEY>lLaXP6uCtehdnMt3Upymhj/pKkXvgNCeb8xghGDSK5yBmzwjqV+OXg==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>e8WHZkxrP8ucd0bIbEGVJygnzkTWH/Bg3HP7s3ZDIu4wYH+OG1UnOA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>eLFzvX7Lqc105oN4RckF2KA5nEhSYGUovUwmXEKdUgsEYWYOXlLDUQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
