libmtp version: 1.1.11

Listing raw device(s)
   Found 1 device(s):
   Jolla: Jolla (2931:0a07) @ bus 2, dev 10
Attempting to connect device(s)
USB low-level info:
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 2931
   idProduct: 0a07
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 2
      Device number: 10
      Device entry info:
         Vendor: Jolla
         Vendor id: 0x2931
         Product: Jolla
         Vendor id: 0x0a07
         Device flags: 0x00000000
Configuration 0, interface 0, altsetting 0:
   Interface description contains the string "MTP"
   Device recognized as MTP, no further probing.
Device info:
   Manufacturer: Jolla
   Model: Jolla
   Device version: 2.0.1.11 HW: 1.0.0.17
   Serial number: 359745050206470
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com:1.0; microsoft.com/WMPPD:11.0; 
   Detected object size: 64 bits
   Extensions:
        microsoft.com: 1.0
        microsoft.com/WMPPD: 11.0
Supported operations:
   1001: Unknown(1001)
   1002: Unknown(1002)
   1003: Unknown(1003)
   1004: Unknown(1004)
   1005: Unknown(1005)
   1006: Unknown(1006)
   1007: Unknown(1007)
   1008: Unknown(1008)
   1009: Unknown(1009)
   100b: Unknown(100b)
   100c: Unknown(100c)
   100d: Unknown(100d)
   1014: Unknown(1014)
   1015: Unknown(1015)
   1016: Unknown(1016)
   1019: Unknown(1019)
   101a: Unknown(101a)
   101b: Unknown(101b)
   9801: Unknown(9801)
   9802: Unknown(9802)
   9803: Unknown(9803)
   9804: Unknown(9804)
   9805: Unknown(9805)
   9806: Unknown(9806)
   9808: Unknown(9808)
   9810: Unknown(9810)
   9811: Unknown(9811)
Events supported:
   0x4002
   0x4003
   0x4007
   0xc801
   0x4004
   0x4005
   0x400a
   0x4009
   0x400c
   0x4008
   0x4006
Device Properties Supported:
   0x5001: Battery Level
   0xd402: Friendly Device Name
   0xd401: Synchronization Partner
   0x501f: Copyright Info
   0xd407: Perceived Device Type
   0xd405: Device Icon
   0xd403: Volume Level
Playable File (Object) Types and Object Properties Supported:
   3801: JPEG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14344, 14347,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
   3807: GIF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14344, 14347,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
   380b: PNG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14344, 14347,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
   380d: TIFF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14344, 14347,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
   3804: BMP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14344, 14347,  READ ONLY
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc86: Representative Sample Data array of UINT8 data type byte array:  READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX 5000, STEP 1 READ ONLY
   3008: MS Wave
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
   3009: MP3
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
   b901: WMA
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
   b902: OGG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
   b903: AAC
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de92: Bit Rate Type UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
   300a: MS AVI
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 1920, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 1080, STEP 1 GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 1145656899, 1162629709, 827544397, 827739479, 861293911, 875967048,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 100000, STEP 1 GET/SET
   300b: MPEG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 1920, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 1080, STEP 1 GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 1145656899, 1162629709, 827544397, 827739479, 861293911, 875967048,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 100000, STEP 1 GET/SET
   b984: 3GP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 1920, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 1080, STEP 1 GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 1145656899, 1162629709, 827544397, 827739479, 861293911, 875967048,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 100000, STEP 1 GET/SET
   b982: MP4
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 1920, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 1080, STEP 1 GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 1145656899, 1162629709, 827544397, 827739479, 861293911, 875967048,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 100000, STEP 1 GET/SET
   b981: WMV
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 1920, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 1080, STEP 1 GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc9d: DRM Status UINT16 data type enumeration: 0, 1,  GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 22050, 44000, 44100, 48000,  GET/SET
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 6, 7, 85, 352, 353, 354, 16897, 41222, 34,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 1145656899, 1162629709, 827544397, 827739479, 861293911, 875967048,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 100000, STEP 1 GET/SET
   3000: Undefined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   3001: Association/Directory
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   3004: Text
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   3005: HTML
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   ba03: Abstract Audio Album
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   ba05: Abstract Audio Video Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   bb82: vCard2
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   bb83: vCard3
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
   be02: vCalendar1
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type GET/SET
      dc08: Date Created STRING data type DATETIME FORM READ ONLY
      dc09: Date Modified STRING data type DATETIME FORM READ ONLY
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  READ ONLY
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 14761832448
      FreeSpaceInBytes: 9813463040
      FreeSpaceInObjects: 4294967295
      StorageDescription: Mass storage
      VolumeIdentifier: media
Special directories:
   Default music folder: 0xffffffff
   Default playlist folder: 0xffffffff
   Default picture folder: 0xffffffff
   Default video folder: 0xffffffff
   Default organizer folder: 0xffffffff
   Default zencast folder: 0xffffffff
   Default album folder: 0xffffffff
   Default text folder: 0xffffffff
MTP-specific device properties:
   Friendly name: Sailfish
   Synchronization partner: Sailfish
   Battery level 0 of 100 (0%)
libmtp supported (playable) filetypes:
   JPEG file
   GIF bitmap file
   Portable Network Graphics
   TIFF bitmap file
   BMP bitmap file
   RIFF WAVE file
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   Ogg container format
   Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
   Audio Video Interleave
   MPEG video stream
   MPEG-4 Part 14 Container Format (Audio+Video Emphasis)
   Microsoft Windows Media Video
   Folder
   Text file
   HTML file
   Abstract Album file
   Abstract Playlist file
   VCard version 2
   VCard version 3
   VCalendar version 1
OK.
