$ mtp-detect
libmtp version: 0.2.1

Attempting to connect device(s)
Detect: Successfully connected 1 devices
USB low-level info:
  Using kernel interface "usbfs"
  bcdUSB: 512
  bDeviceClass: 255
  bDeviceSubClass: 0
  bDeviceProtocol: 0
  idVendor: 0930
  idProduct: 0010
  IN endpoint maxpacket: 512 bytes
  OUT endpoint maxpacket: 512 bytes
  Device flags: 0x00000001
Microsoft device descriptor 0xee:
       0000: 1203 4d00 5300 4600 5400 3100 3000 3000   ..M.S.F.T.1.0.0.
       0010: fe00                                      ..
Microsoft device response to control message 1, CMD 0xfe:
       0000: 2800 0000 0001 0400 0100 0000 0000 0000   (...............
       0010: 0001 4d54 5000 0000 0000 0000 0000 0000   ..MTP...........
       0020: 0000 0000 0000 0000                       ........
Device info:
  Manufacturer: TOSHIBA
  Model: gigabeat S
  Device version: PMC: 2.11 (632:1400); Platform: 1.1 (632.4)
  Serial number: 3c98dbd8 - d0a2274e - 80bd1ff8 - 8ee00652
  Vendor extension ID: 0x00000006
  Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 11.1; microsoft.com/WMPMCPREMCONT: 1.0
Supported operations:
  1001: get device info
  1002: Open session
  1003: Close session
  1004: Get storage IDs
  1005: Get storage info
  1006: Get number of objects
  1007: Get object handles
  1008: Get object info
  1009: Get object
  100b: Delete object
  100c: Send object info
  100d: Send object
  100f: Format storage
  1010: Reset device
  1014: Get device property description
  1015: Get device property value
  1016: Set device property value
  1019: Move object
  101b: Get partial object
  9810: Get object references
  9811: Set object references
  9802: Get object property description
  9807: Get interdependent property description
  9801: Get object properties supported
  9803: Get object property value
  9804: Set object property value
  9805: Get object property list
  9806: Set object property list
  9808: Send object property list
  9101: Get secure time challenge
  9102: Get secure time response
  9103: Set license response
  9104: Get sync list
  9105: Send meter challenge query
  9106: Get meter challenge
  9107: Get meter response
  9108: Clean data store
  9109: Get license state
  910a: Send WMDRM-PD Command
  910b: Send WMDRM-PD Request
  9201: Report Added/Deleted Items
  9202: Report Acquired Items
  9204: Unknown (9204)
Events supported:
  None.
Device Properties Supported:
  0xd181: Unknown property
  0xd101: Secure Time
  0xd401: Synchronization Partner
  0x5001: Battery Level
  0xd102: Device Certificate
  0xd402: Friendly Device Name
  0xd131: PlaysForSure ID
Playable File (Object) Types and Object Properties Supported:
  3009: MP3
     dc44: Name STRING data type GET/SET
     dc04: ObjectSize UINT64 data type READ ONLY
     dc08: DateCreated STRING data type GET/SET
     dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
     dc09: DateModified STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc0a: Keywords STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc07: ObjectFileName STRING data type GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 550000, STEP 1 READ ONLY
     dc9a: AlbumName STRING data type READ ONLY
     dc46: Artist STRING data type GET/SET
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8c: Genre STRING data type GET/SET
     dc95: MetaGenre UINT16 data type ANY 16BIT VALUE form GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 85,  READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
  b901: WMA
     dc44: Name STRING data type GET/SET
     dc04: ObjectSize UINT64 data type READ ONLY
     dc08: DateCreated STRING data type GET/SET
     dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
     dc09: DateModified STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc0a: Keywords STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc07: ObjectFileName STRING data type GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 1572864, STEP 1 READ ONLY
     dc9a: AlbumName STRING data type READ ONLY
     dc46: Artist STRING data type GET/SET
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8c: Genre STRING data type GET/SET
     dc95: MetaGenre UINT16 data type ANY 16BIT VALUE form GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 353, 355, 10,  READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
  3008: MS Wave
     dc44: Name STRING data type GET/SET
     dc04: ObjectSize UINT64 data type READ ONLY
     dc08: DateCreated STRING data type GET/SET
     dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
     dc09: DateModified STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc0a: Keywords STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc07: ObjectFileName STRING data type GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     d901: BuyFlag UINT8 data type enumeration: 0, 1,  GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 1572864, STEP 1 READ ONLY
     dc9a: AlbumName STRING data type READ ONLY
     dc46: Artist STRING data type GET/SET
     dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
     dc8c: Genre STRING data type GET/SET
     dc95: MetaGenre UINT16 data type ANY 16BIT VALUE form GET/SET
     dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
     de93: SampleRate UINT32 data type range: MIN 4000, MAX 48000, STEP 50 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 353, 85, 1, 2, 6, 17, 49,  READ ONLY
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
  300c: ASF
     da84: unknown(da84) STRING data type GET/SET
     dc44: Name STRING data type GET/SET
     dc04: ObjectSize UINT64 data type READ ONLY
     dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
     dc08: DateCreated STRING data type GET/SET
     dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
     dc09: DateModified STRING data type GET/SET
     de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 READ ONLY
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc0a: Keywords STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
     dc47: DateAuthored STRING data type GET/SET
     dc07: ObjectFileName STRING data type GET/SET
     da82: unknown(da82) UINT8 data type ANY 8BIT VALUE form GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc4b: CopyrightInformation array of UINT16 data type ANY 16BIT VALUE form GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dea1: EncodingProfile STRING data type READ ONLY
     da81: unknown(da81) STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     da83: unknown(da83) UINT32 data type ANY 32BIT VALUE form GET/SET
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     de9e: KeyFrameDistance UINT32 data type enumeration: 3,  READ ONLY
     dc9e: SubDescription array of UINT16 data type ANY 16BIT VALUE form GET/SET
     dc4c: Source STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     dc95: MetaGenre UINT16 data type ANY 16BIT VALUE form GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
     dc94: ParentalRating STRING data type GET/SET
     da86: unknown(da86) STRING data type GET/SET
     da85: unknown(da85) UINT32 data type ANY 32BIT VALUE form GET/SET
     dc98: Subtitle STRING data type GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 363520, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 353,  READ ONLY
     de92: BitRateType UINT16 data type enumeration: 1, 2,  READ ONLY
     de9f: BufferSize UINT32 data type enumeration: 3,  READ ONLY
     dea0: EncodingQuality UINT32 data type enumeration: 50,  READ ONLY
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de97: ScanDepth UINT16 data type enumeration: 1,  READ ONLY
     de91: TotalBitRate UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
     de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911, 827739479, 844516695, 1347833175, 844125783,  READ ONLY
     de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 736000, STEP 1 READ ONLY
  b981: WMV
     da84: unknown(da84) STRING data type GET/SET
     dc44: Name STRING data type GET/SET
     dc04: ObjectSize UINT64 data type READ ONLY
     dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
     dc08: DateCreated STRING data type GET/SET
     dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
     dc09: DateModified STRING data type GET/SET
     de9d: FramesPerThousandSeconds UINT32 data type range: MIN 15000, MAX 30000, STEP 1 READ ONLY
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc0a: Keywords STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
     dc47: DateAuthored STRING data type GET/SET
     dc07: ObjectFileName STRING data type GET/SET
     da82: unknown(da82) UINT8 data type ANY 8BIT VALUE form GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc4b: CopyrightInformation array of UINT16 data type ANY 16BIT VALUE form GET/SET
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dea1: EncodingProfile STRING data type READ ONLY
     da81: unknown(da81) STRING data type GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     da83: unknown(da83) UINT32 data type ANY 32BIT VALUE form GET/SET
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     de9e: KeyFrameDistance UINT32 data type enumeration: 3,  READ ONLY
     dc9e: SubDescription array of UINT16 data type ANY 16BIT VALUE form GET/SET
     dc4c: Source STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
     dc95: MetaGenre UINT16 data type ANY 16BIT VALUE form GET/SET
     de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
     dc94: ParentalRating STRING data type GET/SET
     da86: unknown(da86) STRING data type GET/SET
     da85: unknown(da85) UINT32 data type ANY 32BIT VALUE form GET/SET
     dc98: Subtitle STRING data type GET/SET
     de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
     de99: AudioWAVECodec UINT32 data type enumeration: 353,  READ ONLY
     de92: BitRateType UINT16 data type enumeration: 1, 2,  READ ONLY
     de9f: BufferSize UINT32 data type enumeration: 3,  READ ONLY
     dea0: EncodingQuality UINT32 data type enumeration: 50,  READ ONLY
     de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
     de97: ScanDepth UINT16 data type enumeration: 1,  READ ONLY
     de91: TotalBitRate UINT32 data type range: MIN 1, MAX 800000, STEP 1 READ ONLY
     de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911, 827739479, 844516695, 1347833175, 844125783,  READ ONLY
     de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 736000, STEP 1 READ ONLY
  3801: JPEG
     dc44: Name STRING data type GET/SET
     dc04: ObjectSize UINT64 data type READ ONLY
     dc88: Height UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
     dc08: DateCreated STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc0a: Keywords STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc87: Width UINT32 data type range: MIN 0, MAX 640, STEP 1 GET/SET
     dc47: DateAuthored STRING data type GET/SET
     dc07: ObjectFileName STRING data type GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
  3804: BMP
     dc44: Name STRING data type GET/SET
     dc04: ObjectSize UINT64 data type READ ONLY
     dc88: Height UINT32 data type range: MIN 0, MAX 480, STEP 1 GET/SET
     dc08: DateCreated STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc0a: Keywords STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc87: Width UINT32 data type range: MIN 0, MAX 640, STEP 1 GET/SET
     dc47: DateAuthored STRING data type GET/SET
     dc07: ObjectFileName STRING data type GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
  3001: Association/Directory
     dc44: Name STRING data type GET/SET
     dc04: ObjectSize UINT64 data type READ ONLY
     dc08: DateCreated STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc0a: Keywords STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc07: ObjectFileName STRING data type GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
  ba03: Abstract Audio Album
     dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 320, STEP 1 READ ONLY
     dc44: Name STRING data type GET/SET
     dc04: ObjectSize UINT64 data type READ ONLY
     dc08: DateCreated STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc0a: Keywords STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc07: ObjectFileName STRING data type GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, GET/SET
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 240, STEP 1 READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
     dc46: Artist STRING data type GET/SET
     dc8c: Genre STRING data type GET/SET
  ba05: Abstract Audio Video Playlist
     dc44: Name STRING data type GET/SET
     dc04: ObjectSize UINT64 data type READ ONLY
     dc08: DateCreated STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc0a: Keywords STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc07: ObjectFileName STRING data type GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
  3000: Undefined Type
     dc44: Name STRING data type GET/SET
     dc04: ObjectSize UINT64 data type READ ONLY
     dc08: DateCreated STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc0a: Keywords STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc07: ObjectFileName STRING data type GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
  b802: Firmware
     dc44: Name STRING data type GET/SET
     dc04: ObjectSize UINT64 data type READ ONLY
     dc08: DateCreated STRING data type GET/SET
     dc09: DateModified STRING data type GET/SET
     dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
     dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
     dc0a: Keywords STRING data type GET/SET
     dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
     dc07: ObjectFileName STRING data type GET/SET
     dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
     dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
     dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
     dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  GET/SET
Storage Devices:
  StorageID: 0x00010001
     StorageType: 0x0003
     FilesystemType: 0x0002
     AccessCapability: 0x0000
     MaxCapacity: 29804494848
     FreeSpaceInBytes: 29264216064
     FreeSpaceInObjects: 4294967295
     StorageDescription: Storage
     VolumeIdentifier: 3c98dbd8 - d0a2274e - 80bd1ff8 - 8ee00652
Special directories:
  Default music folder: 0x08000002
  Default playlist folder: 0x00000000
  Default picture folder: 0x08000012
  Default video folder: 0x08000001
  Default organizer folder: 0x00000000
  Default zencast folder: 0x00000000
  Default album folder: 0x08000005
  Default text folder: 0x00000000
MTP-specific device properties:
  Friendly name: (NULL)
  Synchronization partner: (NULL)
  Battery level 93 of 100 (93%)
libmtp supported (playable) filetypes:
  ISO MPEG-1 Audio Layer 3
  Microsoft Windows Media Audio
  RIFF WAVE file
  Microsoft Advanced Systems Format
  Microsoft Windows Media Video
  JPEG file
  BMP bitmap file
  Firmware file

Secure Time:
<DRMCLOCK type="status"><VALUE>#20070908
22:35:43Z#</VALUE><FLAG>DRM_CLK_NOT_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID
private="1">I7JMxYhMy06EuG4+cjB3rFuyrCY=</UNIQUEID><PUBLICKEY
private="1">pkprBihWuZMZXU1ppUvFwcljFBDVoPH44NMSAo+G5XLfY/qXwHJAEQ==</PUBLICKEY><KEYDATA>n5eAkeU/mRs1Vzq9NY/xgIkmlws=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>q+pVw9b5+yPsZb29BciPRGCBLBPNcwCDb7KCU/5wWvcBQqgVYsMpBw==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>NZ9XLlac1576Wl4Isz1msc6AbkQ=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.104.7</SECURITYVERSION><CERTIFICATE
private="1">pkprBihWuZMZXU1ppUvFwcljFBDVoPH44NMSAo+G5XLfY/qXwHJAEQIEaAcsAQEodskQHYzfp6Y4rQfI68tCWtwZ2EeK3mUfLutNILfgUfvjs+Eh</CERTIFICATE></FALLBACK><CERTIFICATE
type="GROUP"><DATA><NAME>Gigabeat SX</NAME>
   <MANUFACTURER>Toshiba</MANUFACTURER>
   <MODEL>MESX</MODEL>
   <HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
   <HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR>
   <SECURITYLEVEL>2000</SECURITYLEVEL>
   <FEATURES>
       <CLOCK>2</CLOCK>
       <SECURECLOCK>
           <URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>

<PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY>
       </SECURECLOCK>
       <METERING>1</METERING>
       <LICENSE_ACQ>1</LICENSE_ACQ>
       <LICENSE_SYNC>1</LICENSE_SYNC>
       <ENCRYPTION>0</ENCRYPTION>
       <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
   </FEATURES>
   <LIMITS>
       <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
       <MAXLICENSESIZE>10240</MAXLICENSESIZE>
       <MAXHEADERSIZE>5120</MAXHEADERSIZE>

</LIMITS><PUBLICKEY>mq9FuW1IisvTC7I+VFY5V07b739t9ZBFciSg/Ntg3Ezwk6lB1Zt2hA==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>M1PUu1j1eqHSezQOzt2/JTOy8XrB/pP4h6qWZXGxonNm270x/H2OgQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>875</AUTH_ID><PUBLICKEY>HLFlAm8b55EZcqjzoT5TXEAOVDoG+I2xwgbAWaV0WdOJ7aWD/+HwLQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>qsT0KdwKbh7V9DQs6A+ODoohSWp/KXaJgKtVph2ywIDDKjVNaUjIfg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>ksv+Gms8aGkBXflfmLTMuJ3C3lsrKElMFGcidxk3d756HCidX36vKQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>

Device description WMPInfo.xml file:
<DeviceInfo>
   <WMP DeviceID="{D46CDC32-280A-4898-878C-D0B06CB9720D}"
RelationshipID="{00000000-0000-0000-0000-000000000000}"/>
</DeviceInfo>

OK.