Attempting to connect device(s)
Detect: Successfully connected 1 devices
USB low-level info:
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 4102
   idProduct: 112a
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000018
Device info:
   Manufacturer: iriver
   Model: iriver clix
   Device version: MTP-2.01-N-ENG
   Serial number: 873ff80f000000f93230303530313031
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 10.0; audible.com: 1.0;
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   101b: Get partial object
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9810: Get object references
   9811: Set object references
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   9201: Report Added/Deleted Items
Events supported:
   None.
Device Properties Supported:
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Device Friendly Name
   0xd405: Device Icon
   0xd101: Secure Time
   0xd102: Device Certificate
   0xd100: Unknown property
Playable File (Object) Types and Object Properties Supported:
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type READ ONLY
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type READ ONLY
   3004: Text
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type READ ONLY
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 85, 353,  READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX 10000000, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
   300a: MS AVI
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type READ ONLY
      de93: SampleRate UINT32 data type enumeration: 44100,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 128000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 85,  READ ONLY
      dc87: Width UINT32 data type range: MIN 4, MAX 320, STEP 4 GET/SET
      dc88: Height UINT32 data type range: MIN 4, MAX 240, STEP 4 GET/SET
      de91: TotalBitRate UINT32 data type range: MIN 16000, MAX 512000, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 1145656920,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 8000, MAX 384000, STEP 1 READ ONLY
      de9d: FramesPerThousandSeconds UINT32 data type enumeration: 5000, 6000, 7000, 8000, 9000, 10000, 11000, 12000, 13000, 14000, 15000,  GET/SET
   300c: ASF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 85, 353,  READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX 10000000, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
   3801: JPEG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type READ ONLY
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,  GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 74, MAX 75, STEP 1 GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 99, MAX 100, STEP 1 GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 85, 353,  READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX 10000000, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
   b902: OGG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 85, 353,  READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX 10000000, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
   b904: Audible.com Codec
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
      de99: AudioWAVECodec UINT32 data type enumeration: 85, 353,  READ ONLY
      dc89: Duration UINT32 data type range: MIN 0, MAX 10000000, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      da00: unknown(da00) UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8,  GET/SET
      da01: unknown(da01) STRING data type GET/SET
      da02: unknown(da02) UINT32 data type ANY 32BIT VALUE form GET/SET
      da03: unknown(da03) UINT16 data type enumeration: 0, 0,  GET/SET
   ba03: Abstract Audio Album
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type READ ONLY
      dc9b: AlbumArtist STRING data type GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,  GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 91, MAX 92, STEP 1 GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 91, MAX 92, STEP 1 GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type READ ONLY
   ba82: XMLDocument
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type READ ONLY
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 2005729280
      FreeSpaceInBytes: 1900265472
      FreeSpaceInObjects: 4294967295
      StorageDescription: iriver clix files
      VolumeIdentifier: hipdippaaaaaaajpcdadadfdadbdadbd
Special directories:
   Default music folder: 0x00070000
   Default playlist folder: 0x00060000
   Default picture folder: 0x00090000
   Default video folder: 0x00010000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00080000
   Default text folder: 0x00020000
MTP-specific device properties:
   Friendly name: Richard's Clix
   Synchronization partner: (NULL)
   Battery level 4 of 4 (100%)
libmtp supported (playable) filetypes:
   Text file
   ISO MPEG-1 Audio Layer 3
   Audio Video Interleave
   Microsoft Advanced Systems Format
   JPEG file
   Microsoft Windows Media Audio
   Ogg container format
   Audible.com Audio Codec
   XML file

Secure Time:
<DRMCLOCK type="status"><VALUE>#20060129 11:34:35Z#</VALUE><FLAG>DRM_CLK_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">CgoKCgoKCgoKCgoKCgoKCgoKCgo=</UNIQUEID><PUBLICKEY private="1">7cVY8s5uhwcwJZBCKY0Nzjwdqwa6eafIWthcYw/oCNPK6gB0fzxxNQ==</PUBLICKEY><KEYDATA>3TG4cp+JFr12+hWLOdquLkbrXf4=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>VyF9BrkcNPOlgrMPN7Ldd86Exk8CyzpcW7FehyuAAtXTB4Ns5JXeZA==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>pY98DivHN3zgKe/0MPv2wPx2+7Q=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.102.3</SECURITYVERSION><CERTIFICATE private="1">7cVY8s5uhwcwJZBCKY0Nzjwdqwa6eafIWthcYw/oCNPK6gB0fzxxNQIEZgPBcUIyUBSjrPOpAasS0zG/uY/xA2MSYeYMBFyXNJzlaYDonEw76411</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>iRiver H10 Series</NAME><MANUFACTURER>iRiver</MANUFACTURER><MAKE>iRiver</MAKE><DISTRIBUTOR>ReignCom</DISTRIBUTOR><MODEL>H10</MODEL><SECURITYLEVEL>2000</SECURITYLEVEL><HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR><HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR><FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR><FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR><FEATURES><CLOCK>2</CLOCK><SECURECLOCK><URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL><PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY></SECURECLOCK><METERING>1</METERING><LICENSE_ACQ>1</LICENSE_ACQ><LICENSE_SYNC>1</LICENSE_SYNC><ENCRYPTION>1</ENCRYPTION><SYMMETRIC_OPT>1</SYMMETRIC_OPT></FEATURES><LIMITS><MAXCHAINDEPTH>2</MAXCHAINDEPTH><MAXLICENSESIZE>10240</MAXLICENSESIZE><MAXHEADERSIZE>5120</MAXHEADERSIZE></LIMITS><PUBLICKEY>8jeq4PyJZUL8NpU2+/tgvUZC9ijn3RdlK3wd04Iws6oXHoA+D6vFfQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>HZ85tGf5VnDwKLGq2S0OlK/oJCKbCx3A2yudzMOv8ERwi6drHW5xOA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>359</AUTH_ID><PUBLICKEY>DpMhgaZkXUFNFIs4KJe7S9MZYwuE1bBic6AV6wAc7Ir0Stfx8U+SKw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>GWscwHnDoSazgB+YOP2D7xrqDifWEFztujqAWwrkM7onynIcfOBBMQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>QndHdJ4ZoSgvokVCOWsqVnvuckGL5cn6Vrua0j4tcGBrjD9PgNd0AA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>

Device description WMPInfo.xml file:
<DeviceInfo>
    <WMP DeviceID="{38F6CE81-F97C-4359-B9A8-236F2FCBF6A0}" RelationshipID="{00000000-0000-0000-0000-000000000000}"/>
</DeviceInfo>

OK.
