libmtp version: 0.3.6

Listing raw device(s)
   Found 1 device(s):
   Samsung: YH-999 Portable Media Center/SGH-A707/SGH-L760V/SGH-U900 (04e8:5a0f) @ bus 0, dev 5
Attempting to connect device(s)
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 272
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 04e8
   idProduct: 5a0f
   IN endpoint maxpacket: 64 bytes
   OUT endpoint maxpacket: 64 bytes
   Raw device info:
      Bus location: 0
      Device number: 5
      Device entry info:
         Vendor: Samsung
         Vendor id: 0x04e8
         Product: YH-999 Portable Media Center/SGH-A707/SGH-L760V/SGH-U900
         Vendor id: 0x5a0f
         Device flags: 0x00000001
Microsoft device descriptor 0xee:
	0000: 1203 4d00 5300 4600 5400 3100 3000 3000	..M.S.F.T.1.0.0.
	0010: 0900                                   	..
Microsoft device response to control message 1, CMD 0x09:
	0000: 6a00 0000 0001 0400 0100 0000 0000 0000	j...............
	0010: 0001 4d00 0000 5400 0000 5000 0000 0000	..M...T...P.....
	0020: 0000 0000 0000 0000 0000 0000 0000 0000	................
	0030: 0000 0000 0000 0000 0000 0000 0000 0000	................
	0040: 0000 0000 0000 0000 0000 0000 0000 0000	................
	0050: 0000 0000 0000 0000 0000 0000 0000 0000	................
	0060: 0000 0000 0000 0000 0000               	..........
Device info:
   Manufacturer: Samsung Electronics Co., Ltd. 
   Model: SGH-L760V
   Device version: L760BUGH1
   Serial number: 356603013289914
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMPPD: 10.0; microsoft.com/WMPPD: 11.0; vodafone.com/omadrmv2: 1.0; 
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   101b: Get partial object
   9810: Get object references
   9811: Set object references
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9201: Report Added/Deleted Items
   1011: Self test device
   1012: Set object protection
   1017: Reset device property value
   1019: Move object
   101a: Copy object
   9808: Send object property list
   9001: Unknown (9001)
   9202: Report Acquired Items
Events supported:
   0x4001
   0x4004
   0x4005
Device Properties Supported:
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd404: Unknown property
Playable File (Object) Types and Object Properties Supported:
   b984: 3GP
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 13000, MAX 192999, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14343, 14347, 47361, 12299,  READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: RepresentativeSampleDuration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 13000, MAX 192999, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14343, 14347, 47361, 12299,  READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: RepresentativeSampleDuration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 13000, MAX 192999, STEP 1 READ ONLY
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc96: Composer STRING data type GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14343, 14347, 47361, 12299,  READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: RepresentativeSampleDuration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
   b981: WMV
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 176, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 144, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 13000, MAX 16999, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 827739479, 844516695, 861293911,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 32000, MAX 96000, STEP 1 GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type enumeration: 0, 15000,  GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
   3801: JPEG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 2000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 2000, STEP 1 GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14343, 14347, 47361, 12299,  READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: RepresentativeSampleDuration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 0 GET/SET
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
   3807: GIF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 2000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 2000, STEP 1 GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14343, 14347, 47361, 12299,  READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: RepresentativeSampleDuration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 0 GET/SET
   300c: ASF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 176, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 144, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 6, 7,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 13000, MAX 16999, STEP 1 READ ONLY
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 827739479, 844516695, 861293911,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 32000, MAX 96000, STEP 1 GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type enumeration: 0, 15000,  GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
   ba03: Abstract Audio Album
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc44: Name STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 0, 1,  GET/SET
      dc08: DateCreated STRING data type DATETIME FORM GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 2000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 2000, STEP 1 GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14343, 14347, 47361, 12299,  READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 10000000, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 1000000, STEP 1 READ ONLY
      dc85: RepresentativeSampleDuration UINT32 data type range: MIN 0, MAX 100000, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
      d901: BuyFlag UINT8 data type range: MIN 0, MAX 1, STEP 0 GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 69926912
      FreeSpaceInBytes: 34375680
      FreeSpaceInObjects: 4294967295
      StorageDescription: Phone
      VolumeIdentifier: 356603013289914
Special directories:
   Default music folder: 0x00000003
   Default playlist folder: 0x00000000
   Default picture folder: 0x00000005
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: SGH-L760V
   Synchronization partner: SGH-L760V
   Battery level 85 of 100 (85%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   Microsoft Windows Media Video
   JPEG file
   GIF bitmap file
   Microsoft Advanced Systems Format
Unable to acquire device certificate, perhaps this device does not support this

WMPInfo.xml file contents:
<DeviceInfo>
    <WMP DeviceID="{AA9D2C49-2F20-41F8-853F-82C920DBF235}" RelationshipID="{00000000-0000-0000-0000-000000000000}"/>
</DeviceInfo>

OK.
