libmtp version: 0.2.4

Attempting to connect device(s)
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 069b
   idProduct: 301a
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x0000000a
Microsoft device descriptor 0xee:
	0000: 1203 4d00 5300 4600 5400 3100 3000 3000	..M.S.F.T.1.0.0.
	0010: 0100                                   	..
Device info:
   Manufacturer: THOMSON
   Model: RCA H106
   Device version: V1.71
   Serial number: 30B80000000000000000000000000000
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com/WMDRMPD: 10.1;microsoft.com/AAVT: 1.0;microsoft.com/WMDRMND: 1.0;audible.com: 1.0;
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1010: Reset device
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   9810: Get object references
   9811: Set object references
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   101b: Get partial object
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   9170: Open Media Session
   9171: Close Media Session
   9172: Get Next Data Block
   9173: Set Current Time Position
   9180: Send Registration Request
   9181: Get Registration Response
   9182: Get Proximity Challenge
   9183: Send Proximity Response
   9184: Send WMDRM-ND License Request
   9185: Get WMDRM-ND License Response
Events supported:
   None.
Device Properties Supported:
   0xd100: Unknown property
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd101: Secure Time
   0xd102: Device Certificate
Playable File (Object) Types and Object Properties Supported:
   3009: MP3
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      dc9a: AlbumName STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
   b901: WMA
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 320000, STEP 1 READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      dc9a: AlbumName STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
   3008: MS Wave
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 320000, STEP 1 READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  READ ONLY
      dc9a: AlbumName STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
   b904: Audible.com Codec
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      da00: unknown(da00) UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8,  GET/SET
      da02: unknown(da02) UINT32 data type ANY 32BIT VALUE form READ ONLY
      da03: unknown(da03) UINT16 data type enumeration: 0, 1,  READ ONLY
      da01: unknown(da01) STRING data type GET/SET
      da04: unknown(da04) array of UINT8 data type ANY 8BIT VALUE form GET/SET
   3001: Association/Directory
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
   ba05: Abstract Audio Video Playlist
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
   3000: Undefined Type
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
   b802: Firmware
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
   ba03: Abstract Audio Album
      dc97: EffectiveRating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc44: Name STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 6129004544
      FreeSpaceInBytes: 2242122630
      FreeSpaceInObjects: 6192
      StorageDescription: TCNAND0
      VolumeIdentifier: 30B80000000000000000000000000000
Special directories:
   Default music folder: 0x20000224
   Default playlist folder: 0x20000009
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: RCA H106
   Synchronization partner: Longhorn Sync Engine
   Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Windows Media Audio
   RIFF WAVE file
   Audible.com Audio Codec
   Firmware file

Secure Time:
<DRMCLOCK type="status"><VALUE>#19770910 02:12:11Z#</VALUE><FLAG>DRM_CLK_NOT_SET</FLAG></DRMCLOCK>AG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">MLgAAAAAAAAAAAAAAAAAAAAAAAA=</UNIQUEID><PUBLICKEY private="1">/xk1FRLtUFQtLumioB3hnjjmCCStWRtCZ+OUINvN4wRjglPz1DTagw==</PUBLICKEY><KEYDATA>KkFgl/xxIQnFTSasJdjDCCv/P24=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>LD33X8FUDo00JUcw8aIxaslZOU1gwe23tnsDKRZCKxdEiLkZ6MqtRA==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>lcs/XXhRSo4LmZvRM9Ng82/uNEA=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.103.93</SECURITYVERSION><CERTIFICATE private="1">/xk1FRLtUFQtLumioB3hnjjmCCStWRtCZ+OUINvN4wRjglPz1DTagwIEZ12zLMYIU+hJu3l1M4RYq3Wm7dvKElLPBtkNiU7D3DEFkb5rubXCF6sQ</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>H106</NAME>
    <MANUFACTURER>Thomson</MANUFACTURER>
    <MAKE>Portable Media Player</MAKE>
    <DISTRIBUTOR>Thomson</DISTRIBUTOR>
    <MODEL>H106</MODEL>
    <SECURITYLEVEL>2000</SECURITYLEVEL>
    <HARDWARE_VER_MAJOR>A</HARDWARE_VER_MAJOR>
    <FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR>
    <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
    <FEATURES>
        <CLOCK>2</CLOCK>
	  <SECURECLOCK>
		<URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
		<PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY>
	  </SECURECLOCK>
        <METERING>1</METERING>
        <LICENSE_ACQ>0</LICENSE_ACQ>
        <LICENSE_SYNC>1</LICENSE_SYNC>
        <ENCRYPTION>0</ENCRYPTION>
  <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
    </FEATURES>
    <LIMITS>
        <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
        <MAXLICENSESIZE>10240</MAXLICENSESIZE>
        <MAXHEADERSIZE>5120</MAXHEADERSIZE>
    </LIMITS><PUBLICKEY>eWGqaKD/rEgPNu6GrH4E4KOVmDLU3uH7S0yZJ6AhJCUwYZKiVI3JdQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>bNMpmF0aj44IYQDYnnbcURRgzU1rIlAlL9jNNOzJ0FtEHXngXg2fDw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>705</AUTH_ID><PUBLICKEY>0xGAyvWRMSN9LFmWL0S9WztdgXzTo5nwPQENDz2q6lJ4SPILToOvGQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>YjzR0s45M5rz4YiE8fZjo/rhVHGlVtsW5re00vPgGJS3dc1e3bpHcA==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>RCnBbt41GoYgQEzB4T9r432WenXcYM6rdlEo0hCbDwb7H1LhcmNFJg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
WMPInfo.xml Does not exist on this device
OK.
