libmtp version: 0.2.6.1

Attempting to connect device(s)
PTP: Opening session
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 045e
   idProduct: 0622
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000000
Device info:
   Manufacturer: Microsoft Corporation
   Model: Windows Media Mobile Platform Solutions
   Device version: 100
   Serial number: 12345
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMPPD: 11.0
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   1012: Set object protection
   100d: Send object
   100f: Format storage
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   1019: Move object
   101a: Copy object
   101b: Get partial object
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9810: Get object references
   9811: Set object references
Events supported:
   None.
Device Properties Supported:
   0x5001: Battery Level
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
Playable File (Object) Types and Object Properties Supported:
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 1, 0,  GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 1, 0,  GET/SET
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 1, 0,  GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 1, 0,  GET/SET
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 1, 0,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 0, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 0, MAX 5000000, STEP 1 READ ONLY
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 1, 0,  GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      de95: AudioBitDepth UINT32 data type enumeration: 0, 8, 10, 12, 16, 24, 32,  GET/SET
      dc05: AssociationType UINT16 data type enumeration: 1, 0,  GET/SET
   300c: ASF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 1, 0,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 0, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 0, MAX 5000000, STEP 1 READ ONLY
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 2000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 1500, STEP 1 GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 1, 0,  GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      de95: AudioBitDepth UINT32 data type enumeration: 0, 8, 10, 12, 16, 24, 32,  GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 859189832, 958804552, 1195724877, 827739479, 844516695, 861293911,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 100000000, STEP 1 GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type enumeration: 0, 15000, 25000, 29970, 60000,  GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea0: EncodingQuality UINT32 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 1, 0,  GET/SET
   3801: JPEG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 1, 0,  GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 2000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 1500, STEP 1 GET/SET
      dc05: AssociationType UINT16 data type enumeration: 1, 0,  GET/SET
   b802: Firmware
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 1, 0,  GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 1, 0,  GET/SET
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 1, 0,  GET/SET
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de93: SampleRate UINT32 data type range: MIN 0, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 0, MAX 5000000, STEP 1 READ ONLY
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 1, 0,  GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      de95: AudioBitDepth UINT32 data type enumeration: 0, 8, 10, 12, 16, 24, 32,  GET/SET
      dc05: AssociationType UINT16 data type enumeration: 1, 0,  GET/SET
   b981: WMV
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 1, 0,  GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de93: SampleRate UINT32 data type range: MIN 0, MAX 48000, STEP 50 READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 2, 3, 8, 9, 11, 49, 50, 80, 85, 352, 353, 354, 355, 356, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 0, MAX 5000000, STEP 1 READ ONLY
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 2000, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 1500, STEP 1 GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 1, 0,  GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2, 3,  GET/SET
      de97: ScanDepth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 0, 859189832, 958804552, 1195724877, 827739479, 844516695, 861293911,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 1, MAX 100000000, STEP 1 GET/SET
      de9d: FramesPerThousandSeconds UINT32 data type enumeration: 0, 15000, 25000, 29970, 60000,  GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 100, MAX 300, STEP 1 GET/SET
      dea0: EncodingQuality UINT32 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 1, 0,  GET/SET
   ba03: Abstract Audio Album
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 1, 0,  GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 1, 0,  GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 1, 0,  GET/SET
      dc08: DateCreated STRING data type GET/SET
      dc09: DateModified STRING data type GET/SET
      dc05: AssociationType UINT16 data type enumeration: 1, 0,  GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 270917632
      FreeSpaceInBytes: 266870272
      FreeSpaceInObjects: 0
      StorageDescription: MTP Store - 65537
      VolumeIdentifier: MTP Volume - 65537
Special directories:
   Default music folder: 0x00000000
   Default playlist folder: 0x00000000
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: (NULL)
   Synchronization partner: (NULL)
   Battery level 0 of 100 (0%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   Microsoft Advanced Systems Format
   JPEG file
   Firmware file
   Microsoft Windows Media Audio
   Microsoft Windows Media Video
Unable to acquire device certificate, perhaps this device does not support this
WMPInfo.xml Does not exist on this device
PTP: Closing session
OK.
