libmtp version: 0.3.4

Listing raw device(s)
   Found 1 device(s):
   0421:01f5 @ bus 0, dev 4
Attempting to connect device(s)
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 2
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0421
   idProduct: 01f5
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 0
      Device number: 4
      Device entry info:
         Vendor: (null)
         Vendor id: 0x0421
         Product: (null)
         Vendor id: 0x01f5
         Device flags: 0x00000000
Configuration 0, interface 0, altsetting 0:
   Interface description contains the string "MTP"
   Device recognized as MTP, no further probing.
Device info:
   Manufacturer: Nokia
   Model: N97
   Device version: 01
   Serial number: 354225032477049
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com:1.0;microsoft.com/WMPPD: 11.0;microsoft.com/WMDRMPD: 10.1;vodafone.com/omadrmv2: 1.0
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   1010: Reset device
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9810: Get object references
   9811: Set object references
   9805: Get object property list
   9806: Set object property list
   9807: Get interdependent property description
   9201: Report Added/Deleted Items
   9202: Report Acquired Items
   9203: Get transferable playlist types
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
Events supported:
   0x400a
   0x4004
   0x4005
   0x4003
Device Properties Supported:
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
   0xd404: Unknown property
   0xd102: Device Certificate
   0xd406: Unknown property
Playable File (Object) Types and Object Properties Supported:
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: DateAdded STRING data type DATETIME FORM READ ONLY
      dc08: DateCreated STRING data type DATETIME FORM READ ONLY
      dc09: DateModified STRING data type DATETIME FORM READ ONLY
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: DateAdded STRING data type DATETIME FORM READ ONLY
      dc08: DateCreated STRING data type DATETIME FORM READ ONLY
      dc09: DateModified STRING data type DATETIME FORM READ ONLY
   b903: AAC
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: DateAdded STRING data type DATETIME FORM READ ONLY
      dc08: DateCreated STRING data type DATETIME FORM READ ONLY
      dc09: DateModified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
   b982: MP4
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: DateAdded STRING data type DATETIME FORM READ ONLY
      dc08: DateCreated STRING data type DATETIME FORM READ ONLY
      dc09: DateModified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 16000, MAX 576000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: DateAdded STRING data type DATETIME FORM READ ONLY
      dc08: DateCreated STRING data type DATETIME FORM READ ONLY
      dc09: DateModified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 85,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 320000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
   b984: 3GP
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: DateAdded STRING data type DATETIME FORM READ ONLY
      dc08: DateCreated STRING data type DATETIME FORM READ ONLY
      dc09: DateModified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 16000, MAX 576000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
   b004: Unknown(b004)
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: DateAdded STRING data type DATETIME FORM READ ONLY
      dc08: DateCreated STRING data type DATETIME FORM READ ONLY
      dc09: DateModified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 1, 85, 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 16000, MAX 576000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
   b982: MP4
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: DateAdded STRING data type DATETIME FORM READ ONLY
      dc08: DateCreated STRING data type DATETIME FORM READ ONLY
      dc09: DateModified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 41222,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 16000, MAX 576000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: DateAdded STRING data type DATETIME FORM READ ONLY
      dc08: DateCreated STRING data type DATETIME FORM READ ONLY
      dc09: DateModified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 353,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 384000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
   300c: ASF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: DateAdded STRING data type DATETIME FORM READ ONLY
      dc08: DateCreated STRING data type DATETIME FORM READ ONLY
      dc09: DateModified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 353,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 384000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 176, MAX 320, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 144, MAX 240, STEP 1 GET/SET
      de97: ScanDepth UINT16 data type ANY 16BIT VALUE form GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911, 1297101377, 1297101889,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 0, MAX 384000, STEP 1 READ ONLY
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      dea1: EncodingProfile STRING data type GET/SET
   b981: WMV
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc87: Width UINT32 data type range: MIN 176, MAX 320, STEP 1 GET/SET
      dc88: Height UINT32 data type range: MIN 144, MAX 240, STEP 1 GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de97: ScanDepth UINT16 data type ANY 16BIT VALUE form GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 353,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 5000, MAX 384000, STEP 1 GET/SET
      de9b: VideoFourCCCodec UINT32 data type enumeration: 861293911,  GET/SET
      de9c: VideoBitRate UINT32 data type range: MIN 0, MAX 384000, STEP 1 READ ONLY
      de9d: FramesPerThousandSeconds UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      de9e: KeyFrameDistance UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      dea1: EncodingProfile STRING data type GET/SET
      dc94: ParentalRating STRING data type GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
   ba11: M3U Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: DateAdded STRING data type DATETIME FORM READ ONLY
      dc08: DateCreated STRING data type DATETIME FORM READ ONLY
      dc09: DateModified STRING data type DATETIME FORM READ ONLY
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: DateAdded STRING data type DATETIME FORM READ ONLY
      dc08: DateCreated STRING data type DATETIME FORM READ ONLY
      dc09: DateModified STRING data type DATETIME FORM READ ONLY
   3008: MS Wave
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc4e: DateAdded STRING data type DATETIME FORM READ ONLY
      dc08: DateCreated STRING data type DATETIME FORM READ ONLY
      dc09: DateModified STRING data type DATETIME FORM READ ONLY
      dc46: Artist STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 1,  GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 16000, MAX 1536000, STEP 1 GET/SET
      dc96: Composer STRING data type GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc9d: DRMStatus UINT16 data type enumeration: 0, 1, 16384, 16385,  GET/SET
      db01: unknown(db01) UINT8 data type enumeration: 0, 1,  GET/SET
Storage Devices:
   StorageID: 0x00040001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 32002539520
      FreeSpaceInBytes: 18941128704
      FreeSpaceInObjects: 9054
      StorageDescription: Mass memory
      VolumeIdentifier: 1695920643
   StorageID: 0x00020001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 76582912
      FreeSpaceInBytes: 17272832
      FreeSpaceInObjects: 8
      StorageDescription: Phone memory
      VolumeIdentifier: 1196836185
   StorageID: 0x00050001
      StorageType: 0x0004 removable RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 1015283712
      FreeSpaceInBytes: 809226240
      FreeSpaceInObjects: 386
      StorageDescription: Memory card (WafaaMcSD1G)
      VolumeIdentifier: 1684419169
Special directories:
   Default music folder: 0x00857a00
   Default playlist folder: 0x0085b078
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: Nokia N97
   Synchronization partner: Nokia N97
libmtp supported (playable) filetypes:
   Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
   MPEG-4 Part 14 Container Format (Audio+Video Empahsis)
   ISO MPEG-1 Audio Layer 3
   MPEG-4 Part 14 Container Format (Audio+Video Empahsis)
   Microsoft Windows Media Audio
   Microsoft Advanced Systems Format
   Microsoft Windows Media Video
   RIFF WAVE file

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">D8ABB2Z1AFK//5MvJZXyovnmv9w=</UNIQUEID><PUBLICKEY private="1">pNify9zkLFCu+AzarhGKjaVZy2dwRnJAYsb7gBTKcIIVe0c5f8TaLA==</PUBLICKEY><KEYDATA>KmRKV6lO4ud9sZgA0CvjjEGlx6g=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>zxWktCvCM82zWPlIAsw2zIO4roArHwfR/yuYdD4WAY9vvqrriv8PSg==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>Wf/mNFW8vYxfdmJrl6IvwkwcgLU=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.113.133</SECURITYVERSION><CERTIFICATE private="1">pNify9zkLFCu+AzarhGKjaVZy2dwRnJAYsb7gBTKcIIVe0c5f8TaLAIEcYWBNc0i5G82u6t+A4dzS8UqBz6BQ35tebS6nQRLc6R23YWGcJQ5QCx3</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>N97</NAME>
    <MANUFACTURER>Nokia</MANUFACTURER>
    <MAKE>Nokia</MAKE>
    <DISTRIBUTOR>Nokia</DISTRIBUTOR>
    <MODEL>RM-505</MODEL>
    <SECURITYLEVEL>2000</SECURITYLEVEL>
    <HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
    <HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR>
    <FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR>
    <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
    <FEATURES>
        <CLOCK>1</CLOCK>
        <METERING>1</METERING>
        <LICENSE_ACQ>1</LICENSE_ACQ>
        <LICENSE_SYNC>1</LICENSE_SYNC>
        <ENCRYPTION>1</ENCRYPTION>
        <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
    </FEATURES>
    <LIMITS>
        <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
        <MAXLICENSESIZE>10240</MAXLICENSESIZE>
        <MAXHEADERSIZE>5120</MAXHEADERSIZE>
    </LIMITS><PUBLICKEY>Bnzrf4HfEQFTluAifcOGnShfozcFCl4rCLvkVkNrqzPekHu01kt5Yg==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>xC5BssDKi9GawHZmwNbRPhF3K1JY+AmWQkeEaxQyC/mNdsY1zwgLZw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>3305</AUTH_ID><PUBLICKEY>pLjNChqCyqHpXcXp91vyznAAHwsCciuxTK5jBIJD5p+kP+JQ/BCLZQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>LvMELOwmIdYTJ0biMpfssiO2nB+LsVIpMU9UG/gK6Lm2P8ahHTUkXQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>N5pd/yA5Yle17LAFkhh3jZhcgYjwDD0+mjs1ErQswvOVZnX4XtHMag==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
WMPInfo.xml Does not exist on this device
OK.

 	  	 
