libmtp version: 1.0.0

Listing raw device(s)
   Found 1 device(s):
   Philips: GoGear SA1ARA08K/37 (0471:207c) @ bus 0, dev 9
Attempting to connect device(s)
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0471
   idProduct: 207c
   IN endpoint maxpacket: 64 bytes
   OUT endpoint maxpacket: 64 bytes
   Raw device info:
      Bus location: 0
      Device number: 9
      Device entry info:
         Vendor: Philips
         Vendor id: 0x0471
         Product: GoGear SA1ARA08K/37
         Vendor id: 0x207c
         Device flags: 0x00000002
Microsoft device descriptor 0xee:
	0000: 1203 4d00 5300 4600 5400 3100 3000 3000	..M.S.F.T.1.0.0.
	0010: 0100                                   	..
Microsoft device response to control message 1, CMD 0x01:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Device info:
   Manufacturer: Philips
   Model: GoGear Aria
   Device version: PH0E000613
   Serial number: 09FA0000015B9CA90002DA6D74551CA9
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1; microsoft.com/WMPPD: 10.0; microsoft.com/WMPPD: 11.0; audible.com: 1.0
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   101b: Get partial object
   100b: Delete object
   100c: Send object info
   100d: Send object
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   9802: Get object property description
   9801: Get object properties supported
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9808: Send object property list
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   100f: Format storage
   9810: Get object references
   9811: Set object references
   9201: Report Added/Deleted Items
   9202: Report Acquired Items
   9203: Get transferable playlist types
   97f1: Unknown (97f1)
   97f2: Unknown (97f2)
   97f3: Unknown (97f3)
   97f4: Unknown (97f4)
   97f5: Unknown (97f5)
   1010: Reset device
   1012: Set object protection
Events supported:
   0x4004
   0x4005
Device Properties Supported:
   0xd101: Secure Time
   0xd102: Device Certificate
   0xd402: Friendly Device Name
   0xd401: Synchronization Partner
   0x5001: Battery Level
   0xd405: Device Icon
   0xd100: Unknown property
Playable File (Object) Types and Object Properties Supported:
   3009: MP3
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 1, MAX 4300000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 80, 85,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
   3008: MS Wave
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 2304000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 1, 2, 17,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
   b901: WMA
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 352, 353,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
   300c: ASF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0, 352, 353,  GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 240, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 320, STEP 1 GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      de9e: Key Frame Distance UINT32 data type range: MIN 0, MAX 15000, STEP 1 GET/SET
      de9d: Frames Per Thousand Seconds UINT32 data type range: MIN 0, MAX 30050, STEP 1 GET/SET
      de9b: Video Four CC Codec UINT32 data type enumeration: 0, 861293911,  GET/SET
      de9c: Video Bit Rate UINT32 data type range: MIN 5000, MAX 768010, STEP 1 READ ONLY
      de97: Scan Depth UINT16 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7,  GET/SET
      dea1: Encoding Profile STRING data type GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   3001: Association/Directory
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc05: Association Type UINT16 data type enumeration: 0, 1,  GET/SET
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
   3801: JPEG
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   3807: GIF
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   3804: BMP
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc88: Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      dc97: Effective Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   ba03: Abstract Audio Album
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9b: Album Artist STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc84: Representative Sample Width UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc83: Representative Sample Height UINT32 data type range: MIN 0, MAX 10000, STEP 1 GET/SET
      dc82: Representative Sample Sise UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc81: Representative Sample Format UINT16 data type enumeration: 14337, 14340, 14343,  GET/SET
      dc86: Representative Sample Data array of UINT8 data type byte array:  GET/SET
   b905: Unknown(b905)
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
   b907: Unknown(b907)
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
   3000: Undefined Type
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
   b904: Audible.com Codec
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      da00: Unknown property UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9,  READ ONLY
      da02: Unknown property UINT32 data type ANY 32BIT VALUE form GET/SET
      da01: Unknown property STRING data type READ ONLY
      da03: Unknown property UINT16 data type enumeration: 0, 1,  GET/SET
      da04: Unknown property UINT128 data type READ ONLY
   b301: Unknown(b301)
      dc01: Storage ID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: Object Format UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: Protection Status UINT16 data type enumeration: 0, 1,  READ ONLY
      dc04: Object Size UINT64 data type READ ONLY
      dc07: Object File Name STRING data type REGULAR EXPRESSION FORM GET/SET
      dc08: Date Created STRING data type DATETIME FORM GET/SET
      dc0b: Parent Object UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: Persistant Unique Object Identifier UINT128 data type READ ONLY
      dc42: Sync ID STRING data type GET/SET
      dc0d: Hidden UINT16 data type enumeration: 0, 1,  GET/SET
      dc4f: Non Consumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc9a: Album Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc9b: Album Artist STRING data type GET/SET
      de93: Sample Rate UINT32 data type enumeration: 8000, 11025, 16000, 22050, 32000, 44100, 48000,  READ ONLY
      de94: Number Of Channels UINT16 data type enumeration: 1, 2,  GET/SET
      de9a: Audio Bit Rate UINT32 data type range: MIN 5000, MAX 430000, STEP 1 READ ONLY
      dc44: Name STRING data type GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 16777215, STEP 1 GET/SET
      de99: Audio WAVE Codec UINT32 data type enumeration: 0,  GET/SET
      dc09: Date Modified STRING data type DATETIME FORM GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc99: Original Release Date STRING data type DATETIME FORM GET/SET
      d901: Buy flag UINT8 data type range: MIN 0, MAX 1, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: Use Count UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: Skip Count UINT32 data type ANY 32BIT VALUE form GET/SET
      da00: Unknown property UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9,  READ ONLY
      da02: Unknown property UINT32 data type ANY 32BIT VALUE form GET/SET
      da01: Unknown property STRING data type READ ONLY
      da03: Unknown property UINT16 data type enumeration: 0, 1,  GET/SET
      da04: Unknown property UINT128 data type READ ONLY
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 7901544448
      FreeSpaceInBytes: 6680379392
      FreeSpaceInObjects: 4294967295
      StorageDescription: Internal Storage
      VolumeIdentifier: 09FA0000015B9CA90002DA6D74551CA9
Special directories:
   Default music folder: 0x00000073
   Default playlist folder: 0x00000066
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: GoGear Aria
   Synchronization partner: GoGear Aria
   Battery level 98 of 100 (98%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   R
