Potential MTP Device with VendorID:0781 and ProductID:7480 responded to
control message 2 with a response that was too short. Problems may arrise
but continuing
PTP: Opening session
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0781
   idProduct: 7480
   IN endpoint maxpacket: 64 bytes
   OUT endpoint maxpacket: 64 bytes
   Device flags: 0x00000002
Device info:
   Manufacturer: SanDisk
   Model: Sansa Connect
   Device version: 0.002a
   Serial number: <snip>
   Vendor extension ID: 0x00000006
   Vendor extension description:  microsoft.com/WMDRMPD: 10.1;
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1010: Reset device
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9805: Get object property list
   9804: Set object property value
   9807: Get interdependent property description
   4001: Unknown(4001)
   9810: Get object references
   9811: Set object references
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   100f: Format storage
   9806: Set object property list
Events supported:
   None.
Device Properties Supported:
   0x5001: Battery Level
   0xd402: Device Friendly Name
   0xd101: Secure Time
   0xd102: Device Certificate
Playable File (Object) Types and Object Properties Supported:
   b901: WMA
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc48: Description array of UINT16 data type ANY 16BIT VALUE form GET/SET
      dc49: URLReference STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 15918, 22050, 24000, 32000, 44100, 48000,  READ ONLY
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 9, 50, 80, 85, 352, 353, 354,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 32000, MAX 192000, STEP 1 READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc8a: Rating UINT16 data type range: MIN 1, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc8f: SubscriptionContentID STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc96: Composer STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
   ba03: Abstract Audio Album
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,  READ ONLY
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX 65536, STEP 1 READ ONLY
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 88, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 88, STEP 1 READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
   ba05: Abstract Audio Video Playlist
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
   3000: Undefined Type
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
   3001: Association/Directory
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
   3009: MP3
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0, 1, 9, 50, 80, 85, 352, 353, 354,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 32000, MAX 320000, STEP 1 READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc89: Duration UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc8a: Rating UINT16 data type range: MIN 1, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc96: Composer STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
   3801: JPEG
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc87: Width UINT32 data type ANY 32BIT VALUE form GET/SET
      dc88: Height UINT32 data type ANY 32BIT VALUE form GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 3629608960
      FreeSpaceInBytes: 2528118784
      FreeSpaceInObjects: 4294967295
      StorageDescription: Internal Memory
      VolumeIdentifier: 
Special directories:
   Default music folder: 0x01000000
   Default playlist folder: 0x00000000
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: Sansa Connect
   Synchronization partner: (NULL)
   Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
   Microsoft Windows Media Audio
   ISO MPEG-1 Audio Layer 3
   JPEG file

Secure Time:
<DRMCLOCK type="status"><VALUE>#20070625
21:23:41Z#</VALUE><FLAG>DRM_CLK_NOT_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID
private="1">MDAzNTBjZGEwY2Q5NDc3NmY1ZTdkYjNiMDMwMDZjMjA=</UNIQUEID><PUBLICKEY
private="1">N1UNmgK1Q91d+o6jTz1XYeslBBM/4vxftlmeqYP283U853zBDAsXfQ==</PUBLICKEY><KEYDATA>Hh2dgQ6Lf/GmgDqYq/PG170vQyU=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>v/q8lIrrzkrGnEzqrhVU/jRyyS3jDBZa/6cMPRMOlHwy4A54ZdXVLQ==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>L4RaI0MqkghSlXOmxdj2vM8pLeU=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.106.183</SECURITYVERSION><CERTIFICATE
private="1">N1UNmgK1Q91d+o6jTz1XYeslBBM/4vxftlmeqYP283U853zBDAsXfQIEarfnTGArHCv/vfxqC5o1UXrJi39tCh0QhCsFK7SUxyPYqJHv5WmflQh6</CERTIFICATE></FALLBACK><CERTIFICATE
type="GROUP"><DATA><NAME>Sansa</NAME>
    <MANUFACTURER>SanDisk</MANUFACTURER>
    <MODEL>Connect Series</MODEL>
    <SECURITYLEVEL>2000</SECURITYLEVEL>
    <HARDWARE_VER_MAJOR>0</HARDWARE_VER_MAJOR>
    <HARDWARE_VER_MINOR>9</HARDWARE_VER_MINOR>
    <FIRMWARE_VER_MAJOR>0</FIRMWARE_VER_MAJOR>
    <FIRMWARE_VER_MINOR>9</FIRMWARE_VER_MINOR>
    <FEATURES>
        <CLOCK>2</CLOCK>
        <SECURECLOCK>
            <URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
           
<PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY>
        </SECURECLOCK>
        <METERING>1</METERING>
        <LICENSE_ACQ>1</LICENSE_ACQ>
        <LICENSE_SYNC>1</LICENSE_SYNC>
        <ENCRYPTION>1</ENCRYPTION>
        <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
    </FEATURES>
    <LIMITS>
        <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
        <MAXLICENSESIZE>10240</MAXLICENSESIZE>
        <MAXHEADERSIZE>5120</MAXHEADERSIZE>
   
</LIMITS><PUBLICKEY>YMqDiUgOnJSZmC9X4W3Eqq+inhOIlQ7pk7ll0Ar5XY3hdDFFgma/Kw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>uoDlFYjjCQf5DlrrwEurDh6HEVYWLG3M8z+WPlnSmWI7wnbIESf9Nw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>1563</AUTH_ID><PUBLICKEY>87ckEfUSAqzNZAoq2ByX+r4+31AbrSbpViMLb5Wpzbg+DMjG3gZATw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>5zo0gyvJqB8Kf1Lyc5Lym7dBUXzOSc3r7XKCNsHV3NdZuN+dJawlXw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE
type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>F/KiuSv+WSgoRpJjpL7Pe4Hw8IBHtod15X0uvXASBgnechDgNTDpgg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>
WMPInfo.xml Does not exist on this device
PTP: Closing session
OK.
