Listing raw device(s)
  Found 1 device(s):
  MyMusix: PD-6070 (0aa6:9601) @ bus 0, dev 16
Attempting to connect device(s)
PTP_ERROR_IO: Trying again after re-initializing USB interface
USB low-level info:
  Using kernel interface "usbfs"
  bcdUSB: 512
  bDeviceClass: 0
  bDeviceSubClass: 0
  bDeviceProtocol: 0
  idVendor: 0aa6
  idProduct: 9601
  IN endpoint maxpacket: 64 bytes
  OUT endpoint maxpacket: 64 bytes
  Raw device info:
     Bus location: 0
     Device number: 16
     Device entry info:
        Vendor: MyMusix
        Vendor id: 0x0aa6
        Product: PD-6070
        Vendor id: 0x9601
        Device flags: 0x00000002
Microsoft device descriptor 0xee:
       0000: 1203 4d00 5300 4600 5400 3100 3000 3000   ..M.S.F.T.1.0.0.
       0010: 0100                                      ..
Device info:
  Manufacturer: Generic
  Model: Audio Player
  Device version: RAD2010005%OUT_PAD:128%
  Serial number: F03A085089ECCB0C
  Vendor extension ID: 0x00000006
  Vendor extension description: microsoft.com: 1.0; microsoft.com/WMDRMPD: 10.1
  Detected object size: 64 bits
Supported operations:
  1001: get device info
  1002: Open session
  1003: Close session
  1004: Get storage IDs
  1005: Get storage info
  1006: Get number of objects
  1007: Get object handles
  1008: Get object info
  1009: Get object
  100b: Delete object
  100c: Send object info
  100d: Send object
  1014: Get device property description
  1015: Get device property value
  1016: Set device property value
  9802: Get object property description
  9801: Get object properties supported
  9803: Get object property value
  9804: Set object property value
  9805: Get object property list
  9806: Set object property list
  9808: Send object property list
  9101: Get secure time challenge
  9102: Get secure time response
  9103: Set license response
  9104: Get sync list
  9105: Send meter challenge query
  9106: Get meter challenge
  9107: Get meter response
  9108: Clean data store
  9109: Get license state
  910a: Send WMDRM-PD Command
  910b: Send WMDRM-PD Request
  100f: Format storage
  97f1: Unknown (97f1)
  97f2: Unknown (97f2)
Events supported:
  0x4002
  0x4003
Device Properties Supported:
  0xd101: Secure Time
  0xd102: Device Certificate
Playable File (Object) Types and Object Properties Supported:
  3009: MP3
  3008: MS Wave
  b901: WMA
  3001: Association/Directory
  3000: Undefined Type
Storage Devices:
  StorageID: 0x00010001
     StorageType: 0x0003 fixed RAM storage
     FilesystemType: 0x0002 generic hierarchical
     AccessCapability: 0x0000 read/write
     MaxCapacity: 1010696192
     FreeSpaceInBytes: 896000000
     FreeSpaceInObjects: 4294967295
     StorageDescription: Internal Storage
     VolumeIdentifier: (null)
Special directories:
  Default music folder: 0x00000002
  Default playlist folder: 0x00000000
  Default picture folder: 0x00000000
  Default video folder: 0x00000000
  Default organizer folder: 0x00000000
  Default zencast folder: 0x00000000
  Default album folder: 0x00000000
  Default text folder: 0x00000000
MTP-specific device properties:
  Friendly name: (NULL)
  Synchronization partner: (NULL)
libmtp supported (playable) filetypes:
  ISO MPEG-1 Audio Layer 3
  RIFF WAVE file
  Microsoft Windows Media Audio
Unable to acquire device certificate, perhaps this device does not support this
Error 2: PTP Layer error 02ff: get_device_unicode_property(): failed to get
unicode property.
Error 2: (Look this up in ptp.h for an explanation.)
Error 2: PTP Layer error 02ff: LIBMTP_Get_File_To_File_Descriptor(): Could not
get file from device.
Error 2: (Look this up in ptp.h for an explanation.)
ERROR: Could not close session!
inep: usb_get_endpoint_status(): No such device
outep: usb_get_endpoint_status(): No such device
usb_clear_halt() on IN endpoint: No such device
usb_clear_halt() on OUT endpoint: No such device
usb_clear_halt() on INTERRUPT endpoint: No such device
OK.
