Attempting to connect device(s)
Detect: Successfully connected 1 devices
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 0781
   idProduct: 7420
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Device flags: 0x00000002
Device info:
   Manufacturer: SanDisk
   Model: Sansa e270
   Device version: PP5022AF-05.51-S301-02.18-S301.02.18E-D, (Build 32.10)
   Serial number: 00000000-00000000-3224b387-d925f515-00000000
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com/WMDRMPD: 10.1; portalplayer.com: 1.0; 
Supported operations:
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   101b: Get partial object
   100c: Send object info
   100d: Send object
   100b: Delete object
   1012: Set object protection
   100f: Format storage
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9806: Set object property list
   9810: Get object references
   9811: Set object references
   9201: Report Added/Deleted Items
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
Events supported:
   None.
Device Properties Supported:
   0x5001: Battery Level
   0xd101: Secure Time
   0xd102: Device Certificate
   0xd401: Synchronization Partner
   0xd402: Device Friendly Name
Playable File (Object) Types and Object Properties Supported:
   3001: Association/Directory
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc09: DateModified STRING data type GET/SET
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 1500000, STEP 1 GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 50 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
   3008: MS Wave
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 1500000, STEP 1 GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 50 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc44: Name STRING data type GET/SET
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc09: DateModified STRING data type GET/SET
   ba03: Abstract Audio Album
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337,  READ ONLY
      dc86: RepresentativeSampleData array of UINT8 data type ANY 8BIT VALUE form GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX 220, STEP 1 READ ONLY
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX 176, STEP 1 READ ONLY
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc07: ObjectFileName STRING data type GET/SET
      dc04: ObjectSize UINT64 data type READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc09: DateModified STRING data type GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type GET/SET
      dc0a: Keywords STRING data type GET/SET
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc89: Duration UINT32 data type ANY 32BIT VALUE form GET/SET
      de9a: AudioBitRate UINT32 data type range: MIN 8000, MAX 1500000, STEP 1 GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 96000, STEP 50 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 353,  GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003
      FilesystemType: 0x0002
      AccessCapability: 0x0000
      MaxCapacity: 5991725124
      FreeSpaceInBytes: 345147460
      FreeSpaceInObjects: 4090
      StorageDescription: PPI NAND
      VolumeIdentifier: VOL0_Sansa_e270_00000000-00000000-3224b387-d925f515-00000000
Special directories:
   Default music folder: 0x00020000
   Default playlist folder: 0x00060000
   Default picture folder: 0x00070000
   Default video folder: 0x00040000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: Sansa e270
   Synchronization partner: 
   Battery level 100 of 100 (100%)
libmtp supported (playable) filetypes:
   ISO MPEG-1 Audio Layer 3
   RIFF WAVE file
   Microsoft Windows Media Audio

Secure Time:
<DRMCLOCK type="status"><VALUE>#20070607 19:34:14Z#</VALUE><FLAG>DRM_CLK_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">AAAAAAAAAACHsyQyFfUl2QAAAAA=</UNIQUEID><PUBLICKEY private="1">FCkWyEPukCI5BS31jSFZIjyxyGPKFZoslaf6ufe1wlu/a4V3RHHyJw==</PUBLICKEY><KEYDATA>mUERJ1Tli0xgqIHLOYg2PSiAAvI=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>hce/atRvbjgVknKf9H0OVMfg222M5fcG3JirdiF9S78jW10xPQf5Aw==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>8TaelROuKRPMuILqWmCbtRIe3Ow=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.104.93</SECURITYVERSION><CERTIFICATE private="1">FCkWyEPukCI5BS31jSFZIjyxyGPKFZoslaf6ufe1wlu/a4V3RHHyJwIEaF1/wXbrw+RKpSIfecQ1RV8hWwQSQz1fp6sF4VhcXwDA1X2jQ9287YB8</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>Sansa e200 Series</NAME>
   <MANUFACTURER>SanDisk Corporation</MANUFACTURER>
   <MAKE>MicroStar Internatioal</MAKE>
   <SECURITYLEVEL>2000</SECURITYLEVEL>
   <FEATURES>
        <CLOCK>2</CLOCK>
	  <SECURECLOCK>
		<URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
		<PUBLICKEY>
!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==
</PUBLICKEY>
	  </SECURECLOCK>
        <METERING>1</METERING>
        <LICENSE_ACQ>1</LICENSE_ACQ>
        <LICENSE_SYNC>1</LICENSE_SYNC>
        <ENCRYPTION>1</ENCRYPTION>
    <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
    </FEATURES>
    <LIMITS>
        <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
        <MAXLICENSESIZE>10240</MAXLICENSESIZE>
        <MAXHEADERSIZE>5120</MAXHEADERSIZE>
    </LIMITS><PUBLICKEY>n4ahYQBHQ72FRfkzvy7BruWYDSilgfObLpzG0M8SNcfDGWvJhvbrhA==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>lB5HvVHvcXLb0QiYfskM3Wu0eXtx9Tw0QIiCoKLhBIer0k3ablA4Zg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>961</AUTH_ID><PUBLICKEY>vjU5IwzlqSww/T8ihHxTDmbw1hVeXXG8oNVvgBBYFinhSvQ1e0gNEQ==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>3DU5omHe8sFqztXjYZ9vNr2/DkLabfYH5VIfWrf+XXA+RNASNDpnTg==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>sw5Aa1lOYIBJ6TcDvUa1Dxd2HicA66aj6r/YW2pFvx9L8Oiy/zawbQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>

Device description WMPInfo.xml file:
<DeviceInfo>
    <WMP DeviceID="{7C48990D-8196-4700-B113-9135FB82E08A}" RelationshipID="{00000000-0000-0000-0000-000000000000}"/>
</DeviceInfo>

OK.

 	  	 
