libmtp version: 0.3.5

Listing raw device(s)
   Found 1 device(s):
   Pioneer: XMP3 (08e4:0148) @ bus 0, dev 7
Attempting to connect device(s)
USB low-level info:
   Using kernel interface "usbfs"
   bcdUSB: 512
   bDeviceClass: 0
   bDeviceSubClass: 0
   bDeviceProtocol: 0
   idVendor: 08e4
   idProduct: 0148
   IN endpoint maxpacket: 512 bytes
   OUT endpoint maxpacket: 512 bytes
   Raw device info:
      Bus location: 0
      Device number: 7
      Device entry info:
         Vendor: Pioneer
         Vendor id: 0x08e4
         Product: XMP3
         Vendor id: 0x0148
         Device flags: 0x00000000
Microsoft device descriptor 0xee:
	0000: 1203 4d00 5300 4600 5400 3100 3000 3000	..M.S.F.T.1.0.0.
	0010: fe00                                   	..
Microsoft device response to control message 1, CMD 0xfe:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Microsoft device response to control message 2, CMD 0xfe:
	0000: 2800 0000 0001 0400 0100 0000 0000 0000	(...............
	0010: 0001 4d54 5000 0000 0000 0000 0000 0000	..MTP...........
	0020: 0000 0000 0000 0000                    	........
Device info:
   Manufacturer: Pioneer
   Model: GEX-XMP3
   Device version: 1.0
   Serial number: KGJV02WK        
   Vendor extension ID: 0x00000006
   Vendor extension description: microsoft.com/WMDRMPD: 10.1; audible.com: 1.0; microsoft.com: WMPPD10.0; xmradio.com: 1.0; 
   Detected object size: 64 bits
Supported operations:
   1001: get device info
   1002: Open session
   1003: Close session
   1004: Get storage IDs
   1005: Get storage info
   1006: Get number of objects
   1007: Get object handles
   1008: Get object info
   1009: Get object
   100b: Delete object
   100c: Send object info
   100d: Send object
   100f: Format storage
   1014: Get device property description
   1015: Get device property value
   1016: Set device property value
   1017: Reset device property value
   101b: Get partial object
   9101: Get secure time challenge
   9102: Get secure time response
   9103: Set license response
   9104: Get sync list
   9105: Send meter challenge query
   9106: Get meter challenge
   9107: Get meter response
   9108: Clean data store
   9109: Get license state
   910a: Send WMDRM-PD Command
   910b: Send WMDRM-PD Request
   9201: Report Added/Deleted Items
   9801: Get object properties supported
   9802: Get object property description
   9803: Get object property value
   9804: Set object property value
   9805: Get object property list
   9810: Get object references
   9811: Set object references
Events supported:
   None.
Device Properties Supported:
   0xd100: Unknown property
   0xd101: Secure Time
   0xd102: Device Certificate
   0xd401: Synchronization Partner
   0xd402: Friendly Device Name
Playable File (Object) Types and Object Properties Supported:
   3000: Undefined Type
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
   3001: Association/Directory
      d810: unknown(d810) STRING data type GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
   3008: MS Wave
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 1, 17,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
   3009: MP3
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 85,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
   300c: ASF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 353,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
   3801: JPEG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
   3804: BMP
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
   3807: GIF
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc87: Width UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
      dc88: Height UINT32 data type range: MIN 0, MAX -1, STEP 1 READ ONLY
   b300: Unknown(b300)
      d811: unknown(d811) array of UINT8 data type byte array:  GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
   b901: WMA
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 353,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
   b902: OGG
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type enumeration: 8000, 11025, 12000, 16000, 22050, 24000, 32000, 44100, 48000,  GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0,  READ ONLY
      de9a: AudioBitRate UINT32 data type enumeration: 8000, 16000, 24000, 32000, 40000, 48000, 56000, 64000, 80000, 96000, 112000, 128000, 144000, 160000, 192000, 224000, 256000, 320000,  GET/SET
   b903: AAC
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
   b904: Audible.com Codec
      da00: unknown(da00) UINT32 data type enumeration: 0, 1, 2, 3, 4, 5, 6, 7, 8,  GET/SET
      da01: unknown(da01) STRING data type GET/SET
      da02: unknown(da02) UINT32 data type ANY 32BIT VALUE form READ ONLY
      da03: unknown(da03) UINT16 data type enumeration: 0, 1,  READ ONLY
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc46: Artist STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc89: Duration UINT32 data type range: MIN 0, MAX 134217727, STEP 1 GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8b: Track UINT16 data type ANY 16BIT VALUE form GET/SET
      dc8c: Genre STRING data type GET/SET
      dc91: UseCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc92: SkipCount UINT32 data type ANY 32BIT VALUE form GET/SET
      dc99: OriginalReleaseDate STRING data type DATETIME FORM GET/SET
      dc9a: AlbumName STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
      de92: BitRateType UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de93: SampleRate UINT32 data type range: MIN 8000, MAX 48000, STEP 25 GET/SET
      de94: NumberOfChannels UINT16 data type enumeration: 0, 1, 2,  GET/SET
      de99: AudioWAVECodec UINT32 data type enumeration: 0,  READ ONLY
      de9a: AudioBitRate UINT32 data type range: MIN 1, MAX 2147483647, STEP 1 GET/SET
   ba03: Abstract Audio Album
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14343,  GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
   ba04: Abstract Video Album
      d901: BuyFlag UINT8 data type ANY 8BIT VALUE form GET/SET
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
      dc81: RepresentativeSampleFormat UINT16 data type enumeration: 14337, 14343,  GET/SET
      dc82: RepresentativeSampleSize UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc83: RepresentativeSampleHeight UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc84: RepresentativeSampleWidth UINT32 data type range: MIN 0, MAX -1, STEP 1 GET/SET
      dc86: RepresentativeSampleData array of UINT8 data type byte array:  GET/SET
      dc8a: Rating UINT16 data type range: MIN 0, MAX 100, STEP 1 GET/SET
      dc8c: Genre STRING data type GET/SET
      dc9b: AlbumArtist STRING data type GET/SET
   ba05: Abstract Audio Video Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
   ba11: M3U Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
   ba14: PLS Playlist
      dc01: StorageID UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc02: ObjectFormat UINT16 data type ANY 16BIT VALUE form READ ONLY
      dc03: ProtectionStatus UINT16 data type enumeration: 0, 1, 32770, 32771,  READ ONLY
      dc04: ObjectSize UINT64 data type READ ONLY
      dc07: ObjectFileName STRING data type REGULAR EXPRESSION FORM GET/SET
      dc09: DateModified STRING data type DATETIME FORM GET/SET
      dc0b: ParentObject UINT32 data type ANY 32BIT VALUE form READ ONLY
      dc41: PersistantUniqueObjectIdentifier UINT128 data type READ ONLY
      dc44: Name STRING data type GET/SET
      dc4f: NonConsumable UINT8 data type enumeration: 0, 1,  GET/SET
Storage Devices:
   StorageID: 0x00010001
      StorageType: 0x0003 fixed RAM storage
      FilesystemType: 0x0002 generic hierarchical
      AccessCapability: 0x0000 read/write
      MaxCapacity: 1224638464
      FreeSpaceInBytes: 1222197248
      FreeSpaceInObjects: 3016
      StorageDescription: Internal XM
      VolumeIdentifier: (null)
Special directories:
   Default music folder: 0x00000013
   Default playlist folder: 0x00000000
   Default picture folder: 0x00000000
   Default video folder: 0x00000000
   Default organizer folder: 0x00000000
   Default zencast folder: 0x00000000
   Default album folder: 0x00000000
   Default text folder: 0x00000000
MTP-specific device properties:
   Friendly name: GEX-XMP3
   Synchronization partner: Unknown Partner
libmtp supported (playable) filetypes:
   RIFF WAVE file
   ISO MPEG-1 Audio Layer 3
   Microsoft Advanced Systems Format
   JPEG file
   BMP bitmap file
   GIF bitmap file
   Microsoft Windows Media Audio
   Ogg container format
   Advanced Audio Coding (AAC)/MPEG-2 Part 7/MPEG-4 Part 3
   Audible.com Audio Codec

Secure Time:
<DRMCLOCK type="status"><VALUE>#20090107 23:54:22Z#</VALUE><FLAG>DRM_CLK_NOT_SET</FLAG></DRMCLOCK>

Device Certificate:
<DEVCERT version="1.0"><CERTIFICATE type="DEVICE"><DATA><UNIQUEID private="1">CgoKCgoKCgoKCgoKCgoKCgoKCgo=</UNIQUEID><PUBLICKEY private="1">a2x4qcENCiWxYXXRPVzfwTLVN2Sd1e/qCOubm7AJP4tcYauiIurxMw==</PUBLICKEY><KEYDATA>+Z+mokydkgcclOT9I3VY2Dg2RUY=</KEYDATA></DATA><MSDRM_SIGNATURE_VALUE>bCA2nlQJUb13UIalyVeQ858CVkX7/SW/EWeDCulYYoyl+WMCs+eHUw==</MSDRM_SIGNATURE_VALUE><SYMSIGNATURE>Kpp340t8jBkQP6yGHztt4Py8+Fc=</SYMSIGNATURE></CERTIFICATE><FALLBACK><SECURITYVERSION>2.4.112.9</SECURITYVERSION><CERTIFICATE private="1">a2x4qcENCiWxYXXRPVzfwTLVN2Sd1e/qCOubm7AJP4tcYauiIurxMwIEcAkPT7kyzbnqgrVnBLN/T0vPjbKaADOxrhRYTuFDXyC0tDgq4BRLG7N2</CERTIFICATE></FALLBACK><CERTIFICATE type="GROUP"><DATA><NAME>Tuner</NAME>
    <MANUFACTURER>Pioneer Corporation</MANUFACTURER>
    <MAKE>GEX-XMP3</MAKE>
    <DISTRIBUTOR>Pioneer Corporation</DISTRIBUTOR>
    <MODEL>GEX-XMP3</MODEL>
    <SECURITYLEVEL>2000</SECURITYLEVEL>
    <HARDWARE_VER_MAJOR>1</HARDWARE_VER_MAJOR>
    <HARDWARE_VER_MINOR>0</HARDWARE_VER_MINOR>
    <FIRMWARE_VER_MAJOR>1</FIRMWARE_VER_MAJOR>
    <FIRMWARE_VER_MINOR>0</FIRMWARE_VER_MINOR>
    <FEATURES>
        <CLOCK>2</CLOCK>
        <SECURECLOCK>
            <URL>http://go.microsoft.com/fwlink/?LinkId=25817</URL>
            <PUBLICKEY>!CNhvvz1WaNV1AFUmetxkvm9iD4UrE9cnGUi!qcqdxMiXmD1*ikYGA==</PUBLICKEY>
        </SECURECLOCK>
        <METERING>1</METERING>
        <LICENSE_ACQ>1</LICENSE_ACQ>
        <LICENSE_SYNC>1</LICENSE_SYNC>
        <ENCRYPTION>1</ENCRYPTION>
        <SYMMETRIC_OPT>1</SYMMETRIC_OPT>
    </FEATURES>
    <LIMITS>
        <MAXCHAINDEPTH>2</MAXCHAINDEPTH>
        <MAXLICENSESIZE>10240</MAXLICENSESIZE>
        <MAXHEADERSIZE>5120</MAXHEADERSIZE>
    </LIMITS><PUBLICKEY>5gibJa9onBuFn724nkN0WFpB3Vp4qJULn7lHsB1rHIn3tiMhF/EBPA==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>ajkELHT2t30OVOc6Rl3hYTCLhiq0DS+eUfj8KHHANHtN2pKkDTDvUQ==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION"><DATA><SECURITYLEVEL>2000</SECURITYLEVEL><AUTH_ID>2925</AUTH_ID><PUBLICKEY>ilRdvL8rZKkatIhDUPYViKdTemg77FUVS+2pOABaRR9+BmJDm/8vLA==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>zltEMJzjgFZF4b25S/xwGoDAOwXMQ+zRitoaxBa7pRk3WybQBJbYPw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE><CERTIFICATE type="AUTHORIZATION_ROOT"><DATA><AUTH_ID>1</AUTH_ID><PUBLICKEY>a1t3hxrg!qbOgktnbYaEEi4teCse!gz6RvTPuC!zizKJlpU7xoduSw==</PUBLICKEY></DATA><MSDRM_SIGNATURE_VALUE>OcY9VKyByS0dYOkwm1FjpmvuERuGZoDeUzKF8JKzyH5NV3paEWqfDw==</MSDRM_SIGNATURE_VALUE></CERTIFICATE></DEVCERT>

WMPInfo.xml file contents:
<DeviceInfo>
    <WMP DeviceID="{6DF897F3-714C-4352-9EBD-873D57E7B389}" RelationshipID="{00000000-0000-0000-0000-000000000000}"/>
</DeviceInfo>

OK.
